Enumerations
HAL PWM active channel
Peripheral Driver » HAL Driver » PWM » Enumerations

## Enumerations
enum | hal_pwm_active_channel_t { HAL_PWM_ACTIVE_CHANNEL_A = 0x01, HAL_PWM_ACTIVE_CHANNEL_B = 0x02, HAL_PWM_ACTIVE_CHANNEL_C = 0x04, HAL_PWM_ACTIVE_CHANNEL_ALL = 0x07, HAL_PWM_ACTIVE_CHANNEL_CLEARED = 0x00 }
| HAL PWM active channel Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_pwm_active_channel_t

enum hal_pwm_active_channel_t

HAL PWM active channel Enumerations definition.

Enumerator
HAL_PWM_ACTIVE_CHANNEL_A | The active channel is A
HAL_PWM_ACTIVE_CHANNEL_B | The active channel is B
HAL_PWM_ACTIVE_CHANNEL_C | The active channel is C
HAL_PWM_ACTIVE_CHANNEL_ALL | The active channels are ALL
HAL_PWM_ACTIVE_CHANNEL_CLEARED | All active channels are cleared

Definition at line 91 of file gr55xx_hal_pwm.h.