Functions
IO operation functions
Peripheral Driver » HAL Driver » AON_WDT » Functions

IO operation functions. More...

## Functions
hal_status_t | hal_aon_wdt_refresh (aon_wdt_handle_t *p_aon_wdt)
| Refresh the AON_WDT. More...

## Detailed Description

IO operation functions.

      ==============================================================================
                          ##### IO operation functions #####
      ==============================================================================
      [..]
        This section provides functions allowing to:
        (+) Refresh the AON_WDT.
        (+) Handle AON_WDT interrupt request and associated function callback.

## Function Documentation

## ◆ hal_aon_wdt_refresh()

hal_status_t hal_aon_wdt_refresh | ( | aon_wdt_handle_t * | p_aon_wdt | ) |

Refresh the AON_WDT.

Parameters

  [in] | p_aon_wdt | Pointer to a AON_WDT handle which contains the configuration information for the specified AON_WDT module.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.