Modules | Macros
AON_GPIOEx Mux function selection
Peripheral Driver » HAL Driver » AON_GPIOEx » Defines » AON_GPIOEx Exported Constants

## Modules
| AON_GPIO PIN common MUX selection(Available for all AON GPIO pins)
| AON_GPIO_PIN1 MUX selection
| AON_GPIO_PIN2 MUX selection
| AON_GPIO_PIN3 MUX selection
| AON_GPIO_PIN4 MUX selection
| AON_GPIO_PIN5 MUX selection

## Macros
#define | IS_AON_GPIO_MUX(__MUX__) (((__MUX__) <= AON_GPIO_MUX_7))
| Check if AON GPIO Mux mode is valid. More...

## Detailed Description

## Macro Definition Documentation

## ◆ IS_AON_GPIO_MUX

#define IS_AON_GPIO_MUX | ( |  | __MUX__ | ) | (((__MUX__) <= AON_GPIO_MUX_7))

Check if AON GPIO Mux mode is valid.

Parameters

  __MUX__ | AON GPIO Mux mode.

Return values

  SET | (__ACTION__ is valid) or RESET (__ACTION__ is invalid)

Definition at line 159 of file gr55xx_hal_aon_gpio_ex.h.