Enumerations
Enumerations
Peripheral Driver » APP DRIVER » RNG

## Enumerations
enum | app_rng_type_t { APP_RNG_TYPE_INTERRUPT, APP_RNG_TYPE_POLLING, APP_RNG_TYPE_MAX }
| RNG operating mode Enumerations definition. More...
enum | app_rng_evt_type_t { APP_RNG_EVT_DONE, APP_RNG_EVT_ERROR }
| RNG event Enumerations definition. More...
enum | app_rng_state_t { APP_RNG_INVALID = 0, APP_RNG_ACTIVITY }
| App rng state types. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ app_rng_evt_type_t

enum app_rng_evt_type_t

RNG event Enumerations definition.

Enumerator
APP_RNG_EVT_DONE | Generated random by UART peripheral.
APP_RNG_EVT_ERROR | Error reported by UART peripheral.

Definition at line 82 of file app_rng.h.

## ◆ app_rng_state_t

enum app_rng_state_t

App rng state types.

Enumerator
APP_RNG_INVALID |
APP_RNG_ACTIVITY |

Definition at line 119 of file app_rng.h.

## ◆ app_rng_type_t

enum app_rng_type_t

RNG operating mode Enumerations definition.

Enumerator
APP_RNG_TYPE_INTERRUPT | Interrupt operation mode.
APP_RNG_TYPE_POLLING | Polling operation mode.
APP_RNG_TYPE_MAX | Only for check parameter, not used as input parameters.

Definition at line 72 of file app_rng.h.