ble_id.h
Go to the documentation of this file.
1 #ifndef BLE_ID_H_
2 #define BLE_ID_H_
3
4 /*
5 * INCLUDE FILES
6 ****************************************************************************************
7 */
8 #include <stdbool.h>
9 #include <stddef.h>
10 #include <stdint.h>
11
12 /*
13 * DEFINES
14 ****************************************************************************************
15 */
16
17 #define TASK_FIRST_MSG(task) ((uint16_t)((task) << 8))
18 #define MSG_ID(task, idx) (TASK_FIRST_MSG((TASK_ID_ ## task)) + idx)
19
20 #define KE_MSG_DEFAULT_HANDLER (0xFFFF)
21
22 /**************************************************************************************
23 ************** HCI CMDS ****************
24 **************************************************************************************/
25 enum hci_opcode
26 {
27 HCI_NO_OPERATION_CMD_OPCODE = 0x0000,
28
29 //Link Control Commands
30 HCI_INQ_CMD_OPCODE = 0x0401,
31 HCI_INQ_CANCEL_CMD_OPCODE = 0x0402,
32 HCI_PER_INQ_MODE_CMD_OPCODE = 0x0403,
33 HCI_EXIT_PER_INQ_MODE_CMD_OPCODE = 0x0404,
34 HCI_CREATE_CON_CMD_OPCODE = 0x0405,
35 HCI_DISCONNECT_CMD_OPCODE = 0x0406,
36 HCI_CREATE_CON_CANCEL_CMD_OPCODE = 0x0408,
37 HCI_ACCEPT_CON_REQ_CMD_OPCODE = 0x0409,
38 HCI_REJECT_CON_REQ_CMD_OPCODE = 0x040A,
39 HCI_LK_REQ_REPLY_CMD_OPCODE = 0x040B,
40 HCI_LK_REQ_NEG_REPLY_CMD_OPCODE = 0x040C,
41 HCI_PIN_CODE_REQ_REPLY_CMD_OPCODE = 0x040D,
42 HCI_PIN_CODE_REQ_NEG_REPLY_CMD_OPCODE = 0x040E,
43 HCI_CHG_CON_PKT_TYPE_CMD_OPCODE = 0x040F,
44 HCI_AUTH_REQ_CMD_OPCODE = 0x0411,
45 HCI_SET_CON_ENC_CMD_OPCODE = 0x0413,
46 HCI_CHG_CON_LK_CMD_OPCODE = 0x0415,
47 HCI_MASTER_LK_CMD_OPCODE = 0x0417,
48 HCI_REM_NAME_REQ_CMD_OPCODE = 0x0419,
49 HCI_REM_NAME_REQ_CANCEL_CMD_OPCODE = 0x041A,
50 HCI_RD_REM_SUPP_FEATS_CMD_OPCODE = 0x041B,
51 HCI_RD_REM_EXT_FEATS_CMD_OPCODE = 0x041C,
52 HCI_RD_REM_VER_INFO_CMD_OPCODE = 0x041D,
53 HCI_RD_CLK_OFF_CMD_OPCODE = 0x041F,
54 HCI_RD_LMP_HDL_CMD_OPCODE = 0x0420,
55 HCI_SETUP_SYNC_CON_CMD_OPCODE = 0x0428,
56 HCI_ACCEPT_SYNC_CON_REQ_CMD_OPCODE = 0x0429,
57 HCI_REJECT_SYNC_CON_REQ_CMD_OPCODE = 0x042A,
58 HCI_IO_CAP_REQ_REPLY_CMD_OPCODE = 0x042B,
59 HCI_USER_CFM_REQ_REPLY_CMD_OPCODE = 0x042C,
60 HCI_USER_CFM_REQ_NEG_REPLY_CMD_OPCODE = 0x042D,
61 HCI_USER_PASSKEY_REQ_REPLY_CMD_OPCODE = 0x042E,
62 HCI_USER_PASSKEY_REQ_NEG_REPLY_CMD_OPCODE = 0x042F,
63 HCI_REM_OOB_DATA_REQ_REPLY_CMD_OPCODE = 0x0430,
64 HCI_REM_OOB_DATA_REQ_NEG_REPLY_CMD_OPCODE = 0x0433,
65 HCI_IO_CAP_REQ_NEG_REPLY_CMD_OPCODE = 0x0434,
66 HCI_ENH_SETUP_SYNC_CON_CMD_OPCODE = 0x043D,
67 HCI_ENH_ACCEPT_SYNC_CON_CMD_OPCODE = 0x043E,
68 HCI_TRUNC_PAGE_CMD_OPCODE = 0x043F,
69 HCI_TRUNC_PAGE_CAN_CMD_OPCODE = 0x0440,
70 HCI_SET_CON_SLV_BCST_CMD_OPCODE = 0x0441,
71 HCI_SET_CON_SLV_BCST_REC_CMD_OPCODE = 0x0442,
72 HCI_START_SYNC_TRAIN_CMD_OPCODE = 0x0443,
73 HCI_REC_SYNC_TRAIN_CMD_OPCODE = 0x0444,
74 HCI_REM_OOB_EXT_DATA_REQ_REPLY_CMD_OPCODE = 0x0445,
75
76 //Link Policy Commands
77 HCI_HOLD_MODE_CMD_OPCODE = 0x0801,
78 HCI_SNIFF_MODE_CMD_OPCODE = 0x0803,
79 HCI_EXIT_SNIFF_MODE_CMD_OPCODE = 0x0804,
80 HCI_PARK_STATE_CMD_OPCODE = 0x0805,
81 HCI_EXIT_PARK_STATE_CMD_OPCODE = 0x0806,
82 HCI_QOS_SETUP_CMD_OPCODE = 0x0807,
83 HCI_ROLE_DISCOVERY_CMD_OPCODE = 0x0809,
84 HCI_SWITCH_ROLE_CMD_OPCODE = 0x080B,
85 HCI_RD_LINK_POL_STG_CMD_OPCODE = 0x080C,
86 HCI_WR_LINK_POL_STG_CMD_OPCODE = 0x080D,
87 HCI_RD_DFT_LINK_POL_STG_CMD_OPCODE = 0x080E,
88 HCI_WR_DFT_LINK_POL_STG_CMD_OPCODE = 0x080F,
89 HCI_FLOW_SPEC_CMD_OPCODE = 0x0810,
90 HCI_SNIFF_SUB_CMD_OPCODE = 0x0811,
91
92 //Controller and Baseband Commands
93 HCI_SET_EVT_MASK_CMD_OPCODE = 0x0C01,
94 HCI_RESET_CMD_OPCODE = 0x0C03,
95 HCI_SET_EVT_FILTER_CMD_OPCODE = 0x0C05,
96 HCI_FLUSH_CMD_OPCODE = 0x0C08,
97 HCI_RD_PIN_TYPE_CMD_OPCODE = 0x0C09,
98 HCI_WR_PIN_TYPE_CMD_OPCODE = 0x0C0A,
99 HCI_CREATE_NEW_UNIT_KEY_CMD_OPCODE = 0x0C0B,
100 HCI_RD_STORED_LK_CMD_OPCODE = 0x0C0D,
101 HCI_WR_STORED_LK_CMD_OPCODE = 0x0C11,
102 HCI_DEL_STORED_LK_CMD_OPCODE = 0x0C12,
103 HCI_WR_LOCAL_NAME_CMD_OPCODE = 0x0C13,
104 HCI_RD_LOCAL_NAME_CMD_OPCODE = 0x0C14,
105 HCI_RD_CON_ACCEPT_TO_CMD_OPCODE = 0x0C15,
106 HCI_WR_CON_ACCEPT_TO_CMD_OPCODE = 0x0C16,
107 HCI_RD_PAGE_TO_CMD_OPCODE = 0x0C17,
108 HCI_WR_PAGE_TO_CMD_OPCODE = 0x0C18,
109 HCI_RD_SCAN_EN_CMD_OPCODE = 0x0C19,
110 HCI_WR_SCAN_EN_CMD_OPCODE = 0x0C1A,
111 HCI_RD_PAGE_SCAN_ACT_CMD_OPCODE = 0x0C1B,
112 HCI_WR_PAGE_SCAN_ACT_CMD_OPCODE = 0x0C1C,
113 HCI_RD_INQ_SCAN_ACT_CMD_OPCODE = 0x0C1D,
114 HCI_WR_INQ_SCAN_ACT_CMD_OPCODE = 0x0C1E,
115 HCI_RD_AUTH_EN_CMD_OPCODE = 0x0C1F,
116 HCI_WR_AUTH_EN_CMD_OPCODE = 0x0C20,
117 HCI_RD_CLASS_OF_DEV_CMD_OPCODE = 0x0C23,
118 HCI_WR_CLASS_OF_DEV_CMD_OPCODE = 0x0C24,
119 HCI_RD_VOICE_STG_CMD_OPCODE = 0x0C25,
120 HCI_WR_VOICE_STG_CMD_OPCODE = 0x0C26,
121 HCI_RD_AUTO_FLUSH_TO_CMD_OPCODE = 0x0C27,
122 HCI_WR_AUTO_FLUSH_TO_CMD_OPCODE = 0x0C28,
123 HCI_RD_NB_BDCST_RETX_CMD_OPCODE = 0x0C29,
124 HCI_WR_NB_BDCST_RETX_CMD_OPCODE = 0x0C2A,
125 HCI_RD_HOLD_MODE_ACTIVITY_CMD_OPCODE = 0x0C2B,
126 HCI_WR_HOLD_MODE_ACTIVITY_CMD_OPCODE = 0x0C2C,
127 HCI_RD_TX_PWR_LVL_CMD_OPCODE = 0x0C2D,
128 HCI_RD_SYNC_FLOW_CTRL_EN_CMD_OPCODE = 0x0C2E,
129 HCI_WR_SYNC_FLOW_CTRL_EN_CMD_OPCODE = 0x0C2F,
130 HCI_SET_CTRL_TO_HOST_FLOW_CTRL_CMD_OPCODE = 0x0C31,
131 HCI_HOST_BUF_SIZE_CMD_OPCODE = 0x0C33,
132 HCI_HOST_NB_CMP_PKTS_CMD_OPCODE = 0x0C35,
133 HCI_RD_LINK_SUPV_TO_CMD_OPCODE = 0x0C36,
134 HCI_WR_LINK_SUPV_TO_CMD_OPCODE = 0x0C37,
135 HCI_RD_NB_SUPP_IAC_CMD_OPCODE = 0x0C38,
136 HCI_RD_CURR_IAC_LAP_CMD_OPCODE = 0x0C39,
137 HCI_WR_CURR_IAC_LAP_CMD_OPCODE = 0x0C3A,
138 HCI_SET_AFH_HOST_CH_CLASS_CMD_OPCODE = 0x0C3F,
139 HCI_RD_INQ_SCAN_TYPE_CMD_OPCODE = 0x0C42,
140 HCI_WR_INQ_SCAN_TYPE_CMD_OPCODE = 0x0C43,
141 HCI_RD_INQ_MODE_CMD_OPCODE = 0x0C44,
142 HCI_WR_INQ_MODE_CMD_OPCODE = 0x0C45,
143 HCI_RD_PAGE_SCAN_TYPE_CMD_OPCODE = 0x0C46,
144 HCI_WR_PAGE_SCAN_TYPE_CMD_OPCODE = 0x0C47,
145 HCI_RD_AFH_CH_ASSESS_MODE_CMD_OPCODE = 0x0C48,
146 HCI_WR_AFH_CH_ASSESS_MODE_CMD_OPCODE = 0x0C49,
147 HCI_RD_EXT_INQ_RSP_CMD_OPCODE = 0x0C51,
148 HCI_WR_EXT_INQ_RSP_CMD_OPCODE = 0x0C52,
149 HCI_REFRESH_ENC_KEY_CMD_OPCODE = 0x0C53,
150 HCI_RD_SP_MODE_CMD_OPCODE = 0x0C55,
151 HCI_WR_SP_MODE_CMD_OPCODE = 0x0C56,
152 HCI_RD_LOC_OOB_DATA_CMD_OPCODE = 0x0C57,
153 HCI_RD_INQ_RSP_TX_PWR_LVL_CMD_OPCODE = 0x0C58,
154 HCI_WR_INQ_TX_PWR_LVL_CMD_OPCODE = 0x0C59,
155 HCI_RD_DFT_ERR_DATA_REP_CMD_OPCODE = 0x0C5A,
156 HCI_WR_DFT_ERR_DATA_REP_CMD_OPCODE = 0x0C5B,
157 HCI_ENH_FLUSH_CMD_OPCODE = 0x0C5F,
158 HCI_SEND_KEYPRESS_NOTIF_CMD_OPCODE = 0x0C60,
159 HCI_SET_EVT_MASK_PAGE_2_CMD_OPCODE = 0x0C63,
160 HCI_RD_FLOW_CNTL_MODE_CMD_OPCODE = 0x0C66,
161 HCI_WR_FLOW_CNTL_MODE_CMD_OPCODE = 0x0C67,
162 HCI_RD_ENH_TX_PWR_LVL_CMD_OPCODE = 0x0C68,
163 HCI_RD_LE_HOST_SUPP_CMD_OPCODE = 0x0C6C,
164 HCI_WR_LE_HOST_SUPP_CMD_OPCODE = 0x0C6D,
165 HCI_SET_MWS_CHANNEL_PARAMS_CMD_OPCODE = 0x0C6E,
166 HCI_SET_EXTERNAL_FRAME_CONFIG_CMD_OPCODE = 0x0C6F,
167 HCI_SET_MWS_SIGNALING_CMD_OPCODE = 0x0C70,
168 HCI_SET_MWS_TRANSPORT_LAYER_CMD_OPCODE = 0x0C71,
169 HCI_SET_MWS_SCAN_FREQ_TABLE_CMD_OPCODE = 0x0C72,
170 HCI_SET_MWS_PATTERN_CONFIG_CMD_OPCODE = 0x0C73,
171 HCI_SET_RES_LT_ADDR_CMD_OPCODE = 0x0C74,
172 HCI_DEL_RES_LT_ADDR_CMD_OPCODE = 0x0C75,
173 HCI_SET_CON_SLV_BCST_DATA_CMD_OPCODE = 0x0C76,
174 HCI_RD_SYNC_TRAIN_PARAM_CMD_OPCODE = 0x0C77,
175 HCI_WR_SYNC_TRAIN_PARAM_CMD_OPCODE = 0x0C78,
176 HCI_RD_SEC_CON_HOST_SUPP_CMD_OPCODE = 0x0C79,
177 HCI_WR_SEC_CON_HOST_SUPP_CMD_OPCODE = 0x0C7A,
178 HCI_RD_AUTH_PAYL_TO_CMD_OPCODE = 0x0C7B,
179 HCI_WR_AUTH_PAYL_TO_CMD_OPCODE = 0x0C7C,
180 HCI_RD_LOC_OOB_EXT_DATA_CMD_OPCODE = 0x0C7D,
181 HCI_RD_EXT_PAGE_TO_CMD_OPCODE = 0x0C7E,
182 HCI_WR_EXT_PAGE_TO_CMD_OPCODE = 0x0C7F,
183 HCI_RD_EXT_INQ_LEN_CMD_OPCODE = 0x0C80,
184 HCI_WR_EXT_INQ_LEN_CMD_OPCODE = 0x0C81,
185 HCI_SET_ECO_BASE_INTV_CMD_OPCODE = 0x0C82,
186 HCI_CONFIG_DATA_PATH_CMD_OPCODE = 0x0C83,
187
188 //Info Params
189 HCI_RD_LOCAL_VER_INFO_CMD_OPCODE = 0x1001,
190 HCI_RD_LOCAL_SUPP_CMDS_CMD_OPCODE = 0x1002,
191 HCI_RD_LOCAL_SUPP_FEATS_CMD_OPCODE = 0x1003,
192 HCI_RD_LOCAL_EXT_FEATS_CMD_OPCODE = 0x1004,
193 HCI_RD_BUF_SIZE_CMD_OPCODE = 0x1005,
194 HCI_RD_BD_ADDR_CMD_OPCODE = 0x1009,
195 HCI_RD_DATA_BLOCK_SIZE_CMD_OPCODE = 0x100A,
196 HCI_RD_LOCAL_SUPP_CODECS_CMD_OPCODE = 0x100B,
197 HCI_RD_LOCAL_SP_OPT_CMD_OPCODE = 0x100C,
198 HCI_RD_LOCAL_SUPP_CODECS_V2_CMD_OPCODE = 0x100D,
199 HCI_RD_LOCAL_SUPP_CODEC_CAP_CMD_OPCODE = 0x100E,
200 HCI_RD_LOCAL_SUPP_CTRL_DELAY_CMD_OPCODE = 0x100F,
201
202 //Status Params
203 HCI_RD_FAIL_CONTACT_CNT_CMD_OPCODE = 0x1401,
204 HCI_RST_FAIL_CONTACT_CNT_CMD_OPCODE = 0x1402,
205 HCI_RD_LINK_QUAL_CMD_OPCODE = 0x1403,
206 HCI_RD_RSSI_CMD_OPCODE = 0x1405,
207 HCI_RD_AFH_CH_MAP_CMD_OPCODE = 0x1406,
208 HCI_RD_CLK_CMD_OPCODE = 0x1407,
209 HCI_RD_ENC_KEY_SIZE_CMD_OPCODE = 0x1408,
210 HCI_GET_MWS_TRANSPORT_LAYER_CONFIG_CMD_OPCODE = 0x140C,
211
212 //Testing Commands
213 HCI_RD_LOOPBACK_MODE_CMD_OPCODE = 0x1801,
214 HCI_WR_LOOPBACK_MODE_CMD_OPCODE = 0x1802,
215 HCI_EN_DUT_MODE_CMD_OPCODE = 0x1803,
216 HCI_WR_SP_DBG_MODE_CMD_OPCODE = 0x1804,
217 HCI_WR_SEC_CON_TEST_MODE_CMD_OPCODE = 0x180A,
218
219 /// LE Commands Opcodes
220 HCI_LE_SET_EVT_MASK_CMD_OPCODE = 0x2001,
221 HCI_LE_RD_BUF_SIZE_CMD_OPCODE = 0x2002,
222 HCI_LE_RD_LOCAL_SUPP_FEATS_CMD_OPCODE = 0x2003,
223 HCI_LE_SET_RAND_ADDR_CMD_OPCODE = 0x2005,
224 HCI_LE_SET_ADV_PARAM_CMD_OPCODE = 0x2006,
225 HCI_LE_RD_ADV_CHNL_TX_PW_CMD_OPCODE = 0x2007,
226 HCI_LE_SET_ADV_DATA_CMD_OPCODE = 0x2008,
227 HCI_LE_SET_SCAN_RSP_DATA_CMD_OPCODE = 0x2009,
228 HCI_LE_SET_ADV_EN_CMD_OPCODE = 0x200A,
229 HCI_LE_SET_SCAN_PARAM_CMD_OPCODE = 0x200B,
230 HCI_LE_SET_SCAN_EN_CMD_OPCODE = 0x200C,
231 HCI_LE_CREATE_CON_CMD_OPCODE = 0x200D,
232 HCI_LE_CREATE_CON_CANCEL_CMD_OPCODE = 0x200E,
233 HCI_LE_RD_WLST_SIZE_CMD_OPCODE = 0x200F,
234 HCI_LE_CLEAR_WLST_CMD_OPCODE = 0x2010,
235 HCI_LE_ADD_DEV_TO_WLST_CMD_OPCODE = 0x2011,
236 HCI_LE_RMV_DEV_FROM_WLST_CMD_OPCODE = 0x2012,
237 HCI_LE_CON_UPDATE_CMD_OPCODE = 0x2013,
238 HCI_LE_SET_HOST_CH_CLASS_CMD_OPCODE = 0x2014,
239 HCI_LE_RD_CHNL_MAP_CMD_OPCODE = 0x2015,
240 HCI_LE_RD_REM_FEATS_CMD_OPCODE = 0x2016,
241 HCI_LE_ENC_CMD_OPCODE = 0x2017,
242 HCI_LE_RAND_CMD_OPCODE = 0x2018,
243 HCI_LE_EN_ENC_CMD_OPCODE = 0x2019,
244 HCI_LE_LTK_REQ_REPLY_CMD_OPCODE = 0x201A,
245 HCI_LE_LTK_REQ_NEG_REPLY_CMD_OPCODE = 0x201B,
246 HCI_LE_RD_SUPP_STATES_CMD_OPCODE = 0x201C,
247 HCI_LE_RX_TEST_V1_CMD_OPCODE = 0x201D,
248 HCI_LE_TX_TEST_V1_CMD_OPCODE = 0x201E,
249 HCI_LE_TEST_END_CMD_OPCODE = 0x201F,
250 HCI_LE_REM_CON_PARAM_REQ_REPLY_CMD_OPCODE = 0x2020,
251 HCI_LE_REM_CON_PARAM_REQ_NEG_REPLY_CMD_OPCODE = 0x2021,
252 HCI_LE_SET_DATA_LEN_CMD_OPCODE = 0x2022,
253 HCI_LE_RD_SUGGTED_DFT_DATA_LEN_CMD_OPCODE = 0x2023,
254 HCI_LE_WR_SUGGTED_DFT_DATA_LEN_CMD_OPCODE = 0x2024,
255 HCI_LE_RD_LOC_P256_PUB_KEY_CMD_OPCODE = 0x2025,
256 HCI_LE_GEN_DHKEY_V1_CMD_OPCODE = 0x2026,
257 HCI_LE_ADD_DEV_TO_RSLV_LIST_CMD_OPCODE = 0x2027,
258 HCI_LE_RMV_DEV_FROM_RSLV_LIST_CMD_OPCODE = 0x2028,
259 HCI_LE_CLEAR_RSLV_LIST_CMD_OPCODE = 0x2029,
260 HCI_LE_RD_RSLV_LIST_SIZE_CMD_OPCODE = 0x202A,
261 HCI_LE_RD_PEER_RSLV_ADDR_CMD_OPCODE = 0x202B,
262 HCI_LE_RD_LOC_RSLV_ADDR_CMD_OPCODE = 0x202C,
263 HCI_LE_SET_ADDR_RESOL_EN_CMD_OPCODE = 0x202D,
264 HCI_LE_SET_RSLV_PRIV_ADDR_TO_CMD_OPCODE = 0x202E,
265 HCI_LE_RD_MAX_DATA_LEN_CMD_OPCODE = 0x202F,
266 HCI_LE_RD_PHY_CMD_OPCODE = 0x2030,
267 HCI_LE_SET_DFT_PHY_CMD_OPCODE = 0x2031,
268 HCI_LE_SET_PHY_CMD_OPCODE = 0x2032,
269 HCI_LE_RX_TEST_V2_CMD_OPCODE = 0x2033,
270 HCI_LE_TX_TEST_V2_CMD_OPCODE = 0x2034,
271 HCI_LE_SET_ADV_SET_RAND_ADDR_CMD_OPCODE = 0x2035,
272 HCI_LE_SET_EXT_ADV_PARAM_CMD_OPCODE = 0x2036,
273 HCI_LE_SET_EXT_ADV_DATA_CMD_OPCODE = 0x2037,
274 HCI_LE_SET_EXT_SCAN_RSP_DATA_CMD_OPCODE = 0x2038,
275 HCI_LE_SET_EXT_ADV_EN_CMD_OPCODE = 0x2039,
276 HCI_LE_RD_MAX_ADV_DATA_LEN_CMD_OPCODE = 0x203A,
277 HCI_LE_RD_NB_SUPP_ADV_SETS_CMD_OPCODE = 0x203B,
278 HCI_LE_RMV_ADV_SET_CMD_OPCODE = 0x203C,
279 HCI_LE_CLEAR_ADV_SETS_CMD_OPCODE = 0x203D,
280 HCI_LE_SET_PER_ADV_PARAM_CMD_OPCODE = 0x203E,
281 HCI_LE_SET_PER_ADV_DATA_CMD_OPCODE = 0x203F,
282 HCI_LE_SET_PER_ADV_EN_CMD_OPCODE = 0x2040,
283 HCI_LE_SET_EXT_SCAN_PARAM_CMD_OPCODE = 0x2041,
284 HCI_LE_SET_EXT_SCAN_EN_CMD_OPCODE = 0x2042,
285 HCI_LE_EXT_CREATE_CON_CMD_OPCODE = 0x2043,
286 HCI_LE_PER_ADV_CREATE_SYNC_CMD_OPCODE = 0x2044,
287 HCI_LE_PER_ADV_CREATE_SYNC_CANCEL_CMD_OPCODE = 0x2045,
288 HCI_LE_PER_ADV_TERM_SYNC_CMD_OPCODE = 0x2046,
289 HCI_LE_ADD_DEV_TO_PER_ADV_LIST_CMD_OPCODE = 0x2047,
290 HCI_LE_RMV_DEV_FROM_PER_ADV_LIST_CMD_OPCODE = 0x2048,
291 HCI_LE_CLEAR_PER_ADV_LIST_CMD_OPCODE = 0x2049,
292 HCI_LE_RD_PER_ADV_LIST_SIZE_CMD_OPCODE = 0x204A,
293 HCI_LE_RD_TX_PWR_CMD_OPCODE = 0x204B,
294 HCI_LE_RD_RF_PATH_COMP_CMD_OPCODE = 0x204C,
295 HCI_LE_WR_RF_PATH_COMP_CMD_OPCODE = 0x204D,
296 HCI_LE_SET_PRIV_MODE_CMD_OPCODE = 0x204E,
297 HCI_LE_RX_TEST_V3_CMD_OPCODE = 0x204F,
298 HCI_LE_TX_TEST_V3_CMD_OPCODE = 0x2050,
299 HCI_LE_SET_CONLESS_CTE_TX_PARAM_CMD_OPCODE = 0x2051,
300 HCI_LE_SET_CONLESS_CTE_TX_EN_CMD_OPCODE = 0x2052,
301 HCI_LE_SET_CONLESS_IQ_SAMPL_EN_CMD_OPCODE = 0x2053,
302 HCI_LE_SET_CON_CTE_RX_PARAM_CMD_OPCODE = 0x2054,
303 HCI_LE_SET_CON_CTE_TX_PARAM_CMD_OPCODE = 0x2055,
304 HCI_LE_CON_CTE_REQ_EN_CMD_OPCODE = 0x2056,
305 HCI_LE_CON_CTE_RSP_EN_CMD_OPCODE = 0x2057,
306 HCI_LE_RD_ANTENNA_INF_CMD_OPCODE = 0x2058,
307 HCI_LE_SET_PER_ADV_REC_EN_CMD_OPCODE = 0x2059,
308 HCI_LE_PER_ADV_SYNC_TRANSF_CMD_OPCODE = 0x205A,
309 HCI_LE_PER_ADV_SET_INFO_TRANSF_CMD_OPCODE = 0x205B,
310 HCI_LE_SET_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE = 0x205C,
311 HCI_LE_SET_DFT_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE = 0x205D,
312 HCI_LE_GEN_DHKEY_V2_CMD_OPCODE = 0x205E,
313 HCI_LE_MOD_SLEEP_CLK_ACC_CMD_OPCODE = 0x205F,
314 HCI_LE_RD_BUF_SIZE_V2_CMD_OPCODE = 0x2060,
315 HCI_LE_RD_ISO_TX_SYNC_CMD_OPCODE = 0x2061,
316 HCI_LE_SET_CIG_PARAMS_CMD_OPCODE = 0x2062,
317 HCI_LE_SET_CIG_PARAMS_TEST_CMD_OPCODE = 0x2063,
318 HCI_LE_CREATE_CIS_CMD_OPCODE = 0x2064,
319 HCI_LE_REMOVE_CIG_CMD_OPCODE = 0x2065,
320 HCI_LE_ACCEPT_CIS_REQ_CMD_OPCODE = 0x2066,
321 HCI_LE_REJECT_CIS_REQ_CMD_OPCODE = 0x2067,
322 HCI_LE_CREATE_BIG_CMD_OPCODE = 0x2068,
323 HCI_LE_CREATE_BIG_TEST_CMD_OPCODE = 0x2069,
324 HCI_LE_TERMINATE_BIG_CMD_OPCODE = 0x206A,
325 HCI_LE_BIG_CREATE_SYNC_CMD_OPCODE = 0x206B,
326 HCI_LE_BIG_TERMINATE_SYNC_CMD_OPCODE = 0x206C,
327 HCI_LE_REQ_PEER_SCA_CMD_OPCODE = 0x206D,
328 HCI_LE_SETUP_ISO_DATA_PATH_CMD_OPCODE = 0x206E,
329 HCI_LE_REMOVE_ISO_DATA_PATH_CMD_OPCODE = 0x206F,
330 HCI_LE_ISO_TX_TEST_CMD_OPCODE = 0x2070,
331 HCI_LE_ISO_RX_TEST_CMD_OPCODE = 0x2071,
332 HCI_LE_ISO_READ_TEST_COUNTERS_CMD_OPCODE = 0x2072,
333 HCI_LE_ISO_TEST_END_CMD_OPCODE = 0x2073,
334 HCI_LE_SET_HOST_FEATURE_CMD_OPCODE = 0x2074,
335 HCI_LE_RD_ISO_LINK_QUALITY_CMD_OPCODE = 0x2075,
336 HCI_LE_ENH_RD_TX_PWR_LVL_CMD_OPCODE = 0x2076,
337 HCI_LE_RD_REMOTE_TX_PWR_LVL_CMD_OPCODE = 0x2077,
338 HCI_LE_SET_PATH_LOSS_REP_PARAM_CMD_OPCODE = 0x2078,
339 HCI_LE_SET_PATH_LOSS_REP_EN_CMD_OPCODE = 0x2079,
340 HCI_LE_SET_TX_POWER_REP_EN_CMD_OPCODE = 0x207A,
341 HCI_LE_TX_TEST_V4_CMD_OPCODE = 0x207B,
342
343 HCI_LE_SET_GDX_RANGING_PARAMS_CMD_OPCODE = 0x20F9,
344 HCI_LE_START_RANGING_CMD_OPCODE = 0x20FA,
345
346 HCI_PUBLIC_ADDR_SET_CMD_OPCODE = 0x20FB,
347 HCI_LE_TIME_SYNC_EN_CMD_OPCODE = 0x20FC,
348
349 ///Debug commands - OGF = 0x3F (spec)
350 HCI_DBG_RD_MEM_CMD_OPCODE = 0xFC01,
351 HCI_DBG_WR_MEM_CMD_OPCODE = 0xFC02,
352 HCI_DBG_DEL_PAR_CMD_OPCODE = 0xFC03,
353 HCI_DBG_ID_FLASH_CMD_OPCODE = 0xFC05,
354 HCI_DBG_ER_FLASH_CMD_OPCODE = 0xFC06,
355 HCI_DBG_WR_FLASH_CMD_OPCODE = 0xFC07,
356 HCI_DBG_RD_FLASH_CMD_OPCODE = 0xFC08,
357 HCI_DBG_RD_PAR_CMD_OPCODE = 0xFC09,
358 HCI_DBG_WR_PAR_CMD_OPCODE = 0xFC0A,
359 HCI_DBG_WLAN_COEX_CMD_OPCODE = 0xFC0B,
360 HCI_DBG_WLAN_COEXTST_SCEN_CMD_OPCODE = 0xFC0D,
361 HCI_DBG_BT_SEND_LMP_CMD_OPCODE = 0xFC0E,
362 HCI_DBG_SET_LOCAL_CLOCK_CMD_OPCODE = 0xFC0F,
363 HCI_DBG_RD_KE_STATS_CMD_OPCODE = 0xFC10,
364 HCI_DBG_PLF_RESET_CMD_OPCODE = 0xFC11,
365 HCI_DBG_RD_MEM_INFO_CMD_OPCODE = 0xFC12,
366 HCI_VS_SET_PREF_SLAVE_LATENCY_CMD_OPCODE = 0xFC13,
367 HCI_VS_SET_PREF_SLAVE_EVT_DUR_CMD_OPCODE = 0xFC14,
368 HCI_VS_SET_MAX_RX_SIZE_AND_TIME_CMD_OPCODE = 0xFC15,
369 HCI_DBG_RD_CON_INFO_CMD_OPCODE = 0xFC1F,
370 HCI_DBG_BLE_REG_RD_CMD_OPCODE = 0xFC30,
371 HCI_DBG_BLE_REG_WR_CMD_OPCODE = 0xFC31,
372 HCI_DBG_SEND_LLCP_CMD_OPCODE = 0xFC35,
373 HCI_DBG_LLCP_DISCARD_CMD_OPCODE = 0xFC36,
374 HCI_DBG_RF_REG_RD_CMD_OPCODE = 0xFC39,
375 HCI_DBG_RF_REG_WR_CMD_OPCODE = 0xFC3A,
376 HCI_DBG_RF_SWITCH_CLK_CMD_OPCODE = 0xFC3C,
377 HCI_DBG_RF_WR_DATA_TX_CMD_OPCODE = 0xFC3D,
378 HCI_DBG_RF_RD_DATA_RX_CMD_OPCODE = 0xFC3E,
379 HCI_DBG_RF_CNTL_TX_CMD_OPCODE = 0xFC3F,
380 HCI_DBG_RF_SYNC_P_CNTL_CMD_OPCODE = 0xFC40,
381 HCI_TESTER_SET_LE_PARAMS_CMD_OPCODE = 0xFC40,
382 HCI_DBG_WR_DLE_DFT_VALUE_CMD_OPCODE = 0xFC41,
383 HCI_DBG_TST_LLCP_PT_EN_CMD_OPCODE = 0xFC42,
384 HCI_DBG_TST_SEND_LLCP_CMD_OPCODE = 0xFC43,
385 HCI_DBG_BT_DISCARD_LMP_EN_CMD_OPCODE = 0xFC44,
386 HCI_DBG_MWS_COEX_CMD_OPCODE = 0xFC45,
387 HCI_DBG_MWS_COEXTST_SCEN_CMD_OPCODE = 0xFC46,
388 HCI_DBG_WR_LOC_SUPP_FEATS_CMD_OPCODE = 0xFC4E,
389 HCI_DBG_RD_BASE_ADDR_CMD_OPCODE = 0xFC4F,
390 HCI_VS_RD_PICONET_CLOCK_CMD_OPCODE = 0xFC50,
391 /// Debug commands for ISO
392 HCI_DBG_ISO_SET_PARAM_CMD_OPCODE = 0xFC57,
393 HCI_DBG_CIS_SET_PARAM_CMD_OPCODE = 0xFC58,
394 HCI_DBG_BIG_SET_PARAM_CMD_OPCODE = 0xFC59,
395 HCI_VS_SET_ISO_DATA_PATH_TRIGGER_CMD_OPCODE = 0xFC5A,
396 HCI_DBG_TEST_CRYPTO_FUNC_CMD_OPCODE = 0xFC60,
397 HCI_DBG_TEST_SCH_PLAN_SET_CMD_OPCODE = 0xFC61,
398 HCI_DBG_TEST_SCH_PLAN_REM_CMD_OPCODE = 0xFC62,
399 HCI_DBG_TEST_SCH_PLAN_CHK_CMD_OPCODE = 0xFC63,
400 HCI_DBG_TEST_SCH_PLAN_REQ_CMD_OPCODE = 0xFC64,
401 HCI_DBG_IQGEN_CFG_CMD_OPCODE = 0xFC65,
402 HCI_VS_AUSY_CON_EVT_CNT_GET_CMD_OPCODE = 0xFC66,
403 HCI_VS_AUSY_EVT_TX_TIME_GET_CMD_OPCODE = 0xFC67,
404 HCI_VS_AUSY_LAST_RX_TIME_GET_CMD_OPCODE = 0xFC68,
405 HCI_VS_AUSY_CLOCK_SAMPLE_GET_CMD_OPCODE = 0xFC69,
406 HCI_VS_AUSY_CLOCK_CONVERT_CMD_OPCODE = 0xFC6A,
407 HCI_VS_AUSY_CIS_EVT_CTRL_CMD_OPCODE = 0xFC6B,
408 };
409
410 /**************************************************************************************
411 ************** HCI EVENTS ****************
412 **************************************************************************************/
413 enum hci_evt_code
414 {
415 HCI_INQ_CMP_EVT_CODE = 0x01,
416 HCI_INQ_RES_EVT_CODE = 0x02,
417 HCI_CON_CMP_EVT_CODE = 0x03,
418 HCI_CON_REQ_EVT_CODE = 0x04,
419 HCI_DISC_CMP_EVT_CODE = 0x05,
420 HCI_AUTH_CMP_EVT_CODE = 0x06,
421 HCI_REM_NAME_REQ_CMP_EVT_CODE = 0x07,
422 HCI_ENC_CHG_EVT_CODE = 0x08,
423 HCI_CHG_CON_LK_CMP_EVT_CODE = 0x09,
424 HCI_MASTER_LK_CMP_EVT_CODE = 0x0A,
425 HCI_RD_REM_SUPP_FEATS_CMP_EVT_CODE = 0x0B,
426 HCI_RD_REM_VER_INFO_CMP_EVT_CODE = 0x0C,
427 HCI_QOS_SETUP_CMP_EVT_CODE = 0x0D,
428 HCI_CMD_CMP_EVT_CODE = 0x0E,
429 HCI_CMD_STATUS_EVT_CODE = 0x0F,
430 HCI_HW_ERR_EVT_CODE = 0x10,
431 HCI_FLUSH_OCCURRED_EVT_CODE = 0x11,
432 HCI_ROLE_CHG_EVT_CODE = 0x12,
433 HCI_NB_CMP_PKTS_EVT_CODE = 0x13,
434 HCI_MODE_CHG_EVT_CODE = 0x14,
435 HCI_RETURN_LINK_KEYS_EVT_CODE = 0x15,
436 HCI_PIN_CODE_REQ_EVT_CODE = 0x16,
437 HCI_LK_REQ_EVT_CODE = 0x17,
438 HCI_LK_NOTIF_EVT_CODE = 0x18,
439 HCI_DATA_BUF_OVFLW_EVT_CODE = 0x1A,
440 HCI_MAX_SLOT_CHG_EVT_CODE = 0x1B,
441 HCI_RD_CLK_OFF_CMP_EVT_CODE = 0x1C,
442 HCI_CON_PKT_TYPE_CHG_EVT_CODE = 0x1D,
443 HCI_QOS_VIOL_EVT_CODE = 0x1E,
444 HCI_PAGE_SCAN_REPET_MODE_CHG_EVT_CODE = 0x20,
445 HCI_FLOW_SPEC_CMP_EVT_CODE = 0x21,
446 HCI_INQ_RES_WITH_RSSI_EVT_CODE = 0x22,
447 HCI_RD_REM_EXT_FEATS_CMP_EVT_CODE = 0x23,
448 HCI_SYNC_CON_CMP_EVT_CODE = 0x2C,
449 HCI_SYNC_CON_CHG_EVT_CODE = 0x2D,
450 HCI_SNIFF_SUB_EVT_CODE = 0x2E,
451 HCI_EXT_INQ_RES_EVT_CODE = 0x2F,
452 HCI_ENC_KEY_REFRESH_CMP_EVT_CODE = 0x30,
453 HCI_IO_CAP_REQ_EVT_CODE = 0x31,
454 HCI_IO_CAP_RSP_EVT_CODE = 0x32,
455 HCI_USER_CFM_REQ_EVT_CODE = 0x33,
456 HCI_USER_PASSKEY_REQ_EVT_CODE = 0x34,
457 HCI_REM_OOB_DATA_REQ_EVT_CODE = 0x35,
458 HCI_SP_CMP_EVT_CODE = 0x36,
459 HCI_LINK_SUPV_TO_CHG_EVT_CODE = 0x38,
460 HCI_ENH_FLUSH_CMP_EVT_CODE = 0x39,
461 HCI_USER_PASSKEY_NOTIF_EVT_CODE = 0x3B,
462 HCI_KEYPRESS_NOTIF_EVT_CODE = 0x3C,
463 HCI_REM_HOST_SUPP_FEATS_NOTIF_EVT_CODE = 0x3D,
464 HCI_LE_META_EVT_CODE = 0x3E,
465 HCI_MAX_EVT_MSK_PAGE_1_CODE = 0x40,
466 HCI_SYNC_TRAIN_CMP_EVT_CODE = 0x4F,
467 HCI_SYNC_TRAIN_REC_EVT_CODE = 0x50,
468 HCI_CON_SLV_BCST_REC_EVT_CODE = 0x51,
469 HCI_CON_SLV_BCST_TO_EVT_CODE = 0x52,
470 HCI_TRUNC_PAGE_CMP_EVT_CODE = 0x53,
471 HCI_SLV_PAGE_RSP_TO_EVT_CODE = 0x54,
472 HCI_CON_SLV_BCST_CH_MAP_CHG_EVT_CODE = 0x55,
473 HCI_AUTH_PAYL_TO_EXP_EVT_CODE = 0x57,
474 HCI_SAM_STATUS_CHANGE_EVT_CODE = 0x58,
475 HCI_MAX_EVT_MSK_PAGE_2_CODE = 0x59,
476 HCI_DBG_META_EVT_CODE = 0xFF,
477 };
478
479 /**************************************************************************************
480 ************** HCI LE EVENTS ****************
481 **************************************************************************************/
482 enum hci_le_evt_subcode
483 {
484 /// LE Events Subcodes
485 HCI_LE_CON_CMP_EVT_SUBCODE = 0x01,
486 HCI_LE_ADV_REPORT_EVT_SUBCODE = 0x02,
487 HCI_LE_CON_UPDATE_CMP_EVT_SUBCODE = 0x03,
488 HCI_LE_RD_REM_FEATS_CMP_EVT_SUBCODE = 0x04,
489 HCI_LE_LTK_REQUEST_EVT_SUBCODE = 0x05,
490 HCI_LE_REM_CON_PARAM_REQ_EVT_SUBCODE = 0x06,
491 HCI_LE_DATA_LEN_CHG_EVT_SUBCODE = 0x07,
492 HCI_LE_RD_LOC_P256_PUB_KEY_CMP_EVT_SUBCODE = 0x08,
493 HCI_LE_GEN_DHKEY_CMP_EVT_SUBCODE = 0x09,
494 HCI_LE_ENH_CON_CMP_EVT_SUBCODE = 0x0A,
495 HCI_LE_DIR_ADV_REP_EVT_SUBCODE = 0x0B,
496 HCI_LE_PHY_UPD_CMP_EVT_SUBCODE = 0x0C,
497 HCI_LE_EXT_ADV_REPORT_EVT_SUBCODE = 0x0D,
498 HCI_LE_PER_ADV_SYNC_EST_EVT_SUBCODE = 0x0E,
499 HCI_LE_PER_ADV_REPORT_EVT_SUBCODE = 0x0F,
500 HCI_LE_PER_ADV_SYNC_LOST_EVT_SUBCODE = 0x10,
501 HCI_LE_SCAN_TIMEOUT_EVT_SUBCODE = 0x11,
502 HCI_LE_ADV_SET_TERMINATED_EVT_SUBCODE = 0x12,
503 HCI_LE_SCAN_REQ_RCVD_EVT_SUBCODE = 0x13,
504 HCI_LE_CH_SEL_ALGO_EVT_SUBCODE = 0x14,
505 HCI_LE_CONLESS_IQ_REPORT_EVT_SUBCODE = 0x15,
506 HCI_LE_CON_IQ_REPORT_EVT_SUBCODE = 0x16,
507 HCI_LE_CTE_REQ_FAILED_EVT_SUBCODE = 0x17,
508 HCI_LE_PER_ADV_SYNC_TRANSF_REC_EVT_SUBCODE = 0x18,
509 HCI_LE_CIS_ESTABLISHED_EVT_SUBCODE = 0x19,
510 HCI_LE_CIS_REQUEST_EVT_SUBCODE = 0x1A,
511 HCI_LE_CREATE_BIG_CMP_EVT_SUBCODE = 0x1B,
512 HCI_LE_TERMINATE_BIG_CMP_EVT_SUBCODE = 0x1C,
513 HCI_LE_BIG_SYNC_ESTABLISHED_EVT_SUBCODE = 0x1D,
514 HCI_LE_BIG_SYNC_LOST_EVT_SUBCODE = 0x1E,
515 HCI_LE_REQ_PEER_SCA_CMP_EVT_SUBCODE = 0x1F,
516 HCI_LE_PATH_LOSS_THRESHOLD_EVT_SUBCODE = 0x20,
517 HCI_LE_TX_POWER_REPORTING_EVT_SUBCODE = 0x21,
518 HCI_LE_BIG_INFO_ADV_REPORT_EVT_SUBCODE = 0x22,
519
520 HCI_LE_RANGING_IND_EVT_SUBCODE = 0x31,
521 HCI_LE_RANGING_SAMPLE_REPORT_EVT_SUBCODE = 0x32,
522 HCI_LE_RANGING_CMP_EVT_SUBCODE = 0x33,
523 };
524
525 /**************************************************************************************
526 ************** TASK ID ****************
527 **************************************************************************************/
528 enum TASK_API_ID
529 {
530 TASK_ID_LLM = 0,
531 TASK_ID_LLC = 1,
532 TASK_ID_LLD = 2,
533 TASK_ID_LLI = 3,
534 TASK_ID_DBG = 4,
535 TASK_ID_LM = 5,
536 TASK_ID_LC = 6,
537 TASK_ID_LB = 7,
538 TASK_ID_LD = 8,
539 TASK_ID_SDK = 9,
540 TASK_ID_L2CC = 10,
541 TASK_ID_GATTM = 11,
542 TASK_ID_GATTC = 12,
543 TASK_ID_GAPM = 13,
544 TASK_ID_GAPC = 14,
545 TASK_ID_APP = 15,
546 TASK_ID_AHI = 16,
547 TASK_ID_HCI = 17,
548 TASK_ID_MESH = 200,
549 TASK_ID_RTLS = 250,
550 TASK_ID_INVALID = 0xFF,
551 };
552
553 /**************************************************************************************
554 ************** Message API of the HCI task ****************
555 **************************************************************************************/
556 enum hci_msg_id
557 {
558 HCI_MSG_ID_FIRST = TASK_FIRST_MSG(TASK_ID_HCI),
559
560 HCI_CMD_CMP_EVENT,
561 HCI_CMD_STAT_EVENT,
562 HCI_EVENT,
563 HCI_LE_EVENT,
564 HCI_COMMAND,
565 HCI_ACL_DATA,
566 HCI_SYNC_DATA,
567 HCI_MSG_ID_LAST
568 };
569
570 /**************************************************************************************
571 ************** Message API of the GAPC task ****************
572 **************************************************************************************/
573 enum gapc_msg_id
574 {
575 GAPC_CMP_EVT = MSG_ID(GAPC, 0x00),
576 GAPC_CONNECTION_REQ_IND = MSG_ID(GAPC, 0x01),
577 GAPC_CONNECTION_CFM = MSG_ID(GAPC, 0x02),
578 GAPC_DISCONNECT_IND = MSG_ID(GAPC, 0x03),
579 GAPC_DISCONNECT_CMD = MSG_ID(GAPC, 0x04),
580 GAPC_GET_INFO_CMD = MSG_ID(GAPC, 0x05),
581 GAPC_PEER_ATT_INFO_IND = MSG_ID(GAPC, 0x06),
582 GAPC_PEER_VERSION_IND = MSG_ID(GAPC, 0x07),
583 GAPC_PEER_FEATURES_IND = MSG_ID(GAPC, 0x08),
584 GAPC_CON_RSSI_IND = MSG_ID(GAPC, 0x09),
585 GAPC_GET_DEV_INFO_REQ_IND = MSG_ID(GAPC, 0x0A),
586 GAPC_GET_DEV_INFO_CFM = MSG_ID(GAPC, 0x0B),
587 GAPC_SET_DEV_INFO_REQ_IND = MSG_ID(GAPC, 0x0C),
588 GAPC_SET_DEV_INFO_CFM = MSG_ID(GAPC, 0x0D),
589 GAPC_PARAM_UPDATE_CMD = MSG_ID(GAPC, 0x0E),
590 GAPC_PARAM_UPDATE_REQ_IND = MSG_ID(GAPC, 0x0F),
591 GAPC_PARAM_UPDATE_CFM = MSG_ID(GAPC, 0x10),
592 GAPC_PARAM_UPDATED_IND = MSG_ID(GAPC, 0x11),
593 GAPC_BOND_CMD = MSG_ID(GAPC, 0x12),
594 GAPC_BOND_REQ_IND = MSG_ID(GAPC, 0x13),
595 GAPC_BOND_CFM = MSG_ID(GAPC, 0x14),
596 GAPC_BOND_IND = MSG_ID(GAPC, 0x15),
597 GAPC_ENCRYPT_CMD = MSG_ID(GAPC, 0x16),
598 GAPC_ENCRYPT_REQ_IND = MSG_ID(GAPC, 0x17),
599 GAPC_ENCRYPT_CFM = MSG_ID(GAPC, 0x18),
600 GAPC_ENCRYPT_IND = MSG_ID(GAPC, 0x19),
601 GAPC_SECURITY_CMD = MSG_ID(GAPC, 0x1A),
602 GAPC_SECURITY_IND = MSG_ID(GAPC, 0x1B),
603 GAPC_SIGN_COUNTER_IND = MSG_ID(GAPC, 0x1C),
604 GAPC_CON_CHANNEL_MAP_IND = MSG_ID(GAPC, 0x1D),
605 GAPC_SEC_REQ_TIMEOUT_IND = MSG_ID(GAPC, 0x1E),
606 GAPC_SET_LE_PING_TO_CMD = MSG_ID(GAPC, 0x28),
607 GAPC_LE_PING_TO_VAL_IND = MSG_ID(GAPC, 0x29),
608 GAPC_LE_PING_TO_IND = MSG_ID(GAPC, 0x2A),
609 GAPC_SET_LE_PKT_SIZE_CMD = MSG_ID(GAPC, 0x2B),
610 GAPC_LE_PKT_SIZE_IND = MSG_ID(GAPC, 0x2C),
611 GAPC_KEY_PRESS_NOTIFICATION_CMD = MSG_ID(GAPC, 0x2D),
612 GAPC_KEY_PRESS_NOTIFICATION_IND = MSG_ID(GAPC, 0x2E),
613 GAPC_SET_PHY_CMD = MSG_ID(GAPC, 0x2F),
614 GAPC_LE_PHY_IND = MSG_ID(GAPC, 0x30),
615 GAPC_CHAN_SEL_ALGO_IND = MSG_ID(GAPC, 0x31),
616 GAPC_SET_PREF_SLAVE_LATENCY_CMD = MSG_ID(GAPC, 0x32),
617 GAPC_SET_PREF_SLAVE_EVT_DUR_CMD = MSG_ID(GAPC, 0x33),
618 GAPC_UNKNOWN_MSG_IND = MSG_ID(GAPC, 0x34),
619 GAPC_PER_ADV_SYNC_TRANS_CMD = MSG_ID(GAPC, 0x35),
620 GAPC_CTE_TX_CFG_CMD = MSG_ID(GAPC, 0x38),
621 GAPC_CTE_RX_CFG_CMD = MSG_ID(GAPC, 0x39),
622 GAPC_CTE_REQ_CTRL_CMD = MSG_ID(GAPC, 0x3A),
623 GAPC_CTE_RSP_CTRL_CMD = MSG_ID(GAPC, 0x3B),
624 GAPC_CTE_IQ_REPORT_IND = MSG_ID(GAPC, 0x3C),
625 GAPC_READ_LOCAL_TX_PWR_CMD = MSG_ID(GAPC, 0x3D),
626 GAPC_READ_REMOTE_TX_PWR_CMD = MSG_ID(GAPC, 0x3E),
627 GAPC_SET_PATH_LOSS_REPORTING_PARAM_CMD = MSG_ID(GAPC, 0x3F),
628 GAPC_SET_PATH_LOSS_REPORTING_ENABLE_CMD = MSG_ID(GAPC, 0x40),
629 GAPC_SET_TX_PWR_REPORTING_ENABLE_CMD = MSG_ID(GAPC, 0x41),
630 GAPC_READ_LOCAL_TX_PWR_IND = MSG_ID(GAPC, 0x42),
631 GAPC_READ_REMOTE_TX_PWR_IND = MSG_ID(GAPC, 0x43),
632 GAPC_TX_PWR_CHANGE_REPORT_IND = MSG_ID(GAPC, 0x44),
633 GAPC_PATH_LOSS_THRESHOLD_REPORT_IND = MSG_ID(GAPC, 0x45),
634 GAPC_RANGING_START_CMD = MSG_ID(GAPC, 0x46),
635 GAPC_RANGING_IND = MSG_ID(GAPC, 0x47),
636 GAPC_RANGING_SAMPLE_REPORT_IND = MSG_ID(GAPC, 0x48),
637 GAPC_RANGING_CMP_IND = MSG_ID(GAPC, 0x49),
638 GAPC_SIGN_CMD = MSG_ID(GAPC, 0xF0),
639 GAPC_SIGN_IND = MSG_ID(GAPC, 0xF1),
640 GAPC_PARAM_UPDATE_TO_IND = MSG_ID(GAPC, 0xF2),
641 GAPC_SMP_TIMEOUT_TIMER_IND = MSG_ID(GAPC, 0xF3),
642 GAPC_SMP_REP_ATTEMPTS_TIMER_IND = MSG_ID(GAPC, 0xF4),
643 };
644
645 /**************************************************************************************
646 ************** Message API of the GAPM task ****************
647 **************************************************************************************/
648 enum gapm_msg_id
649 {
650 GAPM_CMP_EVT = MSG_ID(GAPM, 0x00),
651 GAPM_RESET_CMD = MSG_ID(GAPM, 0x02),
652 GAPM_SET_DEV_CONFIG_CMD = MSG_ID(GAPM, 0x04),
653 GAPM_SET_CHANNEL_MAP_CMD = MSG_ID(GAPM, 0x05),
654 GAPM_GET_DEV_INFO_CMD = MSG_ID(GAPM, 0x06),
655 GAPM_DEV_VERSION_IND = MSG_ID(GAPM, 0x07),
656 GAPM_DEV_BDADDR_IND = MSG_ID(GAPM, 0x08),
657 GAPM_DEV_ADV_TX_POWER_IND = MSG_ID(GAPM, 0x09),
658 GAPM_DBG_MEM_INFO_IND = MSG_ID(GAPM, 0x0A),
659 GAPM_ANTENNA_INF_IND = MSG_ID(GAPM, 0x0B),
660 GAPM_RESOLV_ADDR_CMD = MSG_ID(GAPM, 0x14),
661 GAPM_ADDR_SOLVED_IND = MSG_ID(GAPM, 0x15),
662 GAPM_GEN_RAND_ADDR_CMD = MSG_ID(GAPM, 0x16),
663 GAPM_USE_ENC_BLOCK_CMD = MSG_ID(GAPM, 0x17),
664 GAPM_USE_ENC_BLOCK_IND = MSG_ID(GAPM, 0x18),
665 GAPM_GEN_RAND_NB_CMD = MSG_ID(GAPM, 0x19),
666 GAPM_GEN_RAND_NB_IND = MSG_ID(GAPM, 0x1A),
667 GAPM_PROFILE_TASK_ADD_CMD = MSG_ID(GAPM, 0x1B),
668 GAPM_PROFILE_ADDED_IND = MSG_ID(GAPM, 0x1C),
669 GAPM_UNKNOWN_TASK_IND = MSG_ID(GAPM, 0x1D),
670 GAPM_SUGG_DFLT_DATA_LEN_IND = MSG_ID(GAPM, 0x1E),
671 GAPM_MAX_DATA_LEN_IND = MSG_ID(GAPM, 0x1F),
672 GAPM_RAL_ADDR_IND = MSG_ID(GAPM, 0x22),
673 GAPM_SET_IRK_CMD = MSG_ID(GAPM, 0x23),
674 GAPM_LEPSM_REGISTER_CMD = MSG_ID(GAPM, 0x24),
675 GAPM_LEPSM_UNREGISTER_CMD = MSG_ID(GAPM, 0x25),
676 GAPM_LE_TEST_MODE_CTRL_CMD = MSG_ID(GAPM, 0x26),
677 GAPM_LE_TEST_END_IND = MSG_ID(GAPM, 0x27),
678 GAPM_LE_TEST_IQ_REPORT_IND = MSG_ID(GAPM, 0x2D),
679 GAPM_ISO_STAT_IND = MSG_ID(GAPM, 0x28),
680 GAPM_GEN_DH_KEY_CMD = MSG_ID(GAPM, 0x29),
681 GAPM_GEN_DH_KEY_IND = MSG_ID(GAPM, 0x2A),
682 GAPM_GET_PUB_KEY_CMD = MSG_ID(GAPM, 0x2B),
683 GAPM_PUB_KEY_IND = MSG_ID(GAPM, 0x2C),
684 GAPM_GET_RAL_ADDR_CMD = MSG_ID(GAPM, 0x90),
685 GAPM_LIST_SET_CMD = MSG_ID(GAPM, 0x91),
686 GAPM_LIST_SIZE_IND = MSG_ID(GAPM, 0x92),
687 GAPM_ACTIVITY_CREATE_CMD = MSG_ID(GAPM, 0xA0),
688 GAPM_ACTIVITY_START_CMD = MSG_ID(GAPM, 0xA1),
689 GAPM_ACTIVITY_STOP_CMD = MSG_ID(GAPM, 0xA2),
690 GAPM_ACTIVITY_DELETE_CMD = MSG_ID(GAPM, 0xA3),
691 GAPM_ACTIVITY_CREATED_IND = MSG_ID(GAPM, 0xA4),
692 GAPM_ACTIVITY_STOPPED_IND = MSG_ID(GAPM, 0xA5),
693 GAPM_SET_ADV_DATA_CMD = MSG_ID(GAPM, 0xA6),
694 GAPM_EXT_ADV_REPORT_IND = MSG_ID(GAPM, 0xA7),
695 GAPM_SCAN_REQUEST_IND = MSG_ID(GAPM, 0xA8),
696 GAPM_SYNC_ESTABLISHED_IND = MSG_ID(GAPM, 0xA9),
697 GAPM_MAX_ADV_DATA_LEN_IND = MSG_ID(GAPM, 0xAA),
698 GAPM_NB_ADV_SETS_IND = MSG_ID(GAPM, 0xAB),
699 GAPM_DEV_TX_PWR_IND = MSG_ID(GAPM, 0xAC),
700 GAPM_DEV_RF_PATH_COMP_IND = MSG_ID(GAPM, 0xAD),
701 GAPM_UNKNOWN_MSG_IND = MSG_ID(GAPM, 0xAE),
702 GAPM_PER_ADV_REPORT_CTRL_CMD = MSG_ID(GAPM, 0xAF),
703 GAPM_PER_SYNC_IQ_SAMPLING_CTRL_CMD = MSG_ID(GAPM, 0xB0),
704 GAPM_PER_ADV_IQ_REPORT_IND = MSG_ID(GAPM, 0xB1),
705 GAPM_PER_ADV_CTE_TX_CTL_CMD = MSG_ID(GAPM, 0xB2),
706 GAPM_PER_ADV_CTE_TX_PARAM_SET_CMD = MSG_ID(GAPM, 0xB3),
707 GAPM_DBG_IQGEN_CFG_CMD = MSG_ID(GAPM, 0x50),
708 GAPM_UNKNOWN_TASK_MSG = MSG_ID(GAPM, 0xF0),
709 GAPM_ADDR_RENEW_TO_IND = MSG_ID(GAPM, 0xF1),
710 GAPM_AUTO_CONN_TO_IND = MSG_ID(GAPM, 0xF2),
711 GAPM_ADDR_RENEW_CMD = MSG_ID(GAPM, 0xF3),
712 GAPM_PUBLIC_ADDR_SET_CMD = MSG_ID(GAPM, 0xF4),
713 GAPM_SET_GDX_RANGING_PARAM_CMD = MSG_ID(GAPM, 0xF5),
714 };
715
716 /**************************************************************************************
717 ************** Message API of the GATTC task ****************
718 **************************************************************************************/
719 enum gattc_msg_id
720 {
721 GATTC_CMP_EVT = TASK_FIRST_MSG(TASK_ID_GATTC),
722 GATTC_EXC_MTU_CMD,
723 GATTC_MTU_CHANGED_IND,
724 GATTC_DISC_CMD,
725 GATTC_DISC_SVC_IND,
726 GATTC_DISC_SVC_INCL_IND,
727 GATTC_DISC_CHAR_IND,
728 GATTC_DISC_CHAR_DESC_IND,
729 GATTC_READ_CMD,
730 GATTC_READ_IND,
731 GATTC_WRITE_CMD,
732 GATTC_EXECUTE_WRITE_CMD,
733 GATTC_EVENT_IND,
734 GATTC_EVENT_REQ_IND,
735 GATTC_EVENT_CFM,
736 GATTC_REG_TO_PEER_EVT_CMD,
737 GATTC_SEND_EVT_CMD,
738 GATTC_SEND_SVC_CHANGED_CMD,
739 GATTC_SVC_CHANGED_CFG_IND,
740 GATTC_READ_REQ_IND,
741 GATTC_READ_CFM,
742 GATTC_WRITE_REQ_IND,
743 GATTC_WRITE_CFM,
744 GATTC_ATT_INFO_REQ_IND,
745 GATTC_ATT_INFO_CFM,
746 GATTC_SDP_SVC_DISC_CMD,
747 GATTC_SDP_SVC_IND,
748 GATTC_TRANSACTION_TO_ERROR_IND,
749 GATTC_UNKNOWN_MSG_IND,
750 GATTC_CLIENT_RTX_IND,
751 GATTC_SERVER_RTX_IND,
752 };
753
754 /**************************************************************************************
755 ************** Message API of the L2CC task ****************
756 **************************************************************************************/
757
758 /// Number of L2CC Deprecated messages
759 #define L2CC_NB_DEPRECATED_MSG (4)
760
761 enum l2cc_msg_id
762 {
763 L2CC_CMP_EVT = TASK_FIRST_MSG(TASK_ID_L2CC) + L2CC_NB_DEPRECATED_MSG,
764 L2CC_LECB_CONNECT_CMD,
765 L2CC_LECB_CONNECT_REQ_IND,
766 L2CC_LECB_CONNECT_CFM,
767 L2CC_LECB_CONNECT_IND,
768 L2CC_LECB_DISCONNECT_CMD,
769 L2CC_LECB_DISCONNECT_IND,
770 L2CC_LECB_ADD_CMD,
771 L2CC_LECB_ADD_IND,
772 L2CC_LECB_SDU_SEND_CMD,
773 L2CC_LECB_SDU_RECV_IND,
774 L2CC_UNKNOWN_MSG_IND,
775 L2CC_DBG_PDU_SEND_CMD,
776 L2CC_DBG_PDU_RECV_IND,
777 L2CC_PDU_SEND_CMD,
778 L2CC_PDU_RECV_IND,
779 L2CC_SIGNALING_TRANS_TO_IND,
780 };
781
782 #endif // CO_HCI_H_
783
HCI_DBG_BT_DISCARD_LMP_EN_CMD_OPCODE
@ HCI_DBG_BT_DISCARD_LMP_EN_CMD_OPCODE
Definition: ble_id.h:385
HCI_WR_PAGE_SCAN_TYPE_CMD_OPCODE
@ HCI_WR_PAGE_SCAN_TYPE_CMD_OPCODE
Definition: ble_id.h:144
HCI_LE_SET_CONLESS_CTE_TX_PARAM_CMD_OPCODE
@ HCI_LE_SET_CONLESS_CTE_TX_PARAM_CMD_OPCODE
Definition: ble_id.h:299
HCI_LE_SCAN_REQ_RCVD_EVT_SUBCODE
@ HCI_LE_SCAN_REQ_RCVD_EVT_SUBCODE
Definition: ble_id.h:503
HCI_LE_GEN_DHKEY_CMP_EVT_SUBCODE
@ HCI_LE_GEN_DHKEY_CMP_EVT_SUBCODE
Definition: ble_id.h:493
HCI_DBG_RF_CNTL_TX_CMD_OPCODE
@ HCI_DBG_RF_CNTL_TX_CMD_OPCODE
Definition: ble_id.h:379
GATTC_DISC_SVC_INCL_IND
@ GATTC_DISC_SVC_INCL_IND
Definition: ble_id.h:726
HCI_WR_NB_BDCST_RETX_CMD_OPCODE
@ HCI_WR_NB_BDCST_RETX_CMD_OPCODE
Definition: ble_id.h:124
HCI_VS_AUSY_CLOCK_CONVERT_CMD_OPCODE
@ HCI_VS_AUSY_CLOCK_CONVERT_CMD_OPCODE
Definition: ble_id.h:406
HCI_RD_INQ_RSP_TX_PWR_LVL_CMD_OPCODE
@ HCI_RD_INQ_RSP_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:153
TASK_ID_LLC
@ TASK_ID_LLC
Definition: ble_id.h:531
GAPM_GEN_DH_KEY_IND
@ GAPM_GEN_DH_KEY_IND
Definition: ble_id.h:681
HCI_RD_FLOW_CNTL_MODE_CMD_OPCODE
@ HCI_RD_FLOW_CNTL_MODE_CMD_OPCODE
Definition: ble_id.h:160
HCI_LE_SET_PATH_LOSS_REP_EN_CMD_OPCODE
@ HCI_LE_SET_PATH_LOSS_REP_EN_CMD_OPCODE
Definition: ble_id.h:339
GAPC_CTE_RSP_CTRL_CMD
@ GAPC_CTE_RSP_CTRL_CMD
Definition: ble_id.h:623
GAPM_EXT_ADV_REPORT_IND
@ GAPM_EXT_ADV_REPORT_IND
Definition: ble_id.h:694
HCI_DBG_ID_FLASH_CMD_OPCODE
@ HCI_DBG_ID_FLASH_CMD_OPCODE
Definition: ble_id.h:353
HCI_LE_ISO_TX_TEST_CMD_OPCODE
@ HCI_LE_ISO_TX_TEST_CMD_OPCODE
Definition: ble_id.h:330
GAPM_UNKNOWN_TASK_MSG
@ GAPM_UNKNOWN_TASK_MSG
Definition: ble_id.h:708
GAPC_BOND_CMD
@ GAPC_BOND_CMD
Definition: ble_id.h:593
HCI_DBG_TEST_SCH_PLAN_CHK_CMD_OPCODE
@ HCI_DBG_TEST_SCH_PLAN_CHK_CMD_OPCODE
Definition: ble_id.h:399
HCI_WR_EXT_INQ_LEN_CMD_OPCODE
@ HCI_WR_EXT_INQ_LEN_CMD_OPCODE
Definition: ble_id.h:184
HCI_LE_PER_ADV_SYNC_TRANSF_CMD_OPCODE
@ HCI_LE_PER_ADV_SYNC_TRANSF_CMD_OPCODE
Definition: ble_id.h:308
HCI_HOST_NB_CMP_PKTS_CMD_OPCODE
@ HCI_HOST_NB_CMP_PKTS_CMD_OPCODE
Definition: ble_id.h:132
HCI_LE_SET_EXT_ADV_PARAM_CMD_OPCODE
@ HCI_LE_SET_EXT_ADV_PARAM_CMD_OPCODE
Definition: ble_id.h:272
HCI_WR_EXT_PAGE_TO_CMD_OPCODE
@ HCI_WR_EXT_PAGE_TO_CMD_OPCODE
Definition: ble_id.h:182
HCI_RD_LE_HOST_SUPP_CMD_OPCODE
@ HCI_RD_LE_HOST_SUPP_CMD_OPCODE
Definition: ble_id.h:163
GAPM_SET_IRK_CMD
@ GAPM_SET_IRK_CMD
Definition: ble_id.h:673
HCI_LE_CLEAR_WLST_CMD_OPCODE
@ HCI_LE_CLEAR_WLST_CMD_OPCODE
Definition: ble_id.h:234
HCI_RD_LOCAL_EXT_FEATS_CMD_OPCODE
@ HCI_RD_LOCAL_EXT_FEATS_CMD_OPCODE
Definition: ble_id.h:192
GAPC_CTE_REQ_CTRL_CMD
@ GAPC_CTE_REQ_CTRL_CMD
Definition: ble_id.h:622
GAPM_DEV_BDADDR_IND
@ GAPM_DEV_BDADDR_IND
Definition: ble_id.h:656
HCI_DBG_RD_MEM_CMD_OPCODE
@ HCI_DBG_RD_MEM_CMD_OPCODE
Debug commands - OGF = 0x3F (spec)
Definition: ble_id.h:350
HCI_DBG_META_EVT_CODE
@ HCI_DBG_META_EVT_CODE
Definition: ble_id.h:476
HCI_NO_OPERATION_CMD_OPCODE
@ HCI_NO_OPERATION_CMD_OPCODE
Definition: ble_id.h:27
HCI_LE_RD_SUPP_STATES_CMD_OPCODE
@ HCI_LE_RD_SUPP_STATES_CMD_OPCODE
Definition: ble_id.h:246
HCI_DBG_WLAN_COEXTST_SCEN_CMD_OPCODE
@ HCI_DBG_WLAN_COEXTST_SCEN_CMD_OPCODE
Definition: ble_id.h:360
HCI_RD_INQ_SCAN_ACT_CMD_OPCODE
@ HCI_RD_INQ_SCAN_ACT_CMD_OPCODE
Definition: ble_id.h:113
GAPC_GET_DEV_INFO_CFM
@ GAPC_GET_DEV_INFO_CFM
Definition: ble_id.h:586
HCI_DISCONNECT_CMD_OPCODE
@ HCI_DISCONNECT_CMD_OPCODE
Definition: ble_id.h:35
HCI_LE_CLEAR_ADV_SETS_CMD_OPCODE
@ HCI_LE_CLEAR_ADV_SETS_CMD_OPCODE
Definition: ble_id.h:279
HCI_LE_CREATE_BIG_CMP_EVT_SUBCODE
@ HCI_LE_CREATE_BIG_CMP_EVT_SUBCODE
Definition: ble_id.h:511
GATTC_DISC_CHAR_IND
@ GATTC_DISC_CHAR_IND
Definition: ble_id.h:727
HCI_SET_EXTERNAL_FRAME_CONFIG_CMD_OPCODE
@ HCI_SET_EXTERNAL_FRAME_CONFIG_CMD_OPCODE
Definition: ble_id.h:166
GAPM_PUB_KEY_IND
@ GAPM_PUB_KEY_IND
Definition: ble_id.h:683
HCI_LE_SET_DATA_LEN_CMD_OPCODE
@ HCI_LE_SET_DATA_LEN_CMD_OPCODE
Definition: ble_id.h:252
GAPM_PROFILE_ADDED_IND
@ GAPM_PROFILE_ADDED_IND
Definition: ble_id.h:668
GAPC_SET_TX_PWR_REPORTING_ENABLE_CMD
@ GAPC_SET_TX_PWR_REPORTING_ENABLE_CMD
Definition: ble_id.h:629
HCI_VS_AUSY_CIS_EVT_CTRL_CMD_OPCODE
@ HCI_VS_AUSY_CIS_EVT_CTRL_CMD_OPCODE
Definition: ble_id.h:407
HCI_LE_DATA_LEN_CHG_EVT_SUBCODE
@ HCI_LE_DATA_LEN_CHG_EVT_SUBCODE
Definition: ble_id.h:491
HCI_LE_SET_ADV_PARAM_CMD_OPCODE
@ HCI_LE_SET_ADV_PARAM_CMD_OPCODE
Definition: ble_id.h:224
GAPM_GET_RAL_ADDR_CMD
@ GAPM_GET_RAL_ADDR_CMD
Definition: ble_id.h:684
GAPM_SET_GDX_RANGING_PARAM_CMD
@ GAPM_SET_GDX_RANGING_PARAM_CMD
Definition: ble_id.h:713
HCI_EXT_INQ_RES_EVT_CODE
@ HCI_EXT_INQ_RES_EVT_CODE
Definition: ble_id.h:451
HCI_NB_CMP_PKTS_EVT_CODE
@ HCI_NB_CMP_PKTS_EVT_CODE
Definition: ble_id.h:433
HCI_REJECT_SYNC_CON_REQ_CMD_OPCODE
@ HCI_REJECT_SYNC_CON_REQ_CMD_OPCODE
Definition: ble_id.h:57
HCI_RD_BD_ADDR_CMD_OPCODE
@ HCI_RD_BD_ADDR_CMD_OPCODE
Definition: ble_id.h:194
HCI_LE_RD_RSLV_LIST_SIZE_CMD_OPCODE
@ HCI_LE_RD_RSLV_LIST_SIZE_CMD_OPCODE
Definition: ble_id.h:260
HCI_LE_SET_RAND_ADDR_CMD_OPCODE
@ HCI_LE_SET_RAND_ADDR_CMD_OPCODE
Definition: ble_id.h:223
HCI_LE_PER_ADV_SET_INFO_TRANSF_CMD_OPCODE
@ HCI_LE_PER_ADV_SET_INFO_TRANSF_CMD_OPCODE
Definition: ble_id.h:309
HCI_SYNC_CON_CHG_EVT_CODE
@ HCI_SYNC_CON_CHG_EVT_CODE
Definition: ble_id.h:449
HCI_LE_SET_ADV_EN_CMD_OPCODE
@ HCI_LE_SET_ADV_EN_CMD_OPCODE
Definition: ble_id.h:228
GAPC_READ_LOCAL_TX_PWR_IND
@ GAPC_READ_LOCAL_TX_PWR_IND
Definition: ble_id.h:630
HCI_REM_NAME_REQ_CMP_EVT_CODE
@ HCI_REM_NAME_REQ_CMP_EVT_CODE
Definition: ble_id.h:421
HCI_RD_VOICE_STG_CMD_OPCODE
@ HCI_RD_VOICE_STG_CMD_OPCODE
Definition: ble_id.h:119
HCI_EXIT_SNIFF_MODE_CMD_OPCODE
@ HCI_EXIT_SNIFF_MODE_CMD_OPCODE
Definition: ble_id.h:79
GAPC_SET_DEV_INFO_REQ_IND
@ GAPC_SET_DEV_INFO_REQ_IND
Definition: ble_id.h:587
HCI_TRUNC_PAGE_CMP_EVT_CODE
@ HCI_TRUNC_PAGE_CMP_EVT_CODE
Definition: ble_id.h:470
GAPM_SUGG_DFLT_DATA_LEN_IND
@ GAPM_SUGG_DFLT_DATA_LEN_IND
Definition: ble_id.h:670
HCI_LE_BIG_CREATE_SYNC_CMD_OPCODE
@ HCI_LE_BIG_CREATE_SYNC_CMD_OPCODE
Definition: ble_id.h:325
HCI_WR_FLOW_CNTL_MODE_CMD_OPCODE
@ HCI_WR_FLOW_CNTL_MODE_CMD_OPCODE
Definition: ble_id.h:161
HCI_LE_RD_CHNL_MAP_CMD_OPCODE
@ HCI_LE_RD_CHNL_MAP_CMD_OPCODE
Definition: ble_id.h:239
HCI_RD_REM_EXT_FEATS_CMD_OPCODE
@ HCI_RD_REM_EXT_FEATS_CMD_OPCODE
Definition: ble_id.h:51
HCI_DBG_RD_MEM_INFO_CMD_OPCODE
@ HCI_DBG_RD_MEM_INFO_CMD_OPCODE
Definition: ble_id.h:365
HCI_MSG_ID_LAST
@ HCI_MSG_ID_LAST
Definition: ble_id.h:567
HCI_DBG_SET_LOCAL_CLOCK_CMD_OPCODE
@ HCI_DBG_SET_LOCAL_CLOCK_CMD_OPCODE
Definition: ble_id.h:362
HCI_RD_INQ_SCAN_TYPE_CMD_OPCODE
@ HCI_RD_INQ_SCAN_TYPE_CMD_OPCODE
Definition: ble_id.h:139
L2CC_LECB_DISCONNECT_CMD
@ L2CC_LECB_DISCONNECT_CMD
Definition: ble_id.h:768
GAPC_TX_PWR_CHANGE_REPORT_IND
@ GAPC_TX_PWR_CHANGE_REPORT_IND
Definition: ble_id.h:632
GAPC_CONNECTION_CFM
@ GAPC_CONNECTION_CFM
Definition: ble_id.h:577
HCI_WR_LINK_POL_STG_CMD_OPCODE
@ HCI_WR_LINK_POL_STG_CMD_OPCODE
Definition: ble_id.h:86
HCI_LE_SET_DFT_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE
@ HCI_LE_SET_DFT_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE
Definition: ble_id.h:311
HCI_LE_CTE_REQ_FAILED_EVT_SUBCODE
@ HCI_LE_CTE_REQ_FAILED_EVT_SUBCODE
Definition: ble_id.h:507
GAPM_LIST_SET_CMD
@ GAPM_LIST_SET_CMD
Definition: ble_id.h:685
HCI_DBG_TEST_SCH_PLAN_SET_CMD_OPCODE
@ HCI_DBG_TEST_SCH_PLAN_SET_CMD_OPCODE
Definition: ble_id.h:397
HCI_DBG_WR_DLE_DFT_VALUE_CMD_OPCODE
@ HCI_DBG_WR_DLE_DFT_VALUE_CMD_OPCODE
Definition: ble_id.h:382
GAPM_GET_DEV_INFO_CMD
@ GAPM_GET_DEV_INFO_CMD
Definition: ble_id.h:654
GAPC_KEY_PRESS_NOTIFICATION_CMD
@ GAPC_KEY_PRESS_NOTIFICATION_CMD
Definition: ble_id.h:611
HCI_MAX_SLOT_CHG_EVT_CODE
@ HCI_MAX_SLOT_CHG_EVT_CODE
Definition: ble_id.h:440
HCI_WR_HOLD_MODE_ACTIVITY_CMD_OPCODE
@ HCI_WR_HOLD_MODE_ACTIVITY_CMD_OPCODE
Definition: ble_id.h:126
GATTC_UNKNOWN_MSG_IND
@ GATTC_UNKNOWN_MSG_IND
Definition: ble_id.h:749
HCI_LE_SET_RSLV_PRIV_ADDR_TO_CMD_OPCODE
@ HCI_LE_SET_RSLV_PRIV_ADDR_TO_CMD_OPCODE
Definition: ble_id.h:264
HCI_LE_SET_CIG_PARAMS_TEST_CMD_OPCODE
@ HCI_LE_SET_CIG_PARAMS_TEST_CMD_OPCODE
Definition: ble_id.h:317
HCI_LE_RD_SUGGTED_DFT_DATA_LEN_CMD_OPCODE
@ HCI_LE_RD_SUGGTED_DFT_DATA_LEN_CMD_OPCODE
Definition: ble_id.h:253
GATTC_READ_IND
@ GATTC_READ_IND
Definition: ble_id.h:730
HCI_LE_RD_ADV_CHNL_TX_PW_CMD_OPCODE
@ HCI_LE_RD_ADV_CHNL_TX_PW_CMD_OPCODE
Definition: ble_id.h:225
GAPM_MAX_ADV_DATA_LEN_IND
@ GAPM_MAX_ADV_DATA_LEN_IND
Definition: ble_id.h:697
hci_le_evt_subcode
hci_le_evt_subcode
Definition: ble_id.h:483
HCI_LE_SET_PER_ADV_EN_CMD_OPCODE
@ HCI_LE_SET_PER_ADV_EN_CMD_OPCODE
Definition: ble_id.h:282
HCI_LE_SET_GDX_RANGING_PARAMS_CMD_OPCODE
@ HCI_LE_SET_GDX_RANGING_PARAMS_CMD_OPCODE
Definition: ble_id.h:343
TASK_ID_HCI
@ TASK_ID_HCI
Definition: ble_id.h:547
HCI_ENH_FLUSH_CMD_OPCODE
@ HCI_ENH_FLUSH_CMD_OPCODE
Definition: ble_id.h:157
HCI_PUBLIC_ADDR_SET_CMD_OPCODE
@ HCI_PUBLIC_ADDR_SET_CMD_OPCODE
Definition: ble_id.h:346
TASK_ID_INVALID
@ TASK_ID_INVALID
Definition: ble_id.h:550
GAPC_SMP_REP_ATTEMPTS_TIMER_IND
@ GAPC_SMP_REP_ATTEMPTS_TIMER_IND
Definition: ble_id.h:642
GAPC_SET_PHY_CMD
@ GAPC_SET_PHY_CMD
Definition: ble_id.h:613
HCI_RD_NB_SUPP_IAC_CMD_OPCODE
@ HCI_RD_NB_SUPP_IAC_CMD_OPCODE
Definition: ble_id.h:135
HCI_RD_LOC_OOB_DATA_CMD_OPCODE
@ HCI_RD_LOC_OOB_DATA_CMD_OPCODE
Definition: ble_id.h:152
HCI_QOS_SETUP_CMD_OPCODE
@ HCI_QOS_SETUP_CMD_OPCODE
Definition: ble_id.h:82
HCI_DBG_IQGEN_CFG_CMD_OPCODE
@ HCI_DBG_IQGEN_CFG_CMD_OPCODE
Definition: ble_id.h:401
HCI_DBG_RF_REG_WR_CMD_OPCODE
@ HCI_DBG_RF_REG_WR_CMD_OPCODE
Definition: ble_id.h:375
HCI_LE_PER_ADV_REPORT_EVT_SUBCODE
@ HCI_LE_PER_ADV_REPORT_EVT_SUBCODE
Definition: ble_id.h:499
HCI_DBG_RF_RD_DATA_RX_CMD_OPCODE
@ HCI_DBG_RF_RD_DATA_RX_CMD_OPCODE
Definition: ble_id.h:378
HCI_DBG_RF_SYNC_P_CNTL_CMD_OPCODE
@ HCI_DBG_RF_SYNC_P_CNTL_CMD_OPCODE
Definition: ble_id.h:380
HCI_DBG_LLCP_DISCARD_CMD_OPCODE
@ HCI_DBG_LLCP_DISCARD_CMD_OPCODE
Definition: ble_id.h:373
HCI_RD_AFH_CH_ASSESS_MODE_CMD_OPCODE
@ HCI_RD_AFH_CH_ASSESS_MODE_CMD_OPCODE
Definition: ble_id.h:145
GAPM_PER_ADV_CTE_TX_PARAM_SET_CMD
@ GAPM_PER_ADV_CTE_TX_PARAM_SET_CMD
Definition: ble_id.h:706
HCI_WR_SEC_CON_TEST_MODE_CMD_OPCODE
@ HCI_WR_SEC_CON_TEST_MODE_CMD_OPCODE
Definition: ble_id.h:217
HCI_CON_SLV_BCST_REC_EVT_CODE
@ HCI_CON_SLV_BCST_REC_EVT_CODE
Definition: ble_id.h:468
HCI_LK_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_LK_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:40
HCI_RD_LINK_SUPV_TO_CMD_OPCODE
@ HCI_RD_LINK_SUPV_TO_CMD_OPCODE
Definition: ble_id.h:133
HCI_LE_CON_UPDATE_CMP_EVT_SUBCODE
@ HCI_LE_CON_UPDATE_CMP_EVT_SUBCODE
Definition: ble_id.h:487
GAPM_ACTIVITY_CREATE_CMD
@ GAPM_ACTIVITY_CREATE_CMD
Definition: ble_id.h:687
HCI_RD_PAGE_SCAN_ACT_CMD_OPCODE
@ HCI_RD_PAGE_SCAN_ACT_CMD_OPCODE
Definition: ble_id.h:111
GATTC_EXC_MTU_CMD
@ GATTC_EXC_MTU_CMD
Definition: ble_id.h:722
HCI_DBG_TST_SEND_LLCP_CMD_OPCODE
@ HCI_DBG_TST_SEND_LLCP_CMD_OPCODE
Definition: ble_id.h:384
GAPM_DEV_RF_PATH_COMP_IND
@ GAPM_DEV_RF_PATH_COMP_IND
Definition: ble_id.h:700
GAPC_DISCONNECT_CMD
@ GAPC_DISCONNECT_CMD
Definition: ble_id.h:579
HCI_LE_CON_IQ_REPORT_EVT_SUBCODE
@ HCI_LE_CON_IQ_REPORT_EVT_SUBCODE
Definition: ble_id.h:506
HCI_FLUSH_CMD_OPCODE
@ HCI_FLUSH_CMD_OPCODE
Definition: ble_id.h:96
HCI_DBG_RD_BASE_ADDR_CMD_OPCODE
@ HCI_DBG_RD_BASE_ADDR_CMD_OPCODE
Definition: ble_id.h:389
HCI_MASTER_LK_CMD_OPCODE
@ HCI_MASTER_LK_CMD_OPCODE
Definition: ble_id.h:47
GATTC_TRANSACTION_TO_ERROR_IND
@ GATTC_TRANSACTION_TO_ERROR_IND
Definition: ble_id.h:748
HCI_RD_SYNC_TRAIN_PARAM_CMD_OPCODE
@ HCI_RD_SYNC_TRAIN_PARAM_CMD_OPCODE
Definition: ble_id.h:174
HCI_LE_SET_CIG_PARAMS_CMD_OPCODE
@ HCI_LE_SET_CIG_PARAMS_CMD_OPCODE
Definition: ble_id.h:316
HCI_SET_MWS_SCAN_FREQ_TABLE_CMD_OPCODE
@ HCI_SET_MWS_SCAN_FREQ_TABLE_CMD_OPCODE
Definition: ble_id.h:169
HCI_TESTER_SET_LE_PARAMS_CMD_OPCODE
@ HCI_TESTER_SET_LE_PARAMS_CMD_OPCODE
Definition: ble_id.h:381
HCI_RD_REM_VER_INFO_CMP_EVT_CODE
@ HCI_RD_REM_VER_INFO_CMP_EVT_CODE
Definition: ble_id.h:426
HCI_LE_EXT_ADV_REPORT_EVT_SUBCODE
@ HCI_LE_EXT_ADV_REPORT_EVT_SUBCODE
Definition: ble_id.h:497
HCI_RETURN_LINK_KEYS_EVT_CODE
@ HCI_RETURN_LINK_KEYS_EVT_CODE
Definition: ble_id.h:435
HCI_WR_AUTH_PAYL_TO_CMD_OPCODE
@ HCI_WR_AUTH_PAYL_TO_CMD_OPCODE
Definition: ble_id.h:179
HCI_WR_SYNC_TRAIN_PARAM_CMD_OPCODE
@ HCI_WR_SYNC_TRAIN_PARAM_CMD_OPCODE
Definition: ble_id.h:175
HCI_RD_SYNC_FLOW_CTRL_EN_CMD_OPCODE
@ HCI_RD_SYNC_FLOW_CTRL_EN_CMD_OPCODE
Definition: ble_id.h:128
HCI_ROLE_DISCOVERY_CMD_OPCODE
@ HCI_ROLE_DISCOVERY_CMD_OPCODE
Definition: ble_id.h:83
GAPC_SET_PATH_LOSS_REPORTING_ENABLE_CMD
@ GAPC_SET_PATH_LOSS_REPORTING_ENABLE_CMD
Definition: ble_id.h:628
HCI_LE_REMOVE_ISO_DATA_PATH_CMD_OPCODE
@ HCI_LE_REMOVE_ISO_DATA_PATH_CMD_OPCODE
Definition: ble_id.h:329
HCI_DBG_PLF_RESET_CMD_OPCODE
@ HCI_DBG_PLF_RESET_CMD_OPCODE
Definition: ble_id.h:364
HCI_LE_RMV_DEV_FROM_PER_ADV_LIST_CMD_OPCODE
@ HCI_LE_RMV_DEV_FROM_PER_ADV_LIST_CMD_OPCODE
Definition: ble_id.h:290
GAPC_BOND_REQ_IND
@ GAPC_BOND_REQ_IND
Definition: ble_id.h:594
HCI_RD_LOCAL_SUPP_CTRL_DELAY_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_CTRL_DELAY_CMD_OPCODE
Definition: ble_id.h:200
GAPC_PARAM_UPDATE_CFM
@ GAPC_PARAM_UPDATE_CFM
Definition: ble_id.h:591
HCI_SAM_STATUS_CHANGE_EVT_CODE
@ HCI_SAM_STATUS_CHANGE_EVT_CODE
Definition: ble_id.h:474
HCI_FLUSH_OCCURRED_EVT_CODE
@ HCI_FLUSH_OCCURRED_EVT_CODE
Definition: ble_id.h:431
L2CC_DBG_PDU_RECV_IND
@ L2CC_DBG_PDU_RECV_IND
Definition: ble_id.h:776
GAPC_READ_LOCAL_TX_PWR_CMD
@ GAPC_READ_LOCAL_TX_PWR_CMD
Definition: ble_id.h:625
HCI_LE_RD_REMOTE_TX_PWR_LVL_CMD_OPCODE
@ HCI_LE_RD_REMOTE_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:337
GAPC_READ_REMOTE_TX_PWR_IND
@ GAPC_READ_REMOTE_TX_PWR_IND
Definition: ble_id.h:631
HCI_LE_SETUP_ISO_DATA_PATH_CMD_OPCODE
@ HCI_LE_SETUP_ISO_DATA_PATH_CMD_OPCODE
Definition: ble_id.h:328
TASK_ID_LLD
@ TASK_ID_LLD
Definition: ble_id.h:532
TASK_ID_GAPM
@ TASK_ID_GAPM
Definition: ble_id.h:543
HCI_DBG_WR_LOC_SUPP_FEATS_CMD_OPCODE
@ HCI_DBG_WR_LOC_SUPP_FEATS_CMD_OPCODE
Definition: ble_id.h:388
GATTC_DISC_CMD
@ GATTC_DISC_CMD
Definition: ble_id.h:724
GAPC_SIGN_COUNTER_IND
@ GAPC_SIGN_COUNTER_IND
Definition: ble_id.h:603
HCI_LE_ADD_DEV_TO_WLST_CMD_OPCODE
@ HCI_LE_ADD_DEV_TO_WLST_CMD_OPCODE
Definition: ble_id.h:235
HCI_LE_GEN_DHKEY_V1_CMD_OPCODE
@ HCI_LE_GEN_DHKEY_V1_CMD_OPCODE
Definition: ble_id.h:256
HCI_IO_CAP_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_IO_CAP_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:65
GAPM_ACTIVITY_DELETE_CMD
@ GAPM_ACTIVITY_DELETE_CMD
Definition: ble_id.h:690
HCI_LE_CON_CTE_RSP_EN_CMD_OPCODE
@ HCI_LE_CON_CTE_RSP_EN_CMD_OPCODE
Definition: ble_id.h:305
HCI_IO_CAP_RSP_EVT_CODE
@ HCI_IO_CAP_RSP_EVT_CODE
Definition: ble_id.h:454
GAPC_PEER_VERSION_IND
@ GAPC_PEER_VERSION_IND
Definition: ble_id.h:582
HCI_WR_SP_MODE_CMD_OPCODE
@ HCI_WR_SP_MODE_CMD_OPCODE
Definition: ble_id.h:151
TASK_ID_GAPC
@ TASK_ID_GAPC
Definition: ble_id.h:544
HCI_LE_CREATE_CIS_CMD_OPCODE
@ HCI_LE_CREATE_CIS_CMD_OPCODE
Definition: ble_id.h:318
HCI_WR_SEC_CON_HOST_SUPP_CMD_OPCODE
@ HCI_WR_SEC_CON_HOST_SUPP_CMD_OPCODE
Definition: ble_id.h:177
GAPC_LE_PHY_IND
@ GAPC_LE_PHY_IND
Definition: ble_id.h:614
HCI_SNIFF_MODE_CMD_OPCODE
@ HCI_SNIFF_MODE_CMD_OPCODE
Definition: ble_id.h:78
HCI_LINK_SUPV_TO_CHG_EVT_CODE
@ HCI_LINK_SUPV_TO_CHG_EVT_CODE
Definition: ble_id.h:459
HCI_USER_CFM_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_USER_CFM_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:60
HCI_WR_INQ_MODE_CMD_OPCODE
@ HCI_WR_INQ_MODE_CMD_OPCODE
Definition: ble_id.h:142
HCI_INQ_CANCEL_CMD_OPCODE
@ HCI_INQ_CANCEL_CMD_OPCODE
Definition: ble_id.h:31
GAPC_PARAM_UPDATED_IND
@ GAPC_PARAM_UPDATED_IND
Definition: ble_id.h:592
GAPM_DEV_TX_PWR_IND
@ GAPM_DEV_TX_PWR_IND
Definition: ble_id.h:699
HCI_HOLD_MODE_CMD_OPCODE
@ HCI_HOLD_MODE_CMD_OPCODE
Definition: ble_id.h:77
HCI_FLOW_SPEC_CMD_OPCODE
@ HCI_FLOW_SPEC_CMD_OPCODE
Definition: ble_id.h:89
HCI_RD_AUTH_PAYL_TO_CMD_OPCODE
@ HCI_RD_AUTH_PAYL_TO_CMD_OPCODE
Definition: ble_id.h:178
GAPC_SECURITY_CMD
@ GAPC_SECURITY_CMD
Definition: ble_id.h:601
GATTC_SDP_SVC_DISC_CMD
@ GATTC_SDP_SVC_DISC_CMD
Definition: ble_id.h:746
TASK_ID_LB
@ TASK_ID_LB
Definition: ble_id.h:537
HCI_SNIFF_SUB_CMD_OPCODE
@ HCI_SNIFF_SUB_CMD_OPCODE
Definition: ble_id.h:90
HCI_INQ_RES_WITH_RSSI_EVT_CODE
@ HCI_INQ_RES_WITH_RSSI_EVT_CODE
Definition: ble_id.h:446
GATTC_SEND_SVC_CHANGED_CMD
@ GATTC_SEND_SVC_CHANGED_CMD
Definition: ble_id.h:738
HCI_LE_REQ_PEER_SCA_CMP_EVT_SUBCODE
@ HCI_LE_REQ_PEER_SCA_CMP_EVT_SUBCODE
Definition: ble_id.h:515
GAPM_LIST_SIZE_IND
@ GAPM_LIST_SIZE_IND
Definition: ble_id.h:686
HCI_LE_WR_SUGGTED_DFT_DATA_LEN_CMD_OPCODE
@ HCI_LE_WR_SUGGTED_DFT_DATA_LEN_CMD_OPCODE
Definition: ble_id.h:254
GAPM_ADDR_RENEW_CMD
@ GAPM_ADDR_RENEW_CMD
Definition: ble_id.h:711
HCI_RD_EXT_INQ_LEN_CMD_OPCODE
@ HCI_RD_EXT_INQ_LEN_CMD_OPCODE
Definition: ble_id.h:183
HCI_WR_AFH_CH_ASSESS_MODE_CMD_OPCODE
@ HCI_WR_AFH_CH_ASSESS_MODE_CMD_OPCODE
Definition: ble_id.h:146
HCI_RD_PAGE_SCAN_TYPE_CMD_OPCODE
@ HCI_RD_PAGE_SCAN_TYPE_CMD_OPCODE
Definition: ble_id.h:143
L2CC_PDU_RECV_IND
@ L2CC_PDU_RECV_IND
Definition: ble_id.h:778
HCI_PER_INQ_MODE_CMD_OPCODE
@ HCI_PER_INQ_MODE_CMD_OPCODE
Definition: ble_id.h:32
GAPC_CTE_RX_CFG_CMD
@ GAPC_CTE_RX_CFG_CMD
Definition: ble_id.h:621
HCI_LE_SET_PER_ADV_PARAM_CMD_OPCODE
@ HCI_LE_SET_PER_ADV_PARAM_CMD_OPCODE
Definition: ble_id.h:280
HCI_LE_ADD_DEV_TO_RSLV_LIST_CMD_OPCODE
@ HCI_LE_ADD_DEV_TO_RSLV_LIST_CMD_OPCODE
Definition: ble_id.h:257
HCI_CREATE_CON_CMD_OPCODE
@ HCI_CREATE_CON_CMD_OPCODE
Definition: ble_id.h:34
GAPM_UNKNOWN_TASK_IND
@ GAPM_UNKNOWN_TASK_IND
Definition: ble_id.h:669
GAPM_PER_ADV_IQ_REPORT_IND
@ GAPM_PER_ADV_IQ_REPORT_IND
Definition: ble_id.h:704
HCI_LE_ADD_DEV_TO_PER_ADV_LIST_CMD_OPCODE
@ HCI_LE_ADD_DEV_TO_PER_ADV_LIST_CMD_OPCODE
Definition: ble_id.h:289
HCI_LE_RD_LOC_P256_PUB_KEY_CMP_EVT_SUBCODE
@ HCI_LE_RD_LOC_P256_PUB_KEY_CMP_EVT_SUBCODE
Definition: ble_id.h:492
hci_msg_id
hci_msg_id
Definition: ble_id.h:557
HCI_ACCEPT_CON_REQ_CMD_OPCODE
@ HCI_ACCEPT_CON_REQ_CMD_OPCODE
Definition: ble_id.h:37
HCI_CREATE_NEW_UNIT_KEY_CMD_OPCODE
@ HCI_CREATE_NEW_UNIT_KEY_CMD_OPCODE
Definition: ble_id.h:99
HCI_DBG_TEST_SCH_PLAN_REM_CMD_OPCODE
@ HCI_DBG_TEST_SCH_PLAN_REM_CMD_OPCODE
Definition: ble_id.h:398
HCI_LE_SET_EVT_MASK_CMD_OPCODE
@ HCI_LE_SET_EVT_MASK_CMD_OPCODE
LE Commands Opcodes.
Definition: ble_id.h:220
HCI_LE_SET_SCAN_EN_CMD_OPCODE
@ HCI_LE_SET_SCAN_EN_CMD_OPCODE
Definition: ble_id.h:230
HCI_WR_CON_ACCEPT_TO_CMD_OPCODE
@ HCI_WR_CON_ACCEPT_TO_CMD_OPCODE
Definition: ble_id.h:106
GAPC_SIGN_IND
@ GAPC_SIGN_IND
Definition: ble_id.h:639
HCI_WR_EXT_INQ_RSP_CMD_OPCODE
@ HCI_WR_EXT_INQ_RSP_CMD_OPCODE
Definition: ble_id.h:148
HCI_LE_RD_MAX_DATA_LEN_CMD_OPCODE
@ HCI_LE_RD_MAX_DATA_LEN_CMD_OPCODE
Definition: ble_id.h:265
HCI_PIN_CODE_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_PIN_CODE_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:42
HCI_ENC_CHG_EVT_CODE
@ HCI_ENC_CHG_EVT_CODE
Definition: ble_id.h:422
HCI_CON_SLV_BCST_CH_MAP_CHG_EVT_CODE
@ HCI_CON_SLV_BCST_CH_MAP_CHG_EVT_CODE
Definition: ble_id.h:472
HCI_GET_MWS_TRANSPORT_LAYER_CONFIG_CMD_OPCODE
@ HCI_GET_MWS_TRANSPORT_LAYER_CONFIG_CMD_OPCODE
Definition: ble_id.h:210
HCI_DBG_WR_PAR_CMD_OPCODE
@ HCI_DBG_WR_PAR_CMD_OPCODE
Definition: ble_id.h:358
HCI_RD_BUF_SIZE_CMD_OPCODE
@ HCI_RD_BUF_SIZE_CMD_OPCODE
Definition: ble_id.h:193
HCI_LE_SET_ADV_DATA_CMD_OPCODE
@ HCI_LE_SET_ADV_DATA_CMD_OPCODE
Definition: ble_id.h:226
GAPM_ACTIVITY_CREATED_IND
@ GAPM_ACTIVITY_CREATED_IND
Definition: ble_id.h:691
HCI_VS_AUSY_CON_EVT_CNT_GET_CMD_OPCODE
@ HCI_VS_AUSY_CON_EVT_CNT_GET_CMD_OPCODE
Definition: ble_id.h:402
HCI_DBG_ER_FLASH_CMD_OPCODE
@ HCI_DBG_ER_FLASH_CMD_OPCODE
Definition: ble_id.h:354
HCI_LE_RANGING_CMP_EVT_SUBCODE
@ HCI_LE_RANGING_CMP_EVT_SUBCODE
Definition: ble_id.h:522
HCI_LE_SET_PHY_CMD_OPCODE
@ HCI_LE_SET_PHY_CMD_OPCODE
Definition: ble_id.h:268
GAPC_SET_LE_PING_TO_CMD
@ GAPC_SET_LE_PING_TO_CMD
Definition: ble_id.h:606
HCI_SET_MWS_TRANSPORT_LAYER_CMD_OPCODE
@ HCI_SET_MWS_TRANSPORT_LAYER_CMD_OPCODE
Definition: ble_id.h:168
HCI_SETUP_SYNC_CON_CMD_OPCODE
@ HCI_SETUP_SYNC_CON_CMD_OPCODE
Definition: ble_id.h:55
GATTC_WRITE_REQ_IND
@ GATTC_WRITE_REQ_IND
Definition: ble_id.h:742
HCI_LE_BIG_SYNC_LOST_EVT_SUBCODE
@ HCI_LE_BIG_SYNC_LOST_EVT_SUBCODE
Definition: ble_id.h:514
HCI_LE_ISO_READ_TEST_COUNTERS_CMD_OPCODE
@ HCI_LE_ISO_READ_TEST_COUNTERS_CMD_OPCODE
Definition: ble_id.h:332
HCI_LE_SET_ADV_SET_RAND_ADDR_CMD_OPCODE
@ HCI_LE_SET_ADV_SET_RAND_ADDR_CMD_OPCODE
Definition: ble_id.h:271
gapm_msg_id
gapm_msg_id
Definition: ble_id.h:649
HCI_USER_CFM_REQ_REPLY_CMD_OPCODE
@ HCI_USER_CFM_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:59
HCI_DBG_MWS_COEX_CMD_OPCODE
@ HCI_DBG_MWS_COEX_CMD_OPCODE
Definition: ble_id.h:386
GAPM_LEPSM_UNREGISTER_CMD
@ GAPM_LEPSM_UNREGISTER_CMD
Definition: ble_id.h:675
HCI_SET_MWS_PATTERN_CONFIG_CMD_OPCODE
@ HCI_SET_MWS_PATTERN_CONFIG_CMD_OPCODE
Definition: ble_id.h:170
HCI_TRUNC_PAGE_CAN_CMD_OPCODE
@ HCI_TRUNC_PAGE_CAN_CMD_OPCODE
Definition: ble_id.h:69
HCI_ACL_DATA
@ HCI_ACL_DATA
Definition: ble_id.h:565
HCI_LE_RMV_ADV_SET_CMD_OPCODE
@ HCI_LE_RMV_ADV_SET_CMD_OPCODE
Definition: ble_id.h:278
GATTC_DISC_CHAR_DESC_IND
@ GATTC_DISC_CHAR_DESC_IND
Definition: ble_id.h:728
HCI_RD_REM_EXT_FEATS_CMP_EVT_CODE
@ HCI_RD_REM_EXT_FEATS_CMP_EVT_CODE
Definition: ble_id.h:447
HCI_LE_ENH_RD_TX_PWR_LVL_CMD_OPCODE
@ HCI_LE_ENH_RD_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:336
HCI_WR_LOCAL_NAME_CMD_OPCODE
@ HCI_WR_LOCAL_NAME_CMD_OPCODE
Definition: ble_id.h:103
HCI_LE_START_RANGING_CMD_OPCODE
@ HCI_LE_START_RANGING_CMD_OPCODE
Definition: ble_id.h:344
HCI_MODE_CHG_EVT_CODE
@ HCI_MODE_CHG_EVT_CODE
Definition: ble_id.h:434
HCI_RD_LOCAL_SUPP_FEATS_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_FEATS_CMD_OPCODE
Definition: ble_id.h:191
HCI_LE_SET_SCAN_PARAM_CMD_OPCODE
@ HCI_LE_SET_SCAN_PARAM_CMD_OPCODE
Definition: ble_id.h:229
HCI_SET_CON_SLV_BCST_DATA_CMD_OPCODE
@ HCI_SET_CON_SLV_BCST_DATA_CMD_OPCODE
Definition: ble_id.h:173
HCI_LE_MOD_SLEEP_CLK_ACC_CMD_OPCODE
@ HCI_LE_MOD_SLEEP_CLK_ACC_CMD_OPCODE
Definition: ble_id.h:313
HCI_START_SYNC_TRAIN_CMD_OPCODE
@ HCI_START_SYNC_TRAIN_CMD_OPCODE
Definition: ble_id.h:72
HCI_LE_SET_PRIV_MODE_CMD_OPCODE
@ HCI_LE_SET_PRIV_MODE_CMD_OPCODE
Definition: ble_id.h:296
HCI_LE_PER_ADV_SYNC_TRANSF_REC_EVT_SUBCODE
@ HCI_LE_PER_ADV_SYNC_TRANSF_REC_EVT_SUBCODE
Definition: ble_id.h:508
HCI_REM_HOST_SUPP_FEATS_NOTIF_EVT_CODE
@ HCI_REM_HOST_SUPP_FEATS_NOTIF_EVT_CODE
Definition: ble_id.h:463
HCI_LE_TX_TEST_V2_CMD_OPCODE
@ HCI_LE_TX_TEST_V2_CMD_OPCODE
Definition: ble_id.h:270
HCI_RD_CURR_IAC_LAP_CMD_OPCODE
@ HCI_RD_CURR_IAC_LAP_CMD_OPCODE
Definition: ble_id.h:136
HCI_SET_CON_SLV_BCST_REC_CMD_OPCODE
@ HCI_SET_CON_SLV_BCST_REC_CMD_OPCODE
Definition: ble_id.h:71
GAPC_SECURITY_IND
@ GAPC_SECURITY_IND
Definition: ble_id.h:602
GAPC_SET_PREF_SLAVE_LATENCY_CMD
@ GAPC_SET_PREF_SLAVE_LATENCY_CMD
Definition: ble_id.h:616
GATTC_EVENT_REQ_IND
@ GATTC_EVENT_REQ_IND
Definition: ble_id.h:734
HCI_LE_DIR_ADV_REP_EVT_SUBCODE
@ HCI_LE_DIR_ADV_REP_EVT_SUBCODE
Definition: ble_id.h:495
HCI_COMMAND
@ HCI_COMMAND
Definition: ble_id.h:564
HCI_WR_SCAN_EN_CMD_OPCODE
@ HCI_WR_SCAN_EN_CMD_OPCODE
Definition: ble_id.h:110
HCI_LK_NOTIF_EVT_CODE
@ HCI_LK_NOTIF_EVT_CODE
Definition: ble_id.h:438
HCI_LE_WR_RF_PATH_COMP_CMD_OPCODE
@ HCI_LE_WR_RF_PATH_COMP_CMD_OPCODE
Definition: ble_id.h:295
GAPM_PROFILE_TASK_ADD_CMD
@ GAPM_PROFILE_TASK_ADD_CMD
Definition: ble_id.h:667
HCI_VS_AUSY_EVT_TX_TIME_GET_CMD_OPCODE
@ HCI_VS_AUSY_EVT_TX_TIME_GET_CMD_OPCODE
Definition: ble_id.h:403
HCI_LE_CON_CTE_REQ_EN_CMD_OPCODE
@ HCI_LE_CON_CTE_REQ_EN_CMD_OPCODE
Definition: ble_id.h:304
HCI_DBG_BLE_REG_WR_CMD_OPCODE
@ HCI_DBG_BLE_REG_WR_CMD_OPCODE
Definition: ble_id.h:371
HCI_LE_REQ_PEER_SCA_CMD_OPCODE
@ HCI_LE_REQ_PEER_SCA_CMD_OPCODE
Definition: ble_id.h:327
HCI_LE_SET_HOST_CH_CLASS_CMD_OPCODE
@ HCI_LE_SET_HOST_CH_CLASS_CMD_OPCODE
Definition: ble_id.h:238
HCI_LE_RD_PHY_CMD_OPCODE
@ HCI_LE_RD_PHY_CMD_OPCODE
Definition: ble_id.h:266
GAPC_SMP_TIMEOUT_TIMER_IND
@ GAPC_SMP_TIMEOUT_TIMER_IND
Definition: ble_id.h:641
HCI_EVENT
@ HCI_EVENT
Definition: ble_id.h:562
GAPM_ACTIVITY_STOP_CMD
@ GAPM_ACTIVITY_STOP_CMD
Definition: ble_id.h:689
HCI_DBG_RF_SWITCH_CLK_CMD_OPCODE
@ HCI_DBG_RF_SWITCH_CLK_CMD_OPCODE
Definition: ble_id.h:376
HCI_RD_NB_BDCST_RETX_CMD_OPCODE
@ HCI_RD_NB_BDCST_RETX_CMD_OPCODE
Definition: ble_id.h:123
HCI_CMD_CMP_EVENT
@ HCI_CMD_CMP_EVENT
Definition: ble_id.h:560
GAPM_LE_TEST_IQ_REPORT_IND
@ GAPM_LE_TEST_IQ_REPORT_IND
Definition: ble_id.h:678
HCI_EN_DUT_MODE_CMD_OPCODE
@ HCI_EN_DUT_MODE_CMD_OPCODE
Definition: ble_id.h:215
HCI_SYNC_TRAIN_CMP_EVT_CODE
@ HCI_SYNC_TRAIN_CMP_EVT_CODE
Definition: ble_id.h:466
HCI_RD_LOCAL_SUPP_CODEC_CAP_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_CODEC_CAP_CMD_OPCODE
Definition: ble_id.h:199
HCI_WR_SYNC_FLOW_CTRL_EN_CMD_OPCODE
@ HCI_WR_SYNC_FLOW_CTRL_EN_CMD_OPCODE
Definition: ble_id.h:129
GAPM_GEN_RAND_NB_CMD
@ GAPM_GEN_RAND_NB_CMD
Definition: ble_id.h:665
HCI_DBG_MWS_COEXTST_SCEN_CMD_OPCODE
@ HCI_DBG_MWS_COEXTST_SCEN_CMD_OPCODE
Definition: ble_id.h:387
HCI_CON_REQ_EVT_CODE
@ HCI_CON_REQ_EVT_CODE
Definition: ble_id.h:418
HCI_LE_TX_POWER_REPORTING_EVT_SUBCODE
@ HCI_LE_TX_POWER_REPORTING_EVT_SUBCODE
Definition: ble_id.h:517
HCI_LE_TERMINATE_BIG_CMP_EVT_SUBCODE
@ HCI_LE_TERMINATE_BIG_CMP_EVT_SUBCODE
Definition: ble_id.h:512
HCI_RST_FAIL_CONTACT_CNT_CMD_OPCODE
@ HCI_RST_FAIL_CONTACT_CNT_CMD_OPCODE
Definition: ble_id.h:204
HCI_WR_AUTO_FLUSH_TO_CMD_OPCODE
@ HCI_WR_AUTO_FLUSH_TO_CMD_OPCODE
Definition: ble_id.h:122
HCI_LE_RD_PER_ADV_LIST_SIZE_CMD_OPCODE
@ HCI_LE_RD_PER_ADV_LIST_SIZE_CMD_OPCODE
Definition: ble_id.h:292
GAPC_UNKNOWN_MSG_IND
@ GAPC_UNKNOWN_MSG_IND
Definition: ble_id.h:618
HCI_LE_CH_SEL_ALGO_EVT_SUBCODE
@ HCI_LE_CH_SEL_ALGO_EVT_SUBCODE
Definition: ble_id.h:504
HCI_LE_RANGING_SAMPLE_REPORT_EVT_SUBCODE
@ HCI_LE_RANGING_SAMPLE_REPORT_EVT_SUBCODE
Definition: ble_id.h:521
HCI_DBG_TEST_CRYPTO_FUNC_CMD_OPCODE
@ HCI_DBG_TEST_CRYPTO_FUNC_CMD_OPCODE
Definition: ble_id.h:396
GAPC_CHAN_SEL_ALGO_IND
@ GAPC_CHAN_SEL_ALGO_IND
Definition: ble_id.h:615
TASK_ID_L2CC
@ TASK_ID_L2CC
Definition: ble_id.h:540
HCI_LE_ENC_CMD_OPCODE
@ HCI_LE_ENC_CMD_OPCODE
Definition: ble_id.h:241
GATTC_CLIENT_RTX_IND
@ GATTC_CLIENT_RTX_IND
Definition: ble_id.h:750
GATTC_CMP_EVT
@ GATTC_CMP_EVT
Definition: ble_id.h:721
HCI_LE_PER_ADV_SYNC_EST_EVT_SUBCODE
@ HCI_LE_PER_ADV_SYNC_EST_EVT_SUBCODE
Definition: ble_id.h:498
HCI_DISC_CMP_EVT_CODE
@ HCI_DISC_CMP_EVT_CODE
Definition: ble_id.h:419
L2CC_CMP_EVT
@ L2CC_CMP_EVT
Definition: ble_id.h:763
HCI_LE_SET_CONLESS_IQ_SAMPL_EN_CMD_OPCODE
@ HCI_LE_SET_CONLESS_IQ_SAMPL_EN_CMD_OPCODE
Definition: ble_id.h:301
HCI_WR_PIN_TYPE_CMD_OPCODE
@ HCI_WR_PIN_TYPE_CMD_OPCODE
Definition: ble_id.h:98
HCI_RD_CLASS_OF_DEV_CMD_OPCODE
@ HCI_RD_CLASS_OF_DEV_CMD_OPCODE
Definition: ble_id.h:117
HCI_CMD_STAT_EVENT
@ HCI_CMD_STAT_EVENT
Definition: ble_id.h:561
GAPM_SCAN_REQUEST_IND
@ GAPM_SCAN_REQUEST_IND
Definition: ble_id.h:695
HCI_LE_CIS_ESTABLISHED_EVT_SUBCODE
@ HCI_LE_CIS_ESTABLISHED_EVT_SUBCODE
Definition: ble_id.h:509
HCI_ENH_SETUP_SYNC_CON_CMD_OPCODE
@ HCI_ENH_SETUP_SYNC_CON_CMD_OPCODE
Definition: ble_id.h:66
HCI_ROLE_CHG_EVT_CODE
@ HCI_ROLE_CHG_EVT_CODE
Definition: ble_id.h:432
GAPC_LE_PKT_SIZE_IND
@ GAPC_LE_PKT_SIZE_IND
Definition: ble_id.h:610
GAPM_CMP_EVT
@ GAPM_CMP_EVT
Definition: ble_id.h:650
HCI_LE_SET_HOST_FEATURE_CMD_OPCODE
@ HCI_LE_SET_HOST_FEATURE_CMD_OPCODE
Definition: ble_id.h:334
GAPM_SYNC_ESTABLISHED_IND
@ GAPM_SYNC_ESTABLISHED_IND
Definition: ble_id.h:696
HCI_QOS_VIOL_EVT_CODE
@ HCI_QOS_VIOL_EVT_CODE
Definition: ble_id.h:443
HCI_RD_PAGE_TO_CMD_OPCODE
@ HCI_RD_PAGE_TO_CMD_OPCODE
Definition: ble_id.h:107
HCI_LE_SET_TX_POWER_REP_EN_CMD_OPCODE
@ HCI_LE_SET_TX_POWER_REP_EN_CMD_OPCODE
Definition: ble_id.h:340
HCI_LE_SET_EXT_ADV_DATA_CMD_OPCODE
@ HCI_LE_SET_EXT_ADV_DATA_CMD_OPCODE
Definition: ble_id.h:273
HCI_LE_REM_CON_PARAM_REQ_REPLY_CMD_OPCODE
@ HCI_LE_REM_CON_PARAM_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:250
HCI_CON_CMP_EVT_CODE
@ HCI_CON_CMP_EVT_CODE
Definition: ble_id.h:417
HCI_LE_ISO_RX_TEST_CMD_OPCODE
@ HCI_LE_ISO_RX_TEST_CMD_OPCODE
Definition: ble_id.h:331
HCI_PIN_CODE_REQ_EVT_CODE
@ HCI_PIN_CODE_REQ_EVT_CODE
Definition: ble_id.h:436
HCI_HOST_BUF_SIZE_CMD_OPCODE
@ HCI_HOST_BUF_SIZE_CMD_OPCODE
Definition: ble_id.h:131
HCI_SWITCH_ROLE_CMD_OPCODE
@ HCI_SWITCH_ROLE_CMD_OPCODE
Definition: ble_id.h:84
HCI_LE_RX_TEST_V3_CMD_OPCODE
@ HCI_LE_RX_TEST_V3_CMD_OPCODE
Definition: ble_id.h:297
HCI_LE_RD_BUF_SIZE_V2_CMD_OPCODE
@ HCI_LE_RD_BUF_SIZE_V2_CMD_OPCODE
Definition: ble_id.h:314
HCI_LE_SET_PER_ADV_DATA_CMD_OPCODE
@ HCI_LE_SET_PER_ADV_DATA_CMD_OPCODE
Definition: ble_id.h:281
HCI_REM_OOB_EXT_DATA_REQ_REPLY_CMD_OPCODE
@ HCI_REM_OOB_EXT_DATA_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:74
HCI_LE_SET_EXT_SCAN_EN_CMD_OPCODE
@ HCI_LE_SET_EXT_SCAN_EN_CMD_OPCODE
Definition: ble_id.h:284
HCI_LK_REQ_EVT_CODE
@ HCI_LK_REQ_EVT_CODE
Definition: ble_id.h:437
HCI_RD_REM_SUPP_FEATS_CMP_EVT_CODE
@ HCI_RD_REM_SUPP_FEATS_CMP_EVT_CODE
Definition: ble_id.h:425
HCI_DBG_WR_MEM_CMD_OPCODE
@ HCI_DBG_WR_MEM_CMD_OPCODE
Definition: ble_id.h:351
GAPM_PUBLIC_ADDR_SET_CMD
@ GAPM_PUBLIC_ADDR_SET_CMD
Definition: ble_id.h:712
HCI_LE_RANGING_IND_EVT_SUBCODE
@ HCI_LE_RANGING_IND_EVT_SUBCODE
Definition: ble_id.h:520
HCI_RD_DFT_LINK_POL_STG_CMD_OPCODE
@ HCI_RD_DFT_LINK_POL_STG_CMD_OPCODE
Definition: ble_id.h:87
HCI_LE_BIG_SYNC_ESTABLISHED_EVT_SUBCODE
@ HCI_LE_BIG_SYNC_ESTABLISHED_EVT_SUBCODE
Definition: ble_id.h:513
GAPC_CTE_TX_CFG_CMD
@ GAPC_CTE_TX_CFG_CMD
Definition: ble_id.h:620
TASK_FIRST_MSG
#define TASK_FIRST_MSG(task)
Definition: ble_id.h:17
HCI_SEND_KEYPRESS_NOTIF_CMD_OPCODE
@ HCI_SEND_KEYPRESS_NOTIF_CMD_OPCODE
Definition: ble_id.h:158
HCI_LE_RD_PEER_RSLV_ADDR_CMD_OPCODE
@ HCI_LE_RD_PEER_RSLV_ADDR_CMD_OPCODE
Definition: ble_id.h:261
HCI_VS_AUSY_LAST_RX_TIME_GET_CMD_OPCODE
@ HCI_VS_AUSY_LAST_RX_TIME_GET_CMD_OPCODE
Definition: ble_id.h:404
GAPM_ACTIVITY_START_CMD
@ GAPM_ACTIVITY_START_CMD
Definition: ble_id.h:688
HCI_DBG_RD_FLASH_CMD_OPCODE
@ HCI_DBG_RD_FLASH_CMD_OPCODE
Definition: ble_id.h:356
TASK_ID_RTLS
@ TASK_ID_RTLS
Definition: ble_id.h:549
L2CC_PDU_SEND_CMD
@ L2CC_PDU_SEND_CMD
Definition: ble_id.h:777
GAPC_RANGING_SAMPLE_REPORT_IND
@ GAPC_RANGING_SAMPLE_REPORT_IND
Definition: ble_id.h:636
HCI_ENH_ACCEPT_SYNC_CON_CMD_OPCODE
@ HCI_ENH_ACCEPT_SYNC_CON_CMD_OPCODE
Definition: ble_id.h:67
HCI_LE_SET_CONLESS_CTE_TX_EN_CMD_OPCODE
@ HCI_LE_SET_CONLESS_CTE_TX_EN_CMD_OPCODE
Definition: ble_id.h:300
HCI_LE_REM_CON_PARAM_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_LE_REM_CON_PARAM_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:251
HCI_RD_AFH_CH_MAP_CMD_OPCODE
@ HCI_RD_AFH_CH_MAP_CMD_OPCODE
Definition: ble_id.h:207
HCI_LE_EVENT
@ HCI_LE_EVENT
Definition: ble_id.h:563
HCI_LE_META_EVT_CODE
@ HCI_LE_META_EVT_CODE
Definition: ble_id.h:464
HCI_RD_EXT_INQ_RSP_CMD_OPCODE
@ HCI_RD_EXT_INQ_RSP_CMD_OPCODE
Definition: ble_id.h:147
GAPM_AUTO_CONN_TO_IND
@ GAPM_AUTO_CONN_TO_IND
Definition: ble_id.h:710
HCI_WR_STORED_LK_CMD_OPCODE
@ HCI_WR_STORED_LK_CMD_OPCODE
Definition: ble_id.h:101
GAPM_GEN_RAND_ADDR_CMD
@ GAPM_GEN_RAND_ADDR_CMD
Definition: ble_id.h:662
HCI_LE_SET_EXT_ADV_EN_CMD_OPCODE
@ HCI_LE_SET_EXT_ADV_EN_CMD_OPCODE
Definition: ble_id.h:275
GAPC_PEER_FEATURES_IND
@ GAPC_PEER_FEATURES_IND
Definition: ble_id.h:583
HCI_DBG_DEL_PAR_CMD_OPCODE
@ HCI_DBG_DEL_PAR_CMD_OPCODE
Definition: ble_id.h:352
HCI_REM_OOB_DATA_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_REM_OOB_DATA_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:64
HCI_LE_EN_ENC_CMD_OPCODE
@ HCI_LE_EN_ENC_CMD_OPCODE
Definition: ble_id.h:243
HCI_LE_RD_REM_FEATS_CMD_OPCODE
@ HCI_LE_RD_REM_FEATS_CMD_OPCODE
Definition: ble_id.h:240
GAPC_GET_DEV_INFO_REQ_IND
@ GAPC_GET_DEV_INFO_REQ_IND
Definition: ble_id.h:585
HCI_RD_SEC_CON_HOST_SUPP_CMD_OPCODE
@ HCI_RD_SEC_CON_HOST_SUPP_CMD_OPCODE
Definition: ble_id.h:176
GAPC_PARAM_UPDATE_CMD
@ GAPC_PARAM_UPDATE_CMD
Definition: ble_id.h:589
HCI_RD_HOLD_MODE_ACTIVITY_CMD_OPCODE
@ HCI_RD_HOLD_MODE_ACTIVITY_CMD_OPCODE
Definition: ble_id.h:125
HCI_CHG_CON_LK_CMD_OPCODE
@ HCI_CHG_CON_LK_CMD_OPCODE
Definition: ble_id.h:46
HCI_DATA_BUF_OVFLW_EVT_CODE
@ HCI_DATA_BUF_OVFLW_EVT_CODE
Definition: ble_id.h:439
HCI_SET_EVT_FILTER_CMD_OPCODE
@ HCI_SET_EVT_FILTER_CMD_OPCODE
Definition: ble_id.h:95
GAPM_DBG_IQGEN_CFG_CMD
@ GAPM_DBG_IQGEN_CFG_CMD
Definition: ble_id.h:707
GAPC_DISCONNECT_IND
@ GAPC_DISCONNECT_IND
Definition: ble_id.h:578
HCI_DBG_RD_CON_INFO_CMD_OPCODE
@ HCI_DBG_RD_CON_INFO_CMD_OPCODE
Definition: ble_id.h:369
GATTC_DISC_SVC_IND
@ GATTC_DISC_SVC_IND
Definition: ble_id.h:725
L2CC_LECB_CONNECT_REQ_IND
@ L2CC_LECB_CONNECT_REQ_IND
Definition: ble_id.h:765
HCI_RD_SCAN_EN_CMD_OPCODE
@ HCI_RD_SCAN_EN_CMD_OPCODE
Definition: ble_id.h:109
HCI_LE_RAND_CMD_OPCODE
@ HCI_LE_RAND_CMD_OPCODE
Definition: ble_id.h:242
GATTC_ATT_INFO_REQ_IND
@ GATTC_ATT_INFO_REQ_IND
Definition: ble_id.h:744
HCI_LE_CLEAR_RSLV_LIST_CMD_OPCODE
@ HCI_LE_CLEAR_RSLV_LIST_CMD_OPCODE
Definition: ble_id.h:259
GAPC_PER_ADV_SYNC_TRANS_CMD
@ GAPC_PER_ADV_SYNC_TRANS_CMD
Definition: ble_id.h:619
GAPM_LEPSM_REGISTER_CMD
@ GAPM_LEPSM_REGISTER_CMD
Definition: ble_id.h:674
GATTC_EVENT_IND
@ GATTC_EVENT_IND
Definition: ble_id.h:733
L2CC_LECB_CONNECT_IND
@ L2CC_LECB_CONNECT_IND
Definition: ble_id.h:767
GAPM_UNKNOWN_MSG_IND
@ GAPM_UNKNOWN_MSG_IND
Definition: ble_id.h:701
HCI_DBG_SEND_LLCP_CMD_OPCODE
@ HCI_DBG_SEND_LLCP_CMD_OPCODE
Definition: ble_id.h:372
GATTC_READ_REQ_IND
@ GATTC_READ_REQ_IND
Definition: ble_id.h:740
GAPM_LE_TEST_END_IND
@ GAPM_LE_TEST_END_IND
Definition: ble_id.h:677
TASK_ID_LM
@ TASK_ID_LM
Definition: ble_id.h:535
GAPM_GET_PUB_KEY_CMD
@ GAPM_GET_PUB_KEY_CMD
Definition: ble_id.h:682
HCI_VS_SET_MAX_RX_SIZE_AND_TIME_CMD_OPCODE
@ HCI_VS_SET_MAX_RX_SIZE_AND_TIME_CMD_OPCODE
Definition: ble_id.h:368
L2CC_UNKNOWN_MSG_IND
@ L2CC_UNKNOWN_MSG_IND
Definition: ble_id.h:774
HCI_DBG_RD_PAR_CMD_OPCODE
@ HCI_DBG_RD_PAR_CMD_OPCODE
Definition: ble_id.h:357
HCI_RD_LOCAL_VER_INFO_CMD_OPCODE
@ HCI_RD_LOCAL_VER_INFO_CMD_OPCODE
Definition: ble_id.h:189
HCI_LE_LTK_REQ_REPLY_CMD_OPCODE
@ HCI_LE_LTK_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:244
MSG_ID
#define MSG_ID(task, idx)
Definition: ble_id.h:18
HCI_LE_CREATE_CON_CMD_OPCODE
@ HCI_LE_CREATE_CON_CMD_OPCODE
Definition: ble_id.h:231
HCI_SET_MWS_SIGNALING_CMD_OPCODE
@ HCI_SET_MWS_SIGNALING_CMD_OPCODE
Definition: ble_id.h:167
HCI_RD_REM_VER_INFO_CMD_OPCODE
@ HCI_RD_REM_VER_INFO_CMD_OPCODE
Definition: ble_id.h:52
GAPC_LE_PING_TO_IND
@ GAPC_LE_PING_TO_IND
Definition: ble_id.h:608
HCI_WR_DFT_ERR_DATA_REP_CMD_OPCODE
@ HCI_WR_DFT_ERR_DATA_REP_CMD_OPCODE
Definition: ble_id.h:156
HCI_HW_ERR_EVT_CODE
@ HCI_HW_ERR_EVT_CODE
Definition: ble_id.h:430
HCI_FLOW_SPEC_CMP_EVT_CODE
@ HCI_FLOW_SPEC_CMP_EVT_CODE
Definition: ble_id.h:445
GAPM_PER_ADV_REPORT_CTRL_CMD
@ GAPM_PER_ADV_REPORT_CTRL_CMD
Definition: ble_id.h:702
HCI_RD_AUTH_EN_CMD_OPCODE
@ HCI_RD_AUTH_EN_CMD_OPCODE
Definition: ble_id.h:115
HCI_EXIT_PER_INQ_MODE_CMD_OPCODE
@ HCI_EXIT_PER_INQ_MODE_CMD_OPCODE
Definition: ble_id.h:33
L2CC_DBG_PDU_SEND_CMD
@ L2CC_DBG_PDU_SEND_CMD
Definition: ble_id.h:775
HCI_LE_GEN_DHKEY_V2_CMD_OPCODE
@ HCI_LE_GEN_DHKEY_V2_CMD_OPCODE
Definition: ble_id.h:312
GAPC_SET_PREF_SLAVE_EVT_DUR_CMD
@ GAPC_SET_PREF_SLAVE_EVT_DUR_CMD
Definition: ble_id.h:617
HCI_SET_RES_LT_ADDR_CMD_OPCODE
@ HCI_SET_RES_LT_ADDR_CMD_OPCODE
Definition: ble_id.h:171
HCI_AUTH_PAYL_TO_EXP_EVT_CODE
@ HCI_AUTH_PAYL_TO_EXP_EVT_CODE
Definition: ble_id.h:473
GATTC_EXECUTE_WRITE_CMD
@ GATTC_EXECUTE_WRITE_CMD
Definition: ble_id.h:732
HCI_CON_SLV_BCST_TO_EVT_CODE
@ HCI_CON_SLV_BCST_TO_EVT_CODE
Definition: ble_id.h:469
HCI_EXIT_PARK_STATE_CMD_OPCODE
@ HCI_EXIT_PARK_STATE_CMD_OPCODE
Definition: ble_id.h:81
GAPC_KEY_PRESS_NOTIFICATION_IND
@ GAPC_KEY_PRESS_NOTIFICATION_IND
Definition: ble_id.h:612
HCI_LE_CIS_REQUEST_EVT_SUBCODE
@ HCI_LE_CIS_REQUEST_EVT_SUBCODE
Definition: ble_id.h:510
GAPC_PARAM_UPDATE_REQ_IND
@ GAPC_PARAM_UPDATE_REQ_IND
Definition: ble_id.h:590
HCI_LE_RD_ANTENNA_INF_CMD_OPCODE
@ HCI_LE_RD_ANTENNA_INF_CMD_OPCODE
Definition: ble_id.h:306
GAPM_SET_CHANNEL_MAP_CMD
@ GAPM_SET_CHANNEL_MAP_CMD
Definition: ble_id.h:653
HCI_LE_BIG_TERMINATE_SYNC_CMD_OPCODE
@ HCI_LE_BIG_TERMINATE_SYNC_CMD_OPCODE
Definition: ble_id.h:326
HCI_LE_SET_PATH_LOSS_REP_PARAM_CMD_OPCODE
@ HCI_LE_SET_PATH_LOSS_REP_PARAM_CMD_OPCODE
Definition: ble_id.h:338
GATTC_ATT_INFO_CFM
@ GATTC_ATT_INFO_CFM
Definition: ble_id.h:745
TASK_ID_APP
@ TASK_ID_APP
Definition: ble_id.h:545
GAPC_CONNECTION_REQ_IND
@ GAPC_CONNECTION_REQ_IND
Definition: ble_id.h:576
GAPM_RESOLV_ADDR_CMD
@ GAPM_RESOLV_ADDR_CMD
Definition: ble_id.h:660
HCI_KEYPRESS_NOTIF_EVT_CODE
@ HCI_KEYPRESS_NOTIF_EVT_CODE
Definition: ble_id.h:462
GATTC_READ_CMD
@ GATTC_READ_CMD
Definition: ble_id.h:729
HCI_LE_CREATE_BIG_TEST_CMD_OPCODE
@ HCI_LE_CREATE_BIG_TEST_CMD_OPCODE
Definition: ble_id.h:323
l2cc_msg_id
l2cc_msg_id
Definition: ble_id.h:762
HCI_LE_CON_CMP_EVT_SUBCODE
@ HCI_LE_CON_CMP_EVT_SUBCODE
LE Events Subcodes.
Definition: ble_id.h:485
gattc_msg_id
gattc_msg_id
Definition: ble_id.h:720
GATTC_WRITE_CMD
@ GATTC_WRITE_CMD
Definition: ble_id.h:731
TASK_ID_AHI
@ TASK_ID_AHI
Definition: ble_id.h:546
HCI_LE_ADV_SET_TERMINATED_EVT_SUBCODE
@ HCI_LE_ADV_SET_TERMINATED_EVT_SUBCODE
Definition: ble_id.h:502
GAPM_DBG_MEM_INFO_IND
@ GAPM_DBG_MEM_INFO_IND
Definition: ble_id.h:658
HCI_INQ_CMP_EVT_CODE
@ HCI_INQ_CMP_EVT_CODE
Definition: ble_id.h:415
HCI_CON_PKT_TYPE_CHG_EVT_CODE
@ HCI_CON_PKT_TYPE_CHG_EVT_CODE
Definition: ble_id.h:442
HCI_SET_CON_SLV_BCST_CMD_OPCODE
@ HCI_SET_CON_SLV_BCST_CMD_OPCODE
Definition: ble_id.h:70
GAPM_USE_ENC_BLOCK_CMD
@ GAPM_USE_ENC_BLOCK_CMD
Definition: ble_id.h:663
HCI_RD_DATA_BLOCK_SIZE_CMD_OPCODE
@ HCI_RD_DATA_BLOCK_SIZE_CMD_OPCODE
Definition: ble_id.h:195
GAPC_BOND_IND
@ GAPC_BOND_IND
Definition: ble_id.h:596
HCI_DBG_RF_WR_DATA_TX_CMD_OPCODE
@ HCI_DBG_RF_WR_DATA_TX_CMD_OPCODE
Definition: ble_id.h:377
GATTC_SVC_CHANGED_CFG_IND
@ GATTC_SVC_CHANGED_CFG_IND
Definition: ble_id.h:739
GATTC_WRITE_CFM
@ GATTC_WRITE_CFM
Definition: ble_id.h:743
HCI_VS_SET_PREF_SLAVE_LATENCY_CMD_OPCODE
@ HCI_VS_SET_PREF_SLAVE_LATENCY_CMD_OPCODE
Definition: ble_id.h:366
TASK_ID_GATTM
@ TASK_ID_GATTM
Definition: ble_id.h:541
HCI_LE_RD_WLST_SIZE_CMD_OPCODE
@ HCI_LE_RD_WLST_SIZE_CMD_OPCODE
Definition: ble_id.h:233
GAPM_ISO_STAT_IND
@ GAPM_ISO_STAT_IND
Definition: ble_id.h:679
HCI_SP_CMP_EVT_CODE
@ HCI_SP_CMP_EVT_CODE
Definition: ble_id.h:458
GAPC_PATH_LOSS_THRESHOLD_REPORT_IND
@ GAPC_PATH_LOSS_THRESHOLD_REPORT_IND
Definition: ble_id.h:633
HCI_LE_RD_LOCAL_SUPP_FEATS_CMD_OPCODE
@ HCI_LE_RD_LOCAL_SUPP_FEATS_CMD_OPCODE
Definition: ble_id.h:222
GAPC_CON_CHANNEL_MAP_IND
@ GAPC_CON_CHANNEL_MAP_IND
Definition: ble_id.h:604
HCI_RD_SP_MODE_CMD_OPCODE
@ HCI_RD_SP_MODE_CMD_OPCODE
Definition: ble_id.h:150
HCI_LE_PER_ADV_CREATE_SYNC_CMD_OPCODE
@ HCI_LE_PER_ADV_CREATE_SYNC_CMD_OPCODE
Definition: ble_id.h:286
TASK_ID_SDK
@ TASK_ID_SDK
Definition: ble_id.h:539
HCI_WR_LINK_SUPV_TO_CMD_OPCODE
@ HCI_WR_LINK_SUPV_TO_CMD_OPCODE
Definition: ble_id.h:134
GAPC_SIGN_CMD
@ GAPC_SIGN_CMD
Definition: ble_id.h:638
HCI_LE_RMV_DEV_FROM_RSLV_LIST_CMD_OPCODE
@ HCI_LE_RMV_DEV_FROM_RSLV_LIST_CMD_OPCODE
Definition: ble_id.h:258
HCI_LE_BIG_INFO_ADV_REPORT_EVT_SUBCODE
@ HCI_LE_BIG_INFO_ADV_REPORT_EVT_SUBCODE
Definition: ble_id.h:518
GAPM_GEN_DH_KEY_CMD
@ GAPM_GEN_DH_KEY_CMD
Definition: ble_id.h:680
HCI_DBG_CIS_SET_PARAM_CMD_OPCODE
@ HCI_DBG_CIS_SET_PARAM_CMD_OPCODE
Definition: ble_id.h:393
HCI_WR_PAGE_TO_CMD_OPCODE
@ HCI_WR_PAGE_TO_CMD_OPCODE
Definition: ble_id.h:108
L2CC_LECB_SDU_RECV_IND
@ L2CC_LECB_SDU_RECV_IND
Definition: ble_id.h:773
HCI_LE_RD_ISO_TX_SYNC_CMD_OPCODE
@ HCI_LE_RD_ISO_TX_SYNC_CMD_OPCODE
Definition: ble_id.h:315
TASK_ID_LC
@ TASK_ID_LC
Definition: ble_id.h:536
HCI_RD_RSSI_CMD_OPCODE
@ HCI_RD_RSSI_CMD_OPCODE
Definition: ble_id.h:206
HCI_LE_CONLESS_IQ_REPORT_EVT_SUBCODE
@ HCI_LE_CONLESS_IQ_REPORT_EVT_SUBCODE
Definition: ble_id.h:505
HCI_CONFIG_DATA_PATH_CMD_OPCODE
@ HCI_CONFIG_DATA_PATH_CMD_OPCODE
Definition: ble_id.h:186
GAPM_ANTENNA_INF_IND
@ GAPM_ANTENNA_INF_IND
Definition: ble_id.h:659
GAPM_PER_SYNC_IQ_SAMPLING_CTRL_CMD
@ GAPM_PER_SYNC_IQ_SAMPLING_CTRL_CMD
Definition: ble_id.h:703
HCI_USER_CFM_REQ_EVT_CODE
@ HCI_USER_CFM_REQ_EVT_CODE
Definition: ble_id.h:455
GAPC_CTE_IQ_REPORT_IND
@ GAPC_CTE_IQ_REPORT_IND
Definition: ble_id.h:624
HCI_LE_SET_DFT_PHY_CMD_OPCODE
@ HCI_LE_SET_DFT_PHY_CMD_OPCODE
Definition: ble_id.h:267
HCI_RD_LINK_QUAL_CMD_OPCODE
@ HCI_RD_LINK_QUAL_CMD_OPCODE
Definition: ble_id.h:205
TASK_ID_LD
@ TASK_ID_LD
Definition: ble_id.h:538
L2CC_NB_DEPRECATED_MSG
#define L2CC_NB_DEPRECATED_MSG
Number of L2CC Deprecated messages.
Definition: ble_id.h:759
HCI_WR_AUTH_EN_CMD_OPCODE
@ HCI_WR_AUTH_EN_CMD_OPCODE
Definition: ble_id.h:116
L2CC_LECB_ADD_CMD
@ L2CC_LECB_ADD_CMD
Definition: ble_id.h:770
HCI_RD_INQ_MODE_CMD_OPCODE
@ HCI_RD_INQ_MODE_CMD_OPCODE
Definition: ble_id.h:141
HCI_LE_SET_SCAN_RSP_DATA_CMD_OPCODE
@ HCI_LE_SET_SCAN_RSP_DATA_CMD_OPCODE
Definition: ble_id.h:227
HCI_RD_LOCAL_NAME_CMD_OPCODE
@ HCI_RD_LOCAL_NAME_CMD_OPCODE
Definition: ble_id.h:104
HCI_WR_INQ_SCAN_ACT_CMD_OPCODE
@ HCI_WR_INQ_SCAN_ACT_CMD_OPCODE
Definition: ble_id.h:114
HCI_WR_INQ_SCAN_TYPE_CMD_OPCODE
@ HCI_WR_INQ_SCAN_TYPE_CMD_OPCODE
Definition: ble_id.h:140
HCI_RD_REM_SUPP_FEATS_CMD_OPCODE
@ HCI_RD_REM_SUPP_FEATS_CMD_OPCODE
Definition: ble_id.h:50
GAPC_SET_PATH_LOSS_REPORTING_PARAM_CMD
@ GAPC_SET_PATH_LOSS_REPORTING_PARAM_CMD
Definition: ble_id.h:627
HCI_SET_EVT_MASK_CMD_OPCODE
@ HCI_SET_EVT_MASK_CMD_OPCODE
Definition: ble_id.h:93
HCI_SET_AFH_HOST_CH_CLASS_CMD_OPCODE
@ HCI_SET_AFH_HOST_CH_CLASS_CMD_OPCODE
Definition: ble_id.h:138
HCI_WR_SP_DBG_MODE_CMD_OPCODE
@ HCI_WR_SP_DBG_MODE_CMD_OPCODE
Definition: ble_id.h:216
HCI_CMD_CMP_EVT_CODE
@ HCI_CMD_CMP_EVT_CODE
Definition: ble_id.h:428
GAPC_GET_INFO_CMD
@ GAPC_GET_INFO_CMD
Definition: ble_id.h:580
HCI_LE_RX_TEST_V2_CMD_OPCODE
@ HCI_LE_RX_TEST_V2_CMD_OPCODE
Definition: ble_id.h:269
HCI_LE_REJECT_CIS_REQ_CMD_OPCODE
@ HCI_LE_REJECT_CIS_REQ_CMD_OPCODE
Definition: ble_id.h:321
GAPC_RANGING_START_CMD
@ GAPC_RANGING_START_CMD
Definition: ble_id.h:634
L2CC_LECB_SDU_SEND_CMD
@ L2CC_LECB_SDU_SEND_CMD
Definition: ble_id.h:772
GAPC_SET_LE_PKT_SIZE_CMD
@ GAPC_SET_LE_PKT_SIZE_CMD
Definition: ble_id.h:609
GAPM_SET_DEV_CONFIG_CMD
@ GAPM_SET_DEV_CONFIG_CMD
Definition: ble_id.h:652
HCI_IO_CAP_REQ_REPLY_CMD_OPCODE
@ HCI_IO_CAP_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:58
GAPC_ENCRYPT_REQ_IND
@ GAPC_ENCRYPT_REQ_IND
Definition: ble_id.h:598
HCI_DBG_BT_SEND_LMP_CMD_OPCODE
@ HCI_DBG_BT_SEND_LMP_CMD_OPCODE
Definition: ble_id.h:361
HCI_MAX_EVT_MSK_PAGE_1_CODE
@ HCI_MAX_EVT_MSK_PAGE_1_CODE
Definition: ble_id.h:465
TASK_ID_GATTC
@ TASK_ID_GATTC
Definition: ble_id.h:542
HCI_REC_SYNC_TRAIN_CMD_OPCODE
@ HCI_REC_SYNC_TRAIN_CMD_OPCODE
Definition: ble_id.h:73
HCI_RD_LOCAL_SP_OPT_CMD_OPCODE
@ HCI_RD_LOCAL_SP_OPT_CMD_OPCODE
Definition: ble_id.h:197
HCI_USER_PASSKEY_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_USER_PASSKEY_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:62
HCI_INQ_CMD_OPCODE
@ HCI_INQ_CMD_OPCODE
Definition: ble_id.h:30
GAPM_ACTIVITY_STOPPED_IND
@ GAPM_ACTIVITY_STOPPED_IND
Definition: ble_id.h:692
HCI_RD_EXT_PAGE_TO_CMD_OPCODE
@ HCI_RD_EXT_PAGE_TO_CMD_OPCODE
Definition: ble_id.h:181
HCI_PARK_STATE_CMD_OPCODE
@ HCI_PARK_STATE_CMD_OPCODE
Definition: ble_id.h:80
GAPC_SET_DEV_INFO_CFM
@ GAPC_SET_DEV_INFO_CFM
Definition: ble_id.h:588
HCI_VS_AUSY_CLOCK_SAMPLE_GET_CMD_OPCODE
@ HCI_VS_AUSY_CLOCK_SAMPLE_GET_CMD_OPCODE
Definition: ble_id.h:405
HCI_RD_LOCAL_SUPP_CMDS_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_CMDS_CMD_OPCODE
Definition: ble_id.h:190
TASK_ID_LLI
@ TASK_ID_LLI
Definition: ble_id.h:533
HCI_LE_SET_CON_CTE_RX_PARAM_CMD_OPCODE
@ HCI_LE_SET_CON_CTE_RX_PARAM_CMD_OPCODE
Definition: ble_id.h:302
HCI_WR_LE_HOST_SUPP_CMD_OPCODE
@ HCI_WR_LE_HOST_SUPP_CMD_OPCODE
Definition: ble_id.h:164
TASK_API_ID
TASK_API_ID
Definition: ble_id.h:529
HCI_WR_VOICE_STG_CMD_OPCODE
@ HCI_WR_VOICE_STG_CMD_OPCODE
Definition: ble_id.h:120
HCI_PIN_CODE_REQ_REPLY_CMD_OPCODE
@ HCI_PIN_CODE_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:41
HCI_LE_SET_ADDR_RESOL_EN_CMD_OPCODE
@ HCI_LE_SET_ADDR_RESOL_EN_CMD_OPCODE
Definition: ble_id.h:263
HCI_DBG_RF_REG_RD_CMD_OPCODE
@ HCI_DBG_RF_REG_RD_CMD_OPCODE
Definition: ble_id.h:374
HCI_RD_CLK_OFF_CMP_EVT_CODE
@ HCI_RD_CLK_OFF_CMP_EVT_CODE
Definition: ble_id.h:441
HCI_ENC_KEY_REFRESH_CMP_EVT_CODE
@ HCI_ENC_KEY_REFRESH_CMP_EVT_CODE
Definition: ble_id.h:452
HCI_INQ_RES_EVT_CODE
@ HCI_INQ_RES_EVT_CODE
Definition: ble_id.h:416
HCI_LE_SET_EXT_SCAN_PARAM_CMD_OPCODE
@ HCI_LE_SET_EXT_SCAN_PARAM_CMD_OPCODE
Definition: ble_id.h:283
HCI_CMD_STATUS_EVT_CODE
@ HCI_CMD_STATUS_EVT_CODE
Definition: ble_id.h:429
HCI_USER_PASSKEY_REQ_EVT_CODE
@ HCI_USER_PASSKEY_REQ_EVT_CODE
Definition: ble_id.h:456
GAPC_ENCRYPT_CMD
@ GAPC_ENCRYPT_CMD
Definition: ble_id.h:597
HCI_RD_LOCAL_SUPP_CODECS_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_CODECS_CMD_OPCODE
Definition: ble_id.h:196
GAPM_RESET_CMD
@ GAPM_RESET_CMD
Definition: ble_id.h:651
HCI_REM_NAME_REQ_CMD_OPCODE
@ HCI_REM_NAME_REQ_CMD_OPCODE
Definition: ble_id.h:48
HCI_LE_ISO_TEST_END_CMD_OPCODE
@ HCI_LE_ISO_TEST_END_CMD_OPCODE
Definition: ble_id.h:333
HCI_CHG_CON_PKT_TYPE_CMD_OPCODE
@ HCI_CHG_CON_PKT_TYPE_CMD_OPCODE
Definition: ble_id.h:43
HCI_SYNC_CON_CMP_EVT_CODE
@ HCI_SYNC_CON_CMP_EVT_CODE
Definition: ble_id.h:448
GATTC_EVENT_CFM
@ GATTC_EVENT_CFM
Definition: ble_id.h:735
HCI_RD_AUTO_FLUSH_TO_CMD_OPCODE
@ HCI_RD_AUTO_FLUSH_TO_CMD_OPCODE
Definition: ble_id.h:121
GAPM_DEV_VERSION_IND
@ GAPM_DEV_VERSION_IND
Definition: ble_id.h:655
HCI_LK_REQ_REPLY_CMD_OPCODE
@ HCI_LK_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:39
HCI_DBG_TST_LLCP_PT_EN_CMD_OPCODE
@ HCI_DBG_TST_LLCP_PT_EN_CMD_OPCODE
Definition: ble_id.h:383
HCI_LE_RD_LOC_P256_PUB_KEY_CMD_OPCODE
@ HCI_LE_RD_LOC_P256_PUB_KEY_CMD_OPCODE
Definition: ble_id.h:255
GAPC_CMP_EVT
@ GAPC_CMP_EVT
Definition: ble_id.h:575
HCI_DBG_BLE_REG_RD_CMD_OPCODE
@ HCI_DBG_BLE_REG_RD_CMD_OPCODE
Definition: ble_id.h:370
GATTC_MTU_CHANGED_IND
@ GATTC_MTU_CHANGED_IND
Definition: ble_id.h:723
HCI_REM_NAME_REQ_CANCEL_CMD_OPCODE
@ HCI_REM_NAME_REQ_CANCEL_CMD_OPCODE
Definition: ble_id.h:49
GATTC_SEND_EVT_CMD
@ GATTC_SEND_EVT_CMD
Definition: ble_id.h:737
HCI_REJECT_CON_REQ_CMD_OPCODE
@ HCI_REJECT_CON_REQ_CMD_OPCODE
Definition: ble_id.h:38
L2CC_LECB_CONNECT_CMD
@ L2CC_LECB_CONNECT_CMD
Definition: ble_id.h:764
L2CC_LECB_DISCONNECT_IND
@ L2CC_LECB_DISCONNECT_IND
Definition: ble_id.h:769
HCI_MSG_ID_FIRST
@ HCI_MSG_ID_FIRST
Definition: ble_id.h:558
HCI_LE_ADV_REPORT_EVT_SUBCODE
@ HCI_LE_ADV_REPORT_EVT_SUBCODE
Definition: ble_id.h:486
HCI_LE_RD_ISO_LINK_QUALITY_CMD_OPCODE
@ HCI_LE_RD_ISO_LINK_QUALITY_CMD_OPCODE
Definition: ble_id.h:335
HCI_RD_LOOPBACK_MODE_CMD_OPCODE
@ HCI_RD_LOOPBACK_MODE_CMD_OPCODE
Definition: ble_id.h:213
HCI_LE_EXT_CREATE_CON_CMD_OPCODE
@ HCI_LE_EXT_CREATE_CON_CMD_OPCODE
Definition: ble_id.h:285
HCI_RD_PIN_TYPE_CMD_OPCODE
@ HCI_RD_PIN_TYPE_CMD_OPCODE
Definition: ble_id.h:97
HCI_SYNC_DATA
@ HCI_SYNC_DATA
Definition: ble_id.h:566
HCI_RD_DFT_ERR_DATA_REP_CMD_OPCODE
@ HCI_RD_DFT_ERR_DATA_REP_CMD_OPCODE
Definition: ble_id.h:155
HCI_LE_PHY_UPD_CMP_EVT_SUBCODE
@ HCI_LE_PHY_UPD_CMP_EVT_SUBCODE
Definition: ble_id.h:496
GAPM_DEV_ADV_TX_POWER_IND
@ GAPM_DEV_ADV_TX_POWER_IND
Definition: ble_id.h:657
HCI_RD_ENH_TX_PWR_LVL_CMD_OPCODE
@ HCI_RD_ENH_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:162
HCI_LE_CLEAR_PER_ADV_LIST_CMD_OPCODE
@ HCI_LE_CLEAR_PER_ADV_LIST_CMD_OPCODE
Definition: ble_id.h:291
HCI_SLV_PAGE_RSP_TO_EVT_CODE
@ HCI_SLV_PAGE_RSP_TO_EVT_CODE
Definition: ble_id.h:471
HCI_LE_CREATE_CON_CANCEL_CMD_OPCODE
@ HCI_LE_CREATE_CON_CANCEL_CMD_OPCODE
Definition: ble_id.h:232
HCI_LE_TX_TEST_V3_CMD_OPCODE
@ HCI_LE_TX_TEST_V3_CMD_OPCODE
Definition: ble_id.h:298
HCI_AUTH_REQ_CMD_OPCODE
@ HCI_AUTH_REQ_CMD_OPCODE
Definition: ble_id.h:44
L2CC_LECB_CONNECT_CFM
@ L2CC_LECB_CONNECT_CFM
Definition: ble_id.h:766
GAPM_GEN_RAND_NB_IND
@ GAPM_GEN_RAND_NB_IND
Definition: ble_id.h:666
TASK_ID_MESH
@ TASK_ID_MESH
Definition: ble_id.h:548
HCI_REM_OOB_DATA_REQ_REPLY_CMD_OPCODE
@ HCI_REM_OOB_DATA_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:63
HCI_DBG_WR_FLASH_CMD_OPCODE
@ HCI_DBG_WR_FLASH_CMD_OPCODE
Definition: ble_id.h:355
HCI_RD_TX_PWR_LVL_CMD_OPCODE
@ HCI_RD_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:127
HCI_SYNC_TRAIN_REC_EVT_CODE
@ HCI_SYNC_TRAIN_REC_EVT_CODE
Definition: ble_id.h:467
HCI_LE_RD_NB_SUPP_ADV_SETS_CMD_OPCODE
@ HCI_LE_RD_NB_SUPP_ADV_SETS_CMD_OPCODE
Definition: ble_id.h:277
HCI_LE_PER_ADV_CREATE_SYNC_CANCEL_CMD_OPCODE
@ HCI_LE_PER_ADV_CREATE_SYNC_CANCEL_CMD_OPCODE
Definition: ble_id.h:287
GAPC_PARAM_UPDATE_TO_IND
@ GAPC_PARAM_UPDATE_TO_IND
Definition: ble_id.h:640
HCI_LE_SET_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE
@ HCI_LE_SET_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE
Definition: ble_id.h:310
HCI_SET_CTRL_TO_HOST_FLOW_CTRL_CMD_OPCODE
@ HCI_SET_CTRL_TO_HOST_FLOW_CTRL_CMD_OPCODE
Definition: ble_id.h:130
HCI_CHG_CON_LK_CMP_EVT_CODE
@ HCI_CHG_CON_LK_CMP_EVT_CODE
Definition: ble_id.h:423
HCI_RD_STORED_LK_CMD_OPCODE
@ HCI_RD_STORED_LK_CMD_OPCODE
Definition: ble_id.h:100
GAPC_BOND_CFM
@ GAPC_BOND_CFM
Definition: ble_id.h:595
L2CC_SIGNALING_TRANS_TO_IND
@ L2CC_SIGNALING_TRANS_TO_IND
Definition: ble_id.h:779
HCI_RD_CLK_CMD_OPCODE
@ HCI_RD_CLK_CMD_OPCODE
Definition: ble_id.h:208
HCI_VS_SET_ISO_DATA_PATH_TRIGGER_CMD_OPCODE
@ HCI_VS_SET_ISO_DATA_PATH_TRIGGER_CMD_OPCODE
Definition: ble_id.h:395
GAPC_RANGING_IND
@ GAPC_RANGING_IND
Definition: ble_id.h:635
GATTC_SDP_SVC_IND
@ GATTC_SDP_SVC_IND
Definition: ble_id.h:747
GAPC_LE_PING_TO_VAL_IND
@ GAPC_LE_PING_TO_VAL_IND
Definition: ble_id.h:607
HCI_LE_RD_RF_PATH_COMP_CMD_OPCODE
@ HCI_LE_RD_RF_PATH_COMP_CMD_OPCODE
Definition: ble_id.h:294
HCI_SET_EVT_MASK_PAGE_2_CMD_OPCODE
@ HCI_SET_EVT_MASK_PAGE_2_CMD_OPCODE
Definition: ble_id.h:159
HCI_USER_PASSKEY_REQ_REPLY_CMD_OPCODE
@ HCI_USER_PASSKEY_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:61
TASK_ID_DBG
@ TASK_ID_DBG
Definition: ble_id.h:534
HCI_CREATE_CON_CANCEL_CMD_OPCODE
@ HCI_CREATE_CON_CANCEL_CMD_OPCODE
Definition: ble_id.h:36
HCI_DBG_BIG_SET_PARAM_CMD_OPCODE
@ HCI_DBG_BIG_SET_PARAM_CMD_OPCODE
Definition: ble_id.h:394
HCI_USER_PASSKEY_NOTIF_EVT_CODE
@ HCI_USER_PASSKEY_NOTIF_EVT_CODE
Definition: ble_id.h:461
HCI_WR_CLASS_OF_DEV_CMD_OPCODE
@ HCI_WR_CLASS_OF_DEV_CMD_OPCODE
Definition: ble_id.h:118
HCI_MAX_EVT_MSK_PAGE_2_CODE
@ HCI_MAX_EVT_MSK_PAGE_2_CODE
Definition: ble_id.h:475
HCI_LE_RD_MAX_ADV_DATA_LEN_CMD_OPCODE
@ HCI_LE_RD_MAX_ADV_DATA_LEN_CMD_OPCODE
Definition: ble_id.h:276
GAPC_READ_REMOTE_TX_PWR_CMD
@ GAPC_READ_REMOTE_TX_PWR_CMD
Definition: ble_id.h:626
GAPM_ADDR_RENEW_TO_IND
@ GAPM_ADDR_RENEW_TO_IND
Definition: ble_id.h:709
HCI_LE_RX_TEST_V1_CMD_OPCODE
@ HCI_LE_RX_TEST_V1_CMD_OPCODE
Definition: ble_id.h:247
HCI_WR_LOOPBACK_MODE_CMD_OPCODE
@ HCI_WR_LOOPBACK_MODE_CMD_OPCODE
Definition: ble_id.h:214
GAPC_SEC_REQ_TIMEOUT_IND
@ GAPC_SEC_REQ_TIMEOUT_IND
Definition: ble_id.h:605
HCI_RD_LINK_POL_STG_CMD_OPCODE
@ HCI_RD_LINK_POL_STG_CMD_OPCODE
Definition: ble_id.h:85
GAPC_PEER_ATT_INFO_IND
@ GAPC_PEER_ATT_INFO_IND
Definition: ble_id.h:581
HCI_WR_CURR_IAC_LAP_CMD_OPCODE
@ HCI_WR_CURR_IAC_LAP_CMD_OPCODE
Definition: ble_id.h:137
HCI_LE_RD_REM_FEATS_CMP_EVT_SUBCODE
@ HCI_LE_RD_REM_FEATS_CMP_EVT_SUBCODE
Definition: ble_id.h:488
HCI_SNIFF_SUB_EVT_CODE
@ HCI_SNIFF_SUB_EVT_CODE
Definition: ble_id.h:450
GAPM_PER_ADV_CTE_TX_CTL_CMD
@ GAPM_PER_ADV_CTE_TX_CTL_CMD
Definition: ble_id.h:705
HCI_LE_CON_UPDATE_CMD_OPCODE
@ HCI_LE_CON_UPDATE_CMD_OPCODE
Definition: ble_id.h:237
HCI_SET_MWS_CHANNEL_PARAMS_CMD_OPCODE
@ HCI_SET_MWS_CHANNEL_PARAMS_CMD_OPCODE
Definition: ble_id.h:165
HCI_RD_LOC_OOB_EXT_DATA_CMD_OPCODE
@ HCI_RD_LOC_OOB_EXT_DATA_CMD_OPCODE
Definition: ble_id.h:180
HCI_LE_PER_ADV_SYNC_LOST_EVT_SUBCODE
@ HCI_LE_PER_ADV_SYNC_LOST_EVT_SUBCODE
Definition: ble_id.h:500
gapc_msg_id
gapc_msg_id
Definition: ble_id.h:574
HCI_LE_TIME_SYNC_EN_CMD_OPCODE
@ HCI_LE_TIME_SYNC_EN_CMD_OPCODE
Definition: ble_id.h:347
HCI_LE_TX_TEST_V4_CMD_OPCODE
@ HCI_LE_TX_TEST_V4_CMD_OPCODE
Definition: ble_id.h:341
HCI_LE_SET_CON_CTE_TX_PARAM_CMD_OPCODE
@ HCI_LE_SET_CON_CTE_TX_PARAM_CMD_OPCODE
Definition: ble_id.h:303
HCI_ENH_FLUSH_CMP_EVT_CODE
@ HCI_ENH_FLUSH_CMP_EVT_CODE
Definition: ble_id.h:460
HCI_DEL_RES_LT_ADDR_CMD_OPCODE
@ HCI_DEL_RES_LT_ADDR_CMD_OPCODE
Definition: ble_id.h:172
HCI_DBG_TEST_SCH_PLAN_REQ_CMD_OPCODE
@ HCI_DBG_TEST_SCH_PLAN_REQ_CMD_OPCODE
Definition: ble_id.h:400
HCI_RD_ENC_KEY_SIZE_CMD_OPCODE
@ HCI_RD_ENC_KEY_SIZE_CMD_OPCODE
Definition: ble_id.h:209
HCI_LE_ENH_CON_CMP_EVT_SUBCODE
@ HCI_LE_ENH_CON_CMP_EVT_SUBCODE
Definition: ble_id.h:494
GAPC_ENCRYPT_CFM
@ GAPC_ENCRYPT_CFM
Definition: ble_id.h:599
HCI_DBG_WLAN_COEX_CMD_OPCODE
@ HCI_DBG_WLAN_COEX_CMD_OPCODE
Definition: ble_id.h:359
HCI_DBG_RD_KE_STATS_CMD_OPCODE
@ HCI_DBG_RD_KE_STATS_CMD_OPCODE
Definition: ble_id.h:363
HCI_AUTH_CMP_EVT_CODE
@ HCI_AUTH_CMP_EVT_CODE
Definition: ble_id.h:420
HCI_REM_OOB_DATA_REQ_EVT_CODE
@ HCI_REM_OOB_DATA_REQ_EVT_CODE
Definition: ble_id.h:457
HCI_DEL_STORED_LK_CMD_OPCODE
@ HCI_DEL_STORED_LK_CMD_OPCODE
Definition: ble_id.h:102
HCI_RD_LOCAL_SUPP_CODECS_V2_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_CODECS_V2_CMD_OPCODE
Definition: ble_id.h:198
HCI_LE_TX_TEST_V1_CMD_OPCODE
@ HCI_LE_TX_TEST_V1_CMD_OPCODE
Definition: ble_id.h:248
HCI_LE_PER_ADV_TERM_SYNC_CMD_OPCODE
@ HCI_LE_PER_ADV_TERM_SYNC_CMD_OPCODE
Definition: ble_id.h:288
HCI_LE_RMV_DEV_FROM_WLST_CMD_OPCODE
@ HCI_LE_RMV_DEV_FROM_WLST_CMD_OPCODE
Definition: ble_id.h:236
HCI_LE_RD_BUF_SIZE_CMD_OPCODE
@ HCI_LE_RD_BUF_SIZE_CMD_OPCODE
Definition: ble_id.h:221
GATTC_READ_CFM
@ GATTC_READ_CFM
Definition: ble_id.h:741
HCI_PAGE_SCAN_REPET_MODE_CHG_EVT_CODE
@ HCI_PAGE_SCAN_REPET_MODE_CHG_EVT_CODE
Definition: ble_id.h:444
L2CC_LECB_ADD_IND
@ L2CC_LECB_ADD_IND
Definition: ble_id.h:771
HCI_LE_SET_PER_ADV_REC_EN_CMD_OPCODE
@ HCI_LE_SET_PER_ADV_REC_EN_CMD_OPCODE
Definition: ble_id.h:307
GATTC_SERVER_RTX_IND
@ GATTC_SERVER_RTX_IND
Definition: ble_id.h:751
GAPM_ADDR_SOLVED_IND
@ GAPM_ADDR_SOLVED_IND
Definition: ble_id.h:661
GAPM_NB_ADV_SETS_IND
@ GAPM_NB_ADV_SETS_IND
Definition: ble_id.h:698
HCI_RD_FAIL_CONTACT_CNT_CMD_OPCODE
@ HCI_RD_FAIL_CONTACT_CNT_CMD_OPCODE
Definition: ble_id.h:203
HCI_LE_REM_CON_PARAM_REQ_EVT_SUBCODE
@ HCI_LE_REM_CON_PARAM_REQ_EVT_SUBCODE
Definition: ble_id.h:490
HCI_IO_CAP_REQ_EVT_CODE
@ HCI_IO_CAP_REQ_EVT_CODE
Definition: ble_id.h:453
GAPM_LE_TEST_MODE_CTRL_CMD
@ GAPM_LE_TEST_MODE_CTRL_CMD
Definition: ble_id.h:676
HCI_WR_INQ_TX_PWR_LVL_CMD_OPCODE
@ HCI_WR_INQ_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:154
GAPM_USE_ENC_BLOCK_IND
@ GAPM_USE_ENC_BLOCK_IND
Definition: ble_id.h:664
hci_evt_code
hci_evt_code
Definition: ble_id.h:414
HCI_LE_ACCEPT_CIS_REQ_CMD_OPCODE
@ HCI_LE_ACCEPT_CIS_REQ_CMD_OPCODE
Definition: ble_id.h:320
HCI_MASTER_LK_CMP_EVT_CODE
@ HCI_MASTER_LK_CMP_EVT_CODE
Definition: ble_id.h:424
HCI_LE_SCAN_TIMEOUT_EVT_SUBCODE
@ HCI_LE_SCAN_TIMEOUT_EVT_SUBCODE
Definition: ble_id.h:501
HCI_WR_DFT_LINK_POL_STG_CMD_OPCODE
@ HCI_WR_DFT_LINK_POL_STG_CMD_OPCODE
Definition: ble_id.h:88
HCI_LE_SET_EXT_SCAN_RSP_DATA_CMD_OPCODE
@ HCI_LE_SET_EXT_SCAN_RSP_DATA_CMD_OPCODE
Definition: ble_id.h:274
HCI_LE_RD_LOC_RSLV_ADDR_CMD_OPCODE
@ HCI_LE_RD_LOC_RSLV_ADDR_CMD_OPCODE
Definition: ble_id.h:262
HCI_WR_PAGE_SCAN_ACT_CMD_OPCODE
@ HCI_WR_PAGE_SCAN_ACT_CMD_OPCODE
Definition: ble_id.h:112
HCI_SET_ECO_BASE_INTV_CMD_OPCODE
@ HCI_SET_ECO_BASE_INTV_CMD_OPCODE
Definition: ble_id.h:185
HCI_LE_REMOVE_CIG_CMD_OPCODE
@ HCI_LE_REMOVE_CIG_CMD_OPCODE
Definition: ble_id.h:319
HCI_RESET_CMD_OPCODE
@ HCI_RESET_CMD_OPCODE
Definition: ble_id.h:94
hci_opcode
hci_opcode
Definition: ble_id.h:26
HCI_QOS_SETUP_CMP_EVT_CODE
@ HCI_QOS_SETUP_CMP_EVT_CODE
Definition: ble_id.h:427
HCI_VS_SET_PREF_SLAVE_EVT_DUR_CMD_OPCODE
@ HCI_VS_SET_PREF_SLAVE_EVT_DUR_CMD_OPCODE
Definition: ble_id.h:367
HCI_LE_CREATE_BIG_CMD_OPCODE
@ HCI_LE_CREATE_BIG_CMD_OPCODE
Definition: ble_id.h:322
HCI_LE_LTK_REQUEST_EVT_SUBCODE
@ HCI_LE_LTK_REQUEST_EVT_SUBCODE
Definition: ble_id.h:489
GATTC_REG_TO_PEER_EVT_CMD
@ GATTC_REG_TO_PEER_EVT_CMD
Definition: ble_id.h:736
HCI_VS_RD_PICONET_CLOCK_CMD_OPCODE
@ HCI_VS_RD_PICONET_CLOCK_CMD_OPCODE
Definition: ble_id.h:390
HCI_RD_LMP_HDL_CMD_OPCODE
@ HCI_RD_LMP_HDL_CMD_OPCODE
Definition: ble_id.h:54
GAPM_RAL_ADDR_IND
@ GAPM_RAL_ADDR_IND
Definition: ble_id.h:672
GAPC_RANGING_CMP_IND
@ GAPC_RANGING_CMP_IND
Definition: ble_id.h:637
HCI_DBG_ISO_SET_PARAM_CMD_OPCODE
@ HCI_DBG_ISO_SET_PARAM_CMD_OPCODE
Debug commands for ISO.
Definition: ble_id.h:392
HCI_TRUNC_PAGE_CMD_OPCODE
@ HCI_TRUNC_PAGE_CMD_OPCODE
Definition: ble_id.h:68
HCI_RD_CLK_OFF_CMD_OPCODE
@ HCI_RD_CLK_OFF_CMD_OPCODE
Definition: ble_id.h:53
HCI_LE_TEST_END_CMD_OPCODE
@ HCI_LE_TEST_END_CMD_OPCODE
Definition: ble_id.h:249
HCI_LE_PATH_LOSS_THRESHOLD_EVT_SUBCODE
@ HCI_LE_PATH_LOSS_THRESHOLD_EVT_SUBCODE
Definition: ble_id.h:516
HCI_LE_TERMINATE_BIG_CMD_OPCODE
@ HCI_LE_TERMINATE_BIG_CMD_OPCODE
Definition: ble_id.h:324
GAPC_CON_RSSI_IND
@ GAPC_CON_RSSI_IND
Definition: ble_id.h:584
TASK_ID_LLM
@ TASK_ID_LLM
Definition: ble_id.h:530
GAPC_ENCRYPT_IND
@ GAPC_ENCRYPT_IND
Definition: ble_id.h:600
HCI_LE_RD_TX_PWR_CMD_OPCODE
@ HCI_LE_RD_TX_PWR_CMD_OPCODE
Definition: ble_id.h:293
HCI_REFRESH_ENC_KEY_CMD_OPCODE
@ HCI_REFRESH_ENC_KEY_CMD_OPCODE
Definition: ble_id.h:149
HCI_ACCEPT_SYNC_CON_REQ_CMD_OPCODE
@ HCI_ACCEPT_SYNC_CON_REQ_CMD_OPCODE
Definition: ble_id.h:56
HCI_LE_LTK_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_LE_LTK_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:245
GAPM_SET_ADV_DATA_CMD
@ GAPM_SET_ADV_DATA_CMD
Definition: ble_id.h:693
HCI_RD_CON_ACCEPT_TO_CMD_OPCODE
@ HCI_RD_CON_ACCEPT_TO_CMD_OPCODE
Definition: ble_id.h:105
HCI_SET_CON_ENC_CMD_OPCODE
@ HCI_SET_CON_ENC_CMD_OPCODE
Definition: ble_id.h:45
GAPM_MAX_DATA_LEN_IND
@ GAPM_MAX_DATA_LEN_IND
Definition: ble_id.h:671