Public Attributes | List of all members
ble_gap_adv_prim_cfg_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Configuration for advertising on primary channel. More...

`#include <ble_gapm.h>`

## Public Attributes
uint32_t | adv_intv_min
uint32_t | adv_intv_max
uint8_t | chnl_map
ble_gap_le_phy_value_t | phy

## Detailed Description

Configuration for advertising on primary channel.

Definition at line 554 of file ble_gapm.h.

## Member Data Documentation

## ◆ adv_intv_max

uint32_t ble_gap_adv_prim_cfg_t::adv_intv_max

Maximum advertising interval (in unit of 625 μs). Must be greater than 20 ms.

Definition at line 557 of file ble_gapm.h.

## ◆ adv_intv_min

uint32_t ble_gap_adv_prim_cfg_t::adv_intv_min

Minimum advertising interval (in unit of 625 μs). Must be greater than 20 ms.

Definition at line 556 of file ble_gapm.h.

## ◆ chnl_map

uint8_t ble_gap_adv_prim_cfg_t::chnl_map

Bit field indicating the channel map. See GAP ADV CHANNEL (bitmask).

Definition at line 558 of file ble_gapm.h.

## ◆ phy

ble_gap_le_phy_value_t ble_gap_adv_prim_cfg_t::phy

Indicate on which PHY primary advertising has to be performed. See enum ble_gap_le_phy_value_t. Note that LE 2M PHY is not allowed and that legacy advertising only supports LE 1M PHY.

Definition at line 559 of file ble_gapm.h.

The documentation for this struct was generated from the following file:

- ble_gapm.h