Here is a list of all file members with links to the files they belong to:

### - s -

- s_ble_evt_handler : ble_event.h
- SAMPLES_CONNECTION_MAX : sample_service.h
- samples_evt_handler_t : sample_service.h
- SAMPLES_EVT_INVALID : sample_service.h
- SAMPLES_EVT_RX_RECEIVE_DATA : sample_service.h
- SAMPLES_EVT_TX_NOTIFICATION_DISABLED : sample_service.h
- SAMPLES_EVT_TX_NOTIFICATION_ENABLED : sample_service.h
- SAMPLES_EVT_TX_NOTIFY_COMPLETE : sample_service.h
- samples_evt_type_t : sample_service.h
- SAMPLES_INSTANCE_MAX : sample_service.h
- SAMPLES_MAX_DATA_LEN : sample_service.h
- samples_notify_tx_data() : sample_service.h
- samples_service_init() : sample_service.h
- SAMPLES_SERVICE_UUID : sample_service.h
- SCA0 : ble_iso.h
- SCA1 : ble_iso.h
- SCA2 : ble_iso.h
- SCA3 : ble_iso.h
- SCA4 : ble_iso.h
- SCA5 : ble_iso.h
- SCA6 : ble_iso.h
- SCA7 : ble_iso.h
- SDK_ERR_ADV_DATA_NOT_SET : ble_error.h
- SDK_ERR_APP_ERROR : ble_error.h
- SDK_ERR_BUSY : ble_error.h
- SDK_ERR_CACHE_INVALID : ble_error.h
- SDK_ERR_CACHE_NOT_ENABLE : ble_error.h
- SDK_ERR_DISALLOWED : ble_error.h
- SDK_ERR_DISCONNECTED : ble_error.h
- SDK_ERR_EXT_SCAN_RSP_DATA_NOT_SET : ble_error.h
- SDK_ERR_FEATURE_NOT_ENABLE : ble_error.h
- SDK_ERR_IND_DISABLED : ble_error.h
- SDK_ERR_INVALID_ADDRESS : ble_error.h
- SDK_ERR_INVALID_ADV_DATA_TYPE : ble_error.h
- SDK_ERR_INVALID_ADV_IDX : ble_error.h
- SDK_ERR_INVALID_ADV_INTERVAL : ble_error.h
- SDK_ERR_INVALID_ADV_PARAM : ble_error.h
- SDK_ERR_INVALID_ADV_PEER_ADDR : ble_error.h
- SDK_ERR_INVALID_ATT_VAL_LEN : ble_error.h
- SDK_ERR_INVALID_BUFF_LENGTH : ble_error.h
- SDK_ERR_INVALID_CHL_NUM : ble_error.h
- SDK_ERR_INVALID_CID : ble_error.h
- SDK_ERR_INVALID_CONN_IDX : ble_error.h
- SDK_ERR_INVALID_DATA_LENGTH : ble_error.h
- SDK_ERR_INVALID_DISVCOVERY_MODE : ble_error.h
- SDK_ERR_INVALID_DURATION_PARAM : ble_error.h
- SDK_ERR_INVALID_HANDLE : ble_error.h
- SDK_ERR_INVALID_OFFSET : ble_error.h
- SDK_ERR_INVALID_PARAM : ble_error.h
- SDK_ERR_INVALID_PER_SYNC_IDX : ble_error.h
- SDK_ERR_INVALID_PERM : ble_error.h
- SDK_ERR_INVALID_PSM_ALREADY_REGISTERED : ble_error.h
- SDK_ERR_INVALID_PSM_EXCEEDED_MAX_PSM_NUM : ble_error.h
- SDK_ERR_INVALID_PSM_NUM : ble_error.h
- SDK_ERR_LIST_FULL : ble_error.h
- SDK_ERR_LIST_ITEM_ALREADY_EXISTED : ble_error.h
- SDK_ERR_LIST_ITEM_NOT_FOUND : ble_error.h
- SDK_ERR_NO_RESOURCES : ble_error.h
- SDK_ERR_NOT_ENOUGH_CREDITS : ble_error.h
- SDK_ERR_NTF_DISABLED : ble_error.h
- SDK_ERR_NVDS_NOT_INIT : ble_error.h
- SDK_ERR_PER_ADV_DATA_NOT_SET : ble_error.h
- SDK_ERR_POINTER_NULL : ble_error.h
- SDK_ERR_PROFILE_COUNT : ble_error.h
- SDK_ERR_REPEAT_CID : ble_error.h
- SDK_ERR_REQ_NOT_SUPPORTED : ble_error.h
- SDK_ERR_SDK_INTERNAL : ble_error.h
- sdk_err_t : ble_error.h
- SDK_ERR_TIMER_INSUFFICIENT : ble_error.h
- SDK_SUCCESS : ble_error.h
- sec_rcv_bond_ind_handler() : ble_msg.h
- sec_rcv_bond_req_ind_handler() : ble_msg.h
- sec_rcv_encrypt_ind_handler() : ble_msg.h
- sec_rcv_encrypt_req_ind_handler() : ble_msg.h
- sec_rcv_sec_req_ind_handler() : ble_msg.h
- sec_rcv_sec_req_timeout_ind_handler() : ble_msg.h
- sec_rcv_sign_counter_update_ind_handler() : ble_msg.h
- SEM_NO_WAIT : app_rtos_cfg.h
- sem_t : app_rtos_cfg.h
- SEM_WAIT_FOREVER : app_rtos_cfg.h
- SET_GPIO_ALTFUNCCLR : gr533x_ll_gpio.h
- SET_GPIO_ALTFUNCSET : gr533x_ll_gpio.h
- SET_GPIO_DATA : gr533x_ll_gpio.h
- SET_GPIO_DATAOUT : gr533x_ll_gpio.h
- SET_GPIO_INTDBECLR : gr533x_ll_gpio.h
- SET_GPIO_INTDBESET : gr533x_ll_gpio.h
- SET_GPIO_INTENCLR : gr533x_ll_gpio.h
- SET_GPIO_INTENSET : gr533x_ll_gpio.h
- SET_GPIO_INTPOLCLR : gr533x_ll_gpio.h
- SET_GPIO_INTPOLSET : gr533x_ll_gpio.h
- SET_GPIO_INTSTAT : gr533x_ll_gpio.h
- SET_GPIO_INTTYPECLR : gr533x_ll_gpio.h
- SET_GPIO_INTTYPESET : gr533x_ll_gpio.h
- SET_GPIO_OUTENCLR : gr533x_ll_gpio.h
- SET_GPIO_OUTENSET : gr533x_ll_gpio.h
- set_io_ldo_use_3p3_v() : gr533x_sys_sdk.h
- slow_clock_type_t : platform_sdk.h
- SPI_DATASIZE_10BIT : gr533x_hal_spi.h
- SPI_DATASIZE_11BIT : gr533x_hal_spi.h
- SPI_DATASIZE_12BIT : gr533x_hal_spi.h
- SPI_DATASIZE_13BIT : gr533x_hal_spi.h
- SPI_DATASIZE_14BIT : gr533x_hal_spi.h
- SPI_DATASIZE_15BIT : gr533x_hal_spi.h
- SPI_DATASIZE_16BIT : gr533x_hal_spi.h
- SPI_DATASIZE_17BIT : gr533x_hal_spi.h
- SPI_DATASIZE_18BIT : gr533x_hal_spi.h
- SPI_DATASIZE_19BIT : gr533x_hal_spi.h
- SPI_DATASIZE_20BIT : gr533x_hal_spi.h
- SPI_DATASIZE_21BIT : gr533x_hal_spi.h
- SPI_DATASIZE_22BIT : gr533x_hal_spi.h
- SPI_DATASIZE_23BIT : gr533x_hal_spi.h
- SPI_DATASIZE_24BIT : gr533x_hal_spi.h
- SPI_DATASIZE_25BIT : gr533x_hal_spi.h
- SPI_DATASIZE_26BIT : gr533x_hal_spi.h
- SPI_DATASIZE_27BIT : gr533x_hal_spi.h
- SPI_DATASIZE_28BIT : gr533x_hal_spi.h
- SPI_DATASIZE_29BIT : gr533x_hal_spi.h
- SPI_DATASIZE_30BIT : gr533x_hal_spi.h
- SPI_DATASIZE_31BIT : gr533x_hal_spi.h
- SPI_DATASIZE_32BIT : gr533x_hal_spi.h
- SPI_DATASIZE_4BIT : gr533x_hal_spi.h
- SPI_DATASIZE_5BIT : gr533x_hal_spi.h
- SPI_DATASIZE_6BIT : gr533x_hal_spi.h
- SPI_DATASIZE_7BIT : gr533x_hal_spi.h
- SPI_DATASIZE_8BIT : gr533x_hal_spi.h
- SPI_DATASIZE_9BIT : gr533x_hal_spi.h
- SPI_DIRECTION_FULL_DUPLEX : gr533x_hal_spi.h
- SPI_DIRECTION_READ_EEPROM : gr533x_hal_spi.h
- SPI_DIRECTION_SIMPLEX_RX : gr533x_hal_spi.h
- SPI_DIRECTION_SIMPLEX_TX : gr533x_hal_spi.h
- SPI_FLAG_BUSY : gr533x_hal_spi.h
- SPI_FLAG_DCOL : gr533x_hal_spi.h
- SPI_FLAG_RFF : gr533x_hal_spi.h
- SPI_FLAG_RFNE : gr533x_hal_spi.h
- SPI_FLAG_TFE : gr533x_hal_spi.h
- SPI_FLAG_TFNF : gr533x_hal_spi.h
- SPI_FLAG_TXE : gr533x_hal_spi.h
- spi_handle_t : gr533x_hal_spi.h
- spi_init_t : gr533x_hal_spi.h
- SPI_IT_MST : gr533x_hal_spi.h
- SPI_IT_RXF : gr533x_hal_spi.h
- SPI_IT_RXO : gr533x_hal_spi.h
- SPI_IT_RXU : gr533x_hal_spi.h
- SPI_IT_TXE : gr533x_hal_spi.h
- SPI_IT_TXO : gr533x_hal_spi.h
- SPI_PHASE_1EDGE : gr533x_hal_spi.h
- SPI_PHASE_2EDGE : gr533x_hal_spi.h
- SPI_POLARITY_HIGH : gr533x_hal_spi.h
- SPI_POLARITY_LOW : gr533x_hal_spi.h
- SPI_PWR_ID : app_pwr_mgmt.h
- SPI_RX_FIFO_LEVEL_MAX : gr533x_hal_spi.h
- SPI_SLAVE_SELECT_0 : gr533x_hal_spi.h
- SPI_SLAVE_SELECT_1 : gr533x_hal_spi.h
- SPI_SLAVE_SELECT_ALL : gr533x_hal_spi.h
- SPI_SOFT_CS_MAGIC_NUMBER : gr533x_hal_spi.h
- SPI_TIMODE_DISABLE : gr533x_hal_spi.h
- SPI_TIMODE_ENABLE : gr533x_hal_spi.h
- SPI_TX_FIFO_LEVEL_MAX : gr533x_hal_spi.h
- sram_size_t : gr533x_sys_sdk.h
- srpg_before_func_t : gr533x_pwr.h
- SYNC_STATE_ACTIVE : esls.h
- SYNC_STATE_IDLE : esls.h
- SYNC_STATE_MAX : esls.h
- SYNC_STATE_START : esls.h
- SYNCHRONIZE_STATE : esls.h
- sys_adc_trim_get() : gr533x_sys_sdk.h
- sys_app_printf() : gr533x_sys_sdk.h
- sys_assert_cb_register() : gr533x_sys_sdk.h
- sys_attdb_usage_ratio_get() : gr533x_sys_sdk.h
- SYS_BD_ADDR_LEN : gr533x_sys_sdk.h
- sys_ble_heartbeat_period_get() : gr533x_sys_sdk.h
- sys_ble_heartbeat_period_set() : gr533x_sys_sdk.h
- SYS_BOOT_SETTING_PATTERN : gr533x_sys_sdk.h
- SYS_BOOT_SETTING_RSV_MAGIC : gr533x_sys_sdk.h
- SYS_BOOT_SETTING_SWD_DISABLE : gr533x_sys_sdk.h
- SYS_BOOT_SETTING_SWD_ENABLE : gr533x_sys_sdk.h
- sys_boot_setting_t : gr533x_sys_sdk.h
- SYS_CHIP_UID_LEN : gr533x_sys_sdk.h
- sys_context_func_t : gr533x_sys_sdk.h
- sys_context_save() : gr533x_sys_sdk.h
- sys_crystal_trim_get() : gr533x_sys_sdk.h
- sys_dcdc_sysldo_dcore_init() : platform_sdk.h
- SYS_DEV_SRAM_48K : gr533x_sys_sdk.h
- SYS_DEV_SRAM_64K : gr533x_sys_sdk.h
- SYS_DEV_SRAM_80K : gr533x_sys_sdk.h
- SYS_DEV_SRAM_96K : gr533x_sys_sdk.h
- sys_device_addr_get() : gr533x_sys_sdk.h
- sys_device_is_PACKAGE_GR5331DEBI() : gr533x_sys_sdk.h
- sys_device_lp_gain_offset_2m_get() : gr533x_sys_sdk.h
- sys_device_package_get() : gr533x_sys_sdk.h
- sys_device_sram_get() : gr533x_sys_sdk.h
- sys_device_uid_get() : gr533x_sys_sdk.h
- sys_env_usage_ratio_get() : gr533x_sys_sdk.h
- sys_firmware_jump() : gr533x_sys_sdk.h
- sys_free() : gr533x_sys_sdk.h
- sys_hw_version_get() : gr533x_sys_sdk.h
- sys_hw_version_is_B3() : gr533x_sys_sdk.h
- SYS_INVALID_TIMER_ID : gr533x_sys_sdk.h
- sys_ke_sleep_check() : gr533x_sys_sdk.h
- sys_lld_max_msg_usage_ratio_set() : gr533x_sys_sdk.h
- sys_lpclk_get() : gr533x_sys_sdk.h
- sys_lpclk_set() : gr533x_sys_sdk.h
- sys_lpcycles_2_hus() : gr533x_sys_sdk.h
- sys_lpper_get() : gr533x_sys_sdk.h
- sys_malloc() : gr533x_sys_sdk.h
- sys_max_msg_usage_ratio_set() : gr533x_sys_sdk.h
- sys_msg_usage_ratio_get() : gr533x_sys_sdk.h
- sys_nonret_usage_ratio_get() : gr533x_sys_sdk.h
- sys_pmu_ddvs_dcore_adjust() : platform_sdk.h
- sys_pmu_ddvs_ringo_get() : platform_sdk.h
- sys_pmu_is_ff_chip() : platform_sdk.h
- sys_pmu_is_ss_chip() : platform_sdk.h
- sys_pmu_trim_get() : gr533x_sys_sdk.h
- sys_power_t : platform_sdk.h
- sys_rf_trim_get() : gr533x_sys_sdk.h
- sys_ringo_trim_get() : gr533x_sys_sdk.h
- SYS_ROM_VERSION_ADDR : gr533x_sys_sdk.h
- SYS_SCA_SETTING_ADDR : gr533x_sys_sdk.h
- sys_sdk_ultra_conn_update() : gr533x_sys_sdk.h
- sys_sdk_verison_get() : gr533x_sys_sdk.h
- sys_security_data_use_present() : gr533x_sys_sdk.h
- SYS_SET_BD_ADDR : gr533x_sys_sdk.h
- sys_signal_handler_register() : gr533x_sys_sdk.h
- sys_swd_disable() : gr533x_sys_sdk.h
- sys_swd_enable() : gr533x_sys_sdk.h
- sys_trim_sum_get() : gr533x_sys_sdk.h
- sys_us_2_lpcycles() : gr533x_sys_sdk.h
- SYSLDO_MODE : platform_sdk.h
- system_lp_table_update_twval() : platform_sdk.h
- system_pmu_calibration_stop() : platform_sdk.h
- system_pmu_deinit() : platform_sdk.h
- system_pmu_init() : platform_sdk.h
- system_power_mode() : platform_sdk.h
- SYSTICK_CURRENT_VALUE : gr533x_hal.h
- SYSTICK_RELOAD_VALUE : gr533x_hal.h