### - h -

- hal_adc_conv_cplt_callback() : gr533x_hal_adc.h
- hal_adc_deinit() : gr533x_hal_adc.h
- hal_adc_deinit_ext() : gr533x_hal_br.h
- hal_adc_get_dma_threshold() : gr533x_hal_adc.h
- hal_adc_get_error() : gr533x_hal_adc.h
- hal_adc_get_state() : gr533x_hal_adc.h
- hal_adc_init() : gr533x_hal_adc.h
- hal_adc_init_ext() : gr533x_hal_br.h
- hal_adc_msp_deinit() : gr533x_hal_adc.h
- hal_adc_msp_init() : gr533x_hal_adc.h
- hal_adc_poll_for_conversion() : gr533x_hal_adc.h
- hal_adc_register_callback() : gr533x_hal_br.h
- hal_adc_resume_reg() : gr533x_hal_adc.h
- hal_adc_set_dma_threshold() : gr533x_hal_adc.h
- hal_adc_start_dma() : gr533x_hal_adc.h
- hal_adc_stop_dma() : gr533x_hal_adc.h
- hal_adc_suspend_reg() : gr533x_hal_adc.h
- hal_adc_temperature_conv() : gr533x_hal_adc.h
- hal_adc_vbat_conv() : gr533x_hal_adc.h
- hal_adc_voltage_extern() : gr533x_hal_adc.h
- hal_adc_voltage_intern() : gr533x_hal_adc.h
- hal_aon_gpio_callback() : gr533x_hal_aon_gpio.h
- hal_aon_gpio_deinit() : gr533x_hal_aon_gpio.h
- hal_aon_gpio_deinit_ext() : gr533x_hal_br.h
- hal_aon_gpio_init() : gr533x_hal_aon_gpio.h
- hal_aon_gpio_init_ext() : gr533x_hal_br.h
- hal_aon_gpio_irq_handler() : gr533x_hal_aon_gpio.h
- hal_aon_gpio_read_pin() : gr533x_hal_aon_gpio.h
- hal_aon_gpio_register_callback() : gr533x_hal_br.h
- hal_aon_gpio_toggle_pin() : gr533x_hal_aon_gpio.h
- hal_aon_gpio_write_pin() : gr533x_hal_aon_gpio.h
- hal_aon_wdt_alarm_callback() : gr533x_hal_aon_wdt.h
- hal_aon_wdt_deinit() : gr533x_hal_aon_wdt.h
- hal_aon_wdt_deinit_ext() : gr533x_hal_br.h
- hal_aon_wdt_init() : gr533x_hal_aon_wdt.h
- hal_aon_wdt_init_ext() : gr533x_hal_br.h
- hal_aon_wdt_irq_handler() : gr533x_hal_aon_wdt.h
- hal_aon_wdt_refresh() : gr533x_hal_aon_wdt.h
- hal_aon_wdt_register_callback() : gr533x_hal_br.h
- hal_bod2_auto_power_bypass_enable() : gr533x_hal_bod.h
- hal_bod2_enable() : gr533x_hal_bod.h
- hal_bod2_set_level() : gr533x_hal_bod.h
- hal_bod_deinit() : gr533x_hal_bod.h
- hal_bod_enable() : gr533x_hal_bod.h
- hal_bod_fedge_callback() : gr533x_hal_bod.h
- hal_bod_fedge_irq_handler() : gr533x_hal_bod.h
- hal_bod_init() : gr533x_hal_bod.h
- hal_bod_msp_deinit() : gr533x_hal_bod.h
- hal_bod_msp_init() : gr533x_hal_bod.h
- hal_bod_redge_callback() : gr533x_hal_bod.h
- hal_bod_redge_irq_handler() : gr533x_hal_bod.h
- hal_bod_static_mode_enable() : gr533x_hal_bod.h
- hal_calendar_alarm_callback() : gr533x_hal_calendar.h
- hal_calendar_deinit() : gr533x_hal_calendar.h
- hal_calendar_deinit_ext() : gr533x_hal_br.h
- hal_calendar_disable_event() : gr533x_hal_calendar.h
- hal_calendar_get_time() : gr533x_hal_calendar.h
- hal_calendar_init() : gr533x_hal_calendar.h
- hal_calendar_init_ext() : gr533x_hal_br.h
- hal_calendar_init_time() : gr533x_hal_calendar.h
- hal_calendar_irq_handler() : gr533x_hal_calendar.h
- hal_calendar_overflow_callback() : gr533x_hal_calendar.h
- hal_calendar_register_callback() : gr533x_hal_br.h
- hal_calendar_set_alarm() : gr533x_hal_calendar.h
- hal_calendar_set_tick() : gr533x_hal_calendar.h
- hal_calendar_sync_time() : gr533x_hal_calendar.h
- hal_calendar_tick_callback() : gr533x_hal_calendar.h
- hal_cgc_config_force_clk() : gr533x_hal_cgc.h
- hal_cgc_config_wfi_clk() : gr533x_hal_cgc.h
- hal_cgc_deinit() : gr533x_hal_cgc.h
- hal_cgc_get_force_clk() : gr533x_hal_cgc.h
- hal_cgc_get_wfi_clk() : gr533x_hal_cgc.h
- hal_cgc_init() : gr533x_hal_cgc.h
- hal_clock_get_device_xo_request_status() : gr533x_hal_clock.h
- hal_clock_get_xo_requests() : gr533x_hal_clock.h
- hal_clock_release_xo_osc() : gr533x_hal_clock.h
- hal_clock_release_xo_osc_all() : gr533x_hal_clock.h
- hal_clock_request_xo_osc() : gr533x_hal_clock.h
- hal_comp_deinit() : gr533x_hal_comp.h
- hal_comp_deinit_ext() : gr533x_hal_br.h
- hal_comp_falling_trigger_callback() : gr533x_hal_comp.h
- hal_comp_get_error() : gr533x_hal_comp.h
- hal_comp_get_state() : gr533x_hal_comp.h
- hal_comp_init() : gr533x_hal_comp.h
- hal_comp_init_ext() : gr533x_hal_br.h
- hal_comp_irq_handler() : gr533x_hal_comp.h
- hal_comp_msp_deinit() : gr533x_hal_comp.h
- hal_comp_msp_init() : gr533x_hal_comp.h
- hal_comp_register_callback() : gr533x_hal_br.h
- hal_comp_resume_reg() : gr533x_hal_comp.h
- hal_comp_rising_trigger_callback() : gr533x_hal_comp.h
- hal_comp_start() : gr533x_hal_comp.h
- hal_comp_stop() : gr533x_hal_comp.h
- hal_comp_suspend_reg() : gr533x_hal_comp.h
- hal_deinit() : gr533x_hal.h
- hal_deinit_ext() : gr533x_hal_br.h
- hal_delay() : gr533x_hal.h
- hal_dma_abort() : gr533x_hal_dma.h
- hal_dma_abort_it() : gr533x_hal_dma.h
- hal_dma_deinit() : gr533x_hal_dma.h
- hal_dma_get_error() : gr533x_hal_dma.h
- hal_dma_get_state() : gr533x_hal_dma.h
- hal_dma_init() : gr533x_hal_dma.h
- hal_dma_irq_handler() : gr533x_hal_dma.h
- hal_dma_poll_for_transfer() : gr533x_hal_dma.h
- hal_dma_register_callback() : gr533x_hal_dma.h
- hal_dma_resume_channel() : gr533x_hal_dma.h
- hal_dma_resume_reg() : gr533x_hal_dma.h
- hal_dma_start() : gr533x_hal_dma.h
- hal_dma_start_it() : gr533x_hal_dma.h
- hal_dma_start_it_dc() : gr533x_hal_dma.h
- hal_dma_start_it_lock() : gr533x_hal_dma.h
- hal_dma_start_lock() : gr533x_hal_dma.h
- hal_dma_suspend_channel() : gr533x_hal_dma.h
- hal_dma_suspend_reg() : gr533x_hal_dma.h
- hal_dma_unregister_callback() : gr533x_hal_dma.h
- hal_dual_timer_act_period_event_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_act_start_event_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_act_stop_event_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_base_deinit() : gr533x_hal_dual_tim.h
- hal_dual_timer_base_deinit_ext() : gr533x_hal_br.h
- hal_dual_timer_base_init() : gr533x_hal_dual_tim.h
- hal_dual_timer_base_init_ext() : gr533x_hal_br.h
- hal_dual_timer_base_msp_deinit() : gr533x_hal_dual_tim.h
- hal_dual_timer_base_msp_init() : gr533x_hal_dual_tim.h
- hal_dual_timer_base_start() : gr533x_hal_dual_tim.h
- hal_dual_timer_base_start_it() : gr533x_hal_dual_tim.h
- hal_dual_timer_base_stop() : gr533x_hal_dual_tim.h
- hal_dual_timer_base_stop_it() : gr533x_hal_dual_tim.h
- hal_dual_timer_ble_pulse1_event_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_ble_pulse2_event_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_get_counter_value() : gr533x_hal_dual_tim.h
- hal_dual_timer_get_state() : gr533x_hal_dual_tim.h
- hal_dual_timer_io_crtl_config() : gr533x_hal_dual_tim.h
- hal_dual_timer_ioa_act_c1_event_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_ioa_act_c2_event_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_iob_act_c1_event_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_iob_act_c2_event_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_ioc_act_c1_event_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_ioc_act_c2_event_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_irq_handler() : gr533x_hal_dual_tim.h
- hal_dual_timer_period_elapsed_callback() : gr533x_hal_dual_tim.h
- hal_dual_timer_register_callback() : gr533x_hal_br.h
- hal_dual_timer_set_background_reload() : gr533x_hal_dual_tim.h
- hal_dual_timer_set_config() : gr533x_hal_dual_tim.h
- hal_dual_timer_set_onetime_reload() : gr533x_hal_dual_tim.h
- hal_dual_timer_set_period_count() : gr533x_hal_dual_tim.h
- hal_dual_timer_set_reload_background_reload() : gr533x_hal_dual_tim.h
- hal_dwt_disable() : gr533x_hal.h
- hal_dwt_enable() : gr533x_hal.h
- hal_efuse_deinit() : gr533x_hal_efuse.h
- hal_efuse_deinit_ext() : gr533x_hal_br.h
- hal_efuse_init() : gr533x_hal_efuse.h
- hal_efuse_init_ext() : gr533x_hal_br.h
- hal_efuse_initial_value_check() : gr533x_hal_efuse.h
- hal_efuse_msp_deinit() : gr533x_hal_efuse.h
- hal_efuse_msp_init() : gr533x_hal_efuse.h
- hal_efuse_read() : gr533x_hal_efuse.h
- hal_efuse_register_callback() : gr533x_hal_br.h
- hal_efuse_write() : gr533x_hal_efuse.h
- hal_exflash_block_protect() : gr533x_hal_exflash.h
- hal_exflash_config() : gr533x_hal_exflash.h
- hal_exflash_deepsleep() : gr533x_hal_exflash.h
- hal_exflash_enable_quad() : gr533x_hal_exflash.h
- hal_exflash_erase() : gr533x_hal_exflash.h
- hal_exflash_get_info() : gr533x_hal_exflash.h
- hal_exflash_init() : gr533x_hal_exflash.h
- hal_exflash_read() : gr533x_hal_exflash.h
- hal_exflash_read_status_reg() : gr533x_hal_exflash.h
- hal_exflash_read_uid() : gr533x_hal_exflash.h
- hal_exflash_sr_erase() : gr533x_hal_exflash.h
- hal_exflash_sr_program() : gr533x_hal_exflash.h
- hal_exflash_sr_protect() : gr533x_hal_exflash.h
- hal_exflash_sr_read() : gr533x_hal_exflash.h
- hal_exflash_timing_set() : gr533x_hal_exflash.h
- hal_exflash_wakeup() : gr533x_hal_exflash.h
- hal_exflash_write() : gr533x_hal_exflash.h
- hal_exflash_write_status_reg() : gr533x_hal_exflash.h
- hal_get_hal_version() : gr533x_hal.h , hal.h
- hal_get_tick() : gr533x_hal.h
- hal_gpio_deinit() : gr533x_hal_gpio.h
- hal_gpio_deinit_ext() : gr533x_hal_br.h
- hal_gpio_exti_callback() : gr533x_hal_gpio.h
- hal_gpio_exti_irq_handler() : gr533x_hal_gpio.h
- hal_gpio_init() : gr533x_hal_gpio.h
- hal_gpio_init_ext() : gr533x_hal_br.h
- hal_gpio_read_pin() : gr533x_hal_gpio.h
- hal_gpio_register_callback() : gr533x_hal_br.h
- hal_gpio_toggle_pin() : gr533x_hal_gpio.h
- hal_gpio_write_pin() : gr533x_hal_gpio.h
- hal_i2c_abort_cplt_callback() : gr533x_hal_i2c.h
- hal_i2c_deinit() : gr533x_hal_i2c.h
- hal_i2c_deinit_ext() : gr533x_hal_br.h
- hal_i2c_error_callback() : gr533x_hal_i2c.h
- hal_i2c_get_error() : gr533x_hal_i2c.h
- hal_i2c_get_mode() : gr533x_hal_i2c.h
- hal_i2c_get_state() : gr533x_hal_i2c.h
- hal_i2c_init() : gr533x_hal_i2c.h
- hal_i2c_init_ext() : gr533x_hal_br.h
- hal_i2c_irq_handler() : gr533x_hal_i2c.h
- hal_i2c_master_abort_it() : gr533x_hal_i2c.h
- hal_i2c_master_receive() : gr533x_hal_i2c.h
- hal_i2c_master_receive_dma() : gr533x_hal_i2c.h
- hal_i2c_master_receive_it() : gr533x_hal_i2c.h
- hal_i2c_master_rx_cplt_callback() : gr533x_hal_i2c.h
- hal_i2c_master_transmit() : gr533x_hal_i2c.h
- hal_i2c_master_transmit_dma() : gr533x_hal_i2c.h
- hal_i2c_master_transmit_it() : gr533x_hal_i2c.h
- hal_i2c_master_tx_cplt_callback() : gr533x_hal_i2c.h
- hal_i2c_mem_read() : gr533x_hal_i2c.h
- hal_i2c_mem_read_dma() : gr533x_hal_i2c.h
- hal_i2c_mem_read_it() : gr533x_hal_i2c.h
- hal_i2c_mem_write() : gr533x_hal_i2c.h
- hal_i2c_mem_write_dma() : gr533x_hal_i2c.h
- hal_i2c_mem_write_it() : gr533x_hal_i2c.h
- hal_i2c_msp_deinit() : gr533x_hal_i2c.h
- hal_i2c_msp_init() : gr533x_hal_i2c.h
- hal_i2c_register_callback() : gr533x_hal_br.h
- hal_i2c_resume_reg() : gr533x_hal_i2c.h
- hal_i2c_sda_at_low_is_not_recovered() : gr533x_hal_i2c.h
- hal_i2c_slave_receive() : gr533x_hal_i2c.h
- hal_i2c_slave_receive_dma() : gr533x_hal_i2c.h
- hal_i2c_slave_receive_it() : gr533x_hal_i2c.h
- hal_i2c_slave_rx_cplt_callback() : gr533x_hal_i2c.h
- hal_i2c_slave_transmit() : gr533x_hal_i2c.h
- hal_i2c_slave_transmit_dma() : gr533x_hal_i2c.h
- hal_i2c_slave_transmit_it() : gr533x_hal_i2c.h
- hal_i2c_slave_tx_cplt_callback() : gr533x_hal_i2c.h
- hal_i2c_speed_config() : gr533x_hal_i2c.h
- hal_i2c_suspend_reg() : gr533x_hal_i2c.h
- hal_increment_tick() : gr533x_hal.h
- hal_init() : gr533x_hal.h
- hal_init_ext() : gr533x_hal_br.h
- hal_is_rng_force_clk_enable() : gr533x_hal_rng.h
- hal_is_rng_wfi_clk_enable() : gr533x_hal_rng.h
- hal_msio_deinit() : gr533x_hal_msio.h
- hal_msio_deinit_ext() : gr533x_hal_br.h
- hal_msio_exti_callback() : gr533x_hal_msio.h
- hal_msio_exti_irq_handler() : gr533x_hal_msio.h
- hal_msio_init() : gr533x_hal_msio.h
- hal_msio_init_ext() : gr533x_hal_br.h
- hal_msio_read_pin() : gr533x_hal_msio.h
- hal_msio_register_callback() : gr533x_hal_br.h
- hal_msio_toggle_pin() : gr533x_hal_msio.h
- hal_msio_write_pin() : gr533x_hal_msio.h
- hal_msp_deinit() : gr533x_hal.h
- hal_msp_init() : gr533x_hal.h
- hal_nvic_clear_pending_irq() : gr533x_hal_cortex.h
- hal_nvic_disable_irq() : gr533x_hal_cortex.h
- hal_nvic_enable_irq() : gr533x_hal_cortex.h
- hal_nvic_get_active() : gr533x_hal_cortex.h
- hal_nvic_get_pending_irq() : gr533x_hal_cortex.h
- hal_nvic_get_priority() : gr533x_hal_cortex.h
- hal_nvic_get_priority_grouping() : gr533x_hal_cortex.h
- hal_nvic_set_pending_irq() : gr533x_hal_cortex.h
- hal_nvic_set_priority() : gr533x_hal_cortex.h
- hal_nvic_set_priority_grouping() : gr533x_hal_cortex.h
- hal_nvic_system_reset() : gr533x_hal_cortex.h
- hal_pwm_config_channel() : gr533x_hal_pwm.h
- hal_pwm_deinit() : gr533x_hal_pwm.h
- hal_pwm_deinit_ext() : gr533x_hal_br.h
- hal_pwm_get_state() : gr533x_hal_pwm.h
- hal_pwm_inactive_channel() : gr533x_hal_pwm.h
- hal_pwm_init() : gr533x_hal_pwm.h
- hal_pwm_init_ext() : gr533x_hal_br.h
- hal_pwm_irq_handler() : gr533x_hal_pwm.h
- hal_pwm_msp_deinit() : gr533x_hal_pwm.h
- hal_pwm_msp_init() : gr533x_hal_pwm.h
- hal_pwm_pause() : gr533x_hal_pwm.h
- hal_pwm_register_callback() : gr533x_hal_br.h
- hal_pwm_resume() : gr533x_hal_pwm.h
- hal_pwm_resume_reg() : gr533x_hal_pwm.h
- hal_pwm_set_coding_data_in_one_channel() : gr533x_hal_pwm.h
- hal_pwm_set_coding_data_in_three_channels() : gr533x_hal_pwm.h
- hal_pwm_start() : gr533x_hal_pwm.h
- hal_pwm_start_coding_in_one_channel() : gr533x_hal_pwm.h
- hal_pwm_start_coding_in_three_channels() : gr533x_hal_pwm.h
- hal_pwm_start_coding_with_dma() : gr533x_hal_pwm.h
- hal_pwm_stop() : gr533x_hal_pwm.h
- hal_pwm_suspend_reg() : gr533x_hal_pwm.h
- hal_pwm_update_freq() : gr533x_hal_pwm.h
- hal_pwr_config_timer_wakeup_ext() : gr533x_hal_br.h
- hal_pwr_enter_chip_deepsleep() : gr533x_hal_pwr.h
- hal_pwr_get_timer_current_value() : gr533x_hal_pwr.h
- hal_pwr_mgmt_clear_device_handle() : gr533x_hal_pwr_mgmt.h
- hal_pwr_mgmt_clear_device_sleep_flag() : gr533x_hal_pwr_mgmt.h
- hal_pwr_mgmt_device_resume_register() : gr533x_hal_pwr_mgmt.h
- hal_pwr_mgmt_device_resume_release() : gr533x_hal_pwr_mgmt.h
- hal_pwr_mgmt_device_suspend_register() : gr533x_hal_pwr_mgmt.h
- hal_pwr_mgmt_device_suspend_release() : gr533x_hal_pwr_mgmt.h
- hal_pwr_mgmt_save_device_handle() : gr533x_hal_pwr_mgmt.h
- hal_pwr_mgmt_set_device_renew_flag() : gr533x_hal_pwr_mgmt.h
- hal_pwr_mgmt_set_device_state() : gr533x_hal_pwr_mgmt.h
- hal_pwr_register_timer_elaspsed_handler() : gr533x_hal_br.h
- hal_pwr_sleep_timer_elapsed_callback() : gr533x_hal_sleep_timer.h
- hal_pwr_sleep_timer_irq_handler() : gr533x_hal_sleep_timer.h
- hal_register_callback() : gr533x_hal_br.h
- hal_resume_tick() : gr533x_hal.h
- hal_rng_clk_recover() : gr533x_hal_rng.h
- hal_rng_deinit() : gr533x_hal_rng.h
- hal_rng_deinit_ext() : gr533x_hal_br.h
- hal_rng_generate_random_number() : gr533x_hal_rng.h
- hal_rng_generate_random_number_it() : gr533x_hal_rng.h
- hal_rng_get_state() : gr533x_hal_rng.h
- hal_rng_init() : gr533x_hal_rng.h
- hal_rng_init_ext() : gr533x_hal_br.h
- hal_rng_irq_handler() : gr533x_hal_rng.h
- hal_rng_msp_deinit() : gr533x_hal_rng.h
- hal_rng_msp_init() : gr533x_hal_rng.h
- hal_rng_read_last_random_number() : gr533x_hal_rng.h
- hal_rng_ready_data_callback() : gr533x_hal_rng.h
- hal_rng_register_callback() : gr533x_hal_br.h
- hal_rng_resume_reg() : gr533x_hal_rng.h
- hal_rng_suspend_reg() : gr533x_hal_rng.h
- hal_rtc_alarm_callback() : gr533x_hal_rtc.h
- hal_rtc_clear_wrap() : gr533x_hal_rtc.h
- hal_rtc_deinit() : gr533x_hal_rtc.h
- hal_rtc_get_alarm_value() : gr533x_hal_rtc.h
- hal_rtc_get_cur_count() : gr533x_hal_rtc.h
- hal_rtc_get_cur_tick() : gr533x_hal_rtc.h
- hal_rtc_get_state() : gr533x_hal_rtc.h
- hal_rtc_get_wrap_count() : gr533x_hal_rtc.h
- hal_rtc_init() : gr533x_hal_rtc.h
- hal_rtc_irq_handler() : gr533x_hal_rtc.h
- hal_rtc_overflow_callback() : gr533x_hal_rtc.h
- hal_rtc_restart_tick() : gr533x_hal_rtc.h
- hal_rtc_set_alarm() : gr533x_hal_rtc.h
- hal_rtc_set_tick_and_start() : gr533x_hal_rtc.h
- hal_rtc_stop_alarm() : gr533x_hal_rtc.h
- hal_rtc_stop_tick() : gr533x_hal_rtc.h
- hal_rtc_tick_callback() : gr533x_hal_rtc.h
- hal_sleep_timer_config_and_start() : gr533x_hal_sleep_timer.h
- hal_sleep_timer_get_clock_freq() : gr533x_hal_sleep_timer.h
- hal_sleep_timer_get_current_value() : gr533x_hal_sleep_timer.h
- hal_sleep_timer_get_reload_value() : gr533x_hal_sleep_timer.h
- hal_sleep_timer_status_get() : gr533x_hal_sleep_timer.h
- hal_sleep_timer_stop() : gr533x_hal_sleep_timer.h
- hal_spi_abort() : gr533x_hal_spi.h
- hal_spi_abort_cplt_callback() : gr533x_hal_spi.h
- hal_spi_abort_it() : gr533x_hal_spi.h
- hal_spi_deinit() : gr533x_hal_spi.h
- hal_spi_deinit_ext() : gr533x_hal_br.h
- hal_spi_error_callback() : gr533x_hal_spi.h
- hal_spi_get_error() : gr533x_hal_spi.h
- hal_spi_get_rx_fifo_threshold() : gr533x_hal_spi.h
- hal_spi_get_state() : gr533x_hal_spi.h
- hal_spi_get_tx_fifo_threshold() : gr533x_hal_spi.h
- hal_spi_init() : gr533x_hal_spi.h
- hal_spi_init_ext() : gr533x_hal_br.h
- hal_spi_irq_handler() : gr533x_hal_spi.h
- hal_spi_msp_deinit() : gr533x_hal_spi.h
- hal_spi_msp_init() : gr533x_hal_spi.h
- hal_spi_read_eeprom() : gr533x_hal_spi.h
- hal_spi_read_eeprom_dma() : gr533x_hal_spi.h
- hal_spi_read_eeprom_it() : gr533x_hal_spi.h
- hal_spi_receive() : gr533x_hal_spi.h
- hal_spi_receive_dma() : gr533x_hal_spi.h
- hal_spi_receive_it() : gr533x_hal_spi.h
- hal_spi_register_callback() : gr533x_hal_br.h
- hal_spi_resume_reg() : gr533x_hal_spi.h
- hal_spi_rx_cplt_callback() : gr533x_hal_spi.h
- hal_spi_set_rx_fifo_threshold() : gr533x_hal_spi.h
- hal_spi_set_timeout() : gr533x_hal_spi.h
- hal_spi_set_tx_fifo_threshold() : gr533x_hal_spi.h
- hal_spi_soft_cs_assert() : gr533x_hal_spi.h
- hal_spi_soft_cs_deassert() : gr533x_hal_spi.h
- hal_spi_suspend_reg() : gr533x_hal_spi.h
- hal_spi_transmit() : gr533x_hal_spi.h
- hal_spi_transmit_dma() : gr533x_hal_spi.h
- hal_spi_transmit_dma_with_ia() : gr533x_hal_spi.h
- hal_spi_transmit_dma_with_ia_32addr() : gr533x_hal_spi.h
- hal_spi_transmit_it() : gr533x_hal_spi.h
- hal_spi_transmit_receive() : gr533x_hal_spi.h
- hal_spi_transmit_receive_dma() : gr533x_hal_spi.h
- hal_spi_transmit_receive_it() : gr533x_hal_spi.h
- hal_spi_transmit_with_ia() : gr533x_hal_spi.h
- hal_spi_transmit_with_ia_32addr() : gr533x_hal_spi.h
- hal_spi_tx_cplt_callback() : gr533x_hal_spi.h
- hal_spi_tx_rx_cplt_callback() : gr533x_hal_spi.h
- hal_suspend_tick() : gr533x_hal.h
- hal_systick_callback() : gr533x_hal.h
- hal_systick_config() : gr533x_hal_cortex.h
- hal_systick_irq_handler() : gr533x_hal.h
- hal_timer_base_deinit_ext() : gr533x_hal_br.h
- hal_timer_base_init_ext() : gr533x_hal_br.h
- hal_timer_blepulse1_event_callback() : gr533x_hal_tim.h
- hal_timer_blepulse2_event_callback() : gr533x_hal_tim.h
- hal_timer_channel0_event_callback() : gr533x_hal_tim.h
- hal_timer_channel1_event_callback() : gr533x_hal_tim.h
- hal_timer_channel2_event_callback() : gr533x_hal_tim.h
- hal_timer_channel3_event_callback() : gr533x_hal_tim.h
- hal_timer_deinit() : gr533x_hal_tim.h
- hal_timer_get_channel0_val() : gr533x_hal_tim.h
- hal_timer_get_channel1_val() : gr533x_hal_tim.h
- hal_timer_get_channel2_val() : gr533x_hal_tim.h
- hal_timer_get_channel3_val() : gr533x_hal_tim.h
- hal_timer_get_state() : gr533x_hal_tim.h
- hal_timer_init() : gr533x_hal_tim.h
- hal_timer_irq_handler() : gr533x_hal_tim.h
- hal_timer_msp_deinit() : gr533x_hal_tim.h
- hal_timer_msp_init() : gr533x_hal_tim.h
- hal_timer_period_elapsed_callback() : gr533x_hal_tim.h
- hal_timer_register_callback() : gr533x_hal_br.h
- hal_timer_set_config() : gr533x_hal_tim.h
- hal_timer_start() : gr533x_hal_tim.h
- hal_timer_start_it() : gr533x_hal_tim.h
- hal_timer_stop() : gr533x_hal_tim.h
- hal_timer_stop_it() : gr533x_hal_tim.h
- hal_uart_abort() : gr533x_hal_uart.h
- hal_uart_abort_cplt_callback() : gr533x_hal_uart.h
- hal_uart_abort_it() : gr533x_hal_uart.h
- hal_uart_abort_receive() : gr533x_hal_uart.h
- hal_uart_abort_receive_it() : gr533x_hal_uart.h
- hal_uart_abort_rx_cplt_callback() : gr533x_hal_uart.h
- hal_uart_abort_transmit() : gr533x_hal_uart.h
- hal_uart_abort_transmit_it() : gr533x_hal_uart.h
- hal_uart_abort_tx_cplt_callback() : gr533x_hal_uart.h
- hal_uart_deinit() : gr533x_hal_uart.h
- hal_uart_deinit_ext() : gr533x_hal_br.h
- hal_uart_dma_pause() : gr533x_hal_uart.h
- hal_uart_dma_resume() : gr533x_hal_uart.h
- hal_uart_dma_stop() : gr533x_hal_uart.h
- hal_uart_error_callback() : gr533x_hal_uart.h
- hal_uart_get_error() : gr533x_hal_uart.h
- hal_uart_get_state() : gr533x_hal_uart.h
- hal_uart_init() : gr533x_hal_uart.h
- hal_uart_init_ext() : gr533x_hal_br.h
- hal_uart_irq_handler() : gr533x_hal_uart.h
- hal_uart_msp_deinit() : gr533x_hal_uart.h
- hal_uart_msp_init() : gr533x_hal_uart.h
- hal_uart_receive() : gr533x_hal_uart.h
- hal_uart_receive_dma() : gr533x_hal_uart.h
- hal_uart_receive_it() : gr533x_hal_uart.h
- hal_uart_register_callback() : gr533x_hal_br.h
- hal_uart_resume_reg() : gr533x_hal_uart.h
- hal_uart_rx_cplt_callback() : gr533x_hal_uart.h
- hal_uart_suspend_reg() : gr533x_hal_uart.h
- hal_uart_transmit() : gr533x_hal_uart.h
- hal_uart_transmit_dma() : gr533x_hal_uart.h
- hal_uart_transmit_it() : gr533x_hal_uart.h
- hal_uart_tx_cplt_callback() : gr533x_hal_uart.h
- hal_wdt_deinit() : gr533x_hal_wdt.h
- hal_wdt_deinit_ext() : gr533x_hal_br.h
- hal_wdt_init() : gr533x_hal_wdt.h
- hal_wdt_init_ext() : gr533x_hal_br.h
- hal_wdt_irq_handler() : gr533x_hal_wdt.h
- hal_wdt_msp_deinit() : gr533x_hal_wdt.h
- hal_wdt_msp_init() : gr533x_hal_wdt.h
- hal_wdt_period_elapsed_callback() : gr533x_hal_wdt.h
- hal_wdt_refresh() : gr533x_hal_wdt.h
- hal_wdt_register_callback() : gr533x_hal_br.h
- hal_xqspi_command_receive() : gr533x_hal_xqspi.h
- hal_xqspi_command_transmit() : gr533x_hal_xqspi.h
- hal_xqspi_deinit() : gr533x_hal_xqspi.h
- hal_xqspi_deinit_ext() : gr533x_hal_br.h
- hal_xqspi_get_error() : gr533x_hal_xqspi.h
- hal_xqspi_get_rx_fifo_threshold() : gr533x_hal_xqspi.h
- hal_xqspi_get_state() : gr533x_hal_xqspi.h
- hal_xqspi_get_tx_fifo_threshold() : gr533x_hal_xqspi.h
- hal_xqspi_init() : gr533x_hal_xqspi.h
- hal_xqspi_init_ext() : gr533x_hal_br.h
- hal_xqspi_msp_deinit() : gr533x_hal_xqspi.h
- hal_xqspi_msp_init() : gr533x_hal_xqspi.h
- hal_xqspi_receive() : gr533x_hal_xqspi.h
- hal_xqspi_register_callback() : gr533x_hal_br.h
- hal_xqspi_set_retry() : gr533x_hal_xqspi.h
- hal_xqspi_set_rx_fifo_threshold() : gr533x_hal_xqspi.h
- hal_xqspi_set_tx_fifo_threshold() : gr533x_hal_xqspi.h
- hal_xqspi_transmit() : gr533x_hal_xqspi.h
- hci_basic_cmd_cmp_evt_cfg_handler() : ble_msg.h
- hci_basic_cmd_cmp_evt_rl_cfg_handler() : ble_msg.h
- hci_cte_cmd_cmp_evt_handler() : ble_msg.h
- hci_le_adv_set_term_evt_handler() : ble_msg.h
- hci_le_ch_sel_algo_evt_handler() : ble_msg.h
- hci_le_cmd_cmp_evt_addr_handler() : ble_msg.h
- hci_le_cmd_cmp_evt_adv_handler() : ble_msg.h
- hci_le_cmd_cmp_evt_init_handler() : ble_msg.h
- hci_le_cmd_cmp_evt_list_handler() : ble_msg.h
- hci_le_cmd_cmp_evt_per_sync_handler() : ble_msg.h
- hci_le_cmd_cmp_evt_scan_handler() : ble_msg.h
- hci_le_con_iq_report_evt_handler() : ble_msg.h
- hci_le_con_update_cmp_evt_handler() : ble_msg.h
- hci_le_conless_iq_report_evt_handler() : ble_msg.h
- hci_le_data_len_chg_evt_handler() : ble_msg.h
- hci_le_enh_con_cmp_evt_handler() : ble_msg.h
- hci_le_ext_adv_report_evt_handler() : ble_msg.h
- hci_le_gen_dhkey_cmp_evt_handler() : ble_msg.h
- hci_le_gen_dhkey_v2_stat_evt_handler() : ble_msg.h
- hci_le_ltk_request_evt_handler() : ble_msg.h
- hci_le_per_adv_report_evt_handler() : ble_msg.h
- hci_le_per_adv_sync_est_evt_handler() : ble_msg.h
- hci_le_per_adv_sync_lost_evt_handler() : ble_msg.h
- hci_le_phy_upd_cmp_evt_handler() : ble_msg.h
- hci_le_ranging_cmp_evt_handler() : ble_msg.h
- hci_le_ranging_ind_evt_handler() : ble_msg.h
- hci_le_ranging_sample_report_evt_handler() : ble_msg.h
- hci_le_rd_local_p256_public_key_cmp_evt_handler() : ble_msg.h
- hci_le_rd_phy_cmd_cmp_evt_handler() : ble_msg.h
- hci_le_rd_rem_feats_cmp_evt_handler() : ble_msg.h
- hci_le_rem_con_param_req_evt_handler() : ble_msg.h
- hci_le_scan_timeout_evt_handler() : ble_msg.h
- hci_le_set_conless_cte_tx_en_cmd_cmp_handler() : ble_msg.h
- hci_le_set_conless_cte_tx_param_cmd_cmp_handler() : ble_msg.h
- hci_le_set_conless_iq_sampl_en_cmd_cmp_evt_list_handler() : ble_msg.h
- hci_le_set_data_len_cmd_cmp_evt_handler() : ble_msg.h
- hci_le_set_per_adv_rec_en_cmp_evt_handler() : ble_msg.h
- hci_nb_cmp_pkts_evt_handler() : ble_msg.h
- hci_rd_chnl_map_cmd_cmp_evt_handler() : ble_msg.h
- hci_rd_rssi_cmd_cmp_evt_handler() : ble_msg.h
- hids_boot_kb_in_rep_send() : hids.h
- hids_boot_mouse_in_rep_send() : hids.h
- hids_input_rep_send() : hids.h
- hids_service_init() : hids.h
- hids_service_start_handle_get() : hids.h
- hrrcps_ctrl_pt_rsp_send() : hrrcps.h
- hrrcps_service_init() : hrrcps.h
- hrs_c_ctrl_point_set() : hrs_c.h
- hrs_c_disc_srvc_start() : hrs_c.h
- hrs_c_heart_rate_meas_notify_set() : hrs_c.h
- hrs_c_sensor_loc_read() : hrs_c.h
- hrs_client_init() : hrs_c.h
- hrs_energy_update() : hrs.h
- hrs_heart_rate_measurement_send() : hrs.h
- hrs_rr_interval_add() : hrs.h
- hrs_sensor_contact_detected_update() : hrs.h
- hrs_sensor_contact_supported_set() : hrs.h
- hrs_sensor_location_set() : hrs.h
- hrs_service_init() : hrs.h
- hrs_service_start_handle_get() : hrs.h
- hts_measurement_interval_send() : hts.h
- hts_measurement_send() : hts.h
- hts_service_init() : hts.h