Public Attributes | List of all members
ble_gap_sugg_dflt_data_len_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Suggested default data length info. More...

`#include <ble_gapc.h>`

## Public Attributes
uint16_t | suggted_max_tx_octets
uint16_t | suggted_max_tx_time

## Detailed Description

Suggested default data length info.

Definition at line 359 of file ble_gapc.h.

## Member Data Documentation

## ◆ suggted_max_tx_octets

uint16_t ble_gap_sugg_dflt_data_len_t::suggted_max_tx_octets

The Host's suggested value for the Controller's maximum transmitted number of payload octets to be used for new connections. Range: 0x001B-0x00FB (all other values reserved for future use), default: 0x001B

Definition at line 361 of file ble_gapc.h.

## ◆ suggted_max_tx_time

uint16_t ble_gap_sugg_dflt_data_len_t::suggted_max_tx_time

The Host's suggested value for the Controller's maximum packet transmission time to be used for new connections. Range: 0x0148-0x4290 (all other values reserved for future use), default: 0x0148

Definition at line 363 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h