Macros
Get Flags Defines
Peripheral Driver » LL Driver » UART » Defines » UART Exported Constants

Flags definitions which can be used with LL_UART_ReadReg function. More...

## Macros
#define | LL_UART_LSR_OE UART_LSR_OE
#define | LL_UART_LSR_PE UART_LSR_PE
#define | LL_UART_LSR_FE UART_LSR_FE
#define | LL_UART_LSR_BI UART_LSR_BI
#define | LL_UART_LSR_THRE UART_LSR_THRE
#define | LL_UART_LSR_TEMT UART_LSR_TEMT
#define | LL_UART_LSR_RFE UART_LSR_RFE
#define | LL_UART_IIR_MS UART_IIR_IID_MS
#define | LL_UART_IIR_NIP UART_IIR_IID_NIP
#define | LL_UART_IIR_THRE UART_IIR_IID_THRE
#define | LL_UART_IIR_RDA UART_IIR_IID_RDA
#define | LL_UART_IIR_RLS UART_IIR_IID_RLS
#define | LL_UART_IIR_CTO UART_IIR_IID_CTO
#define | LL_UART_USR_RFF UART_USR_RFF
#define | LL_UART_USR_RFNE UART_USR_RFNE
#define | LL_UART_USR_TFE UART_USR_TFE
#define | LL_UART_USR_TFNF UART_USR_TFNF

## Detailed Description

Flags definitions which can be used with LL_UART_ReadReg function.

## Macro Definition Documentation

## ◆ LL_UART_IIR_CTO

#define LL_UART_IIR_CTO UART_IIR_IID_CTO

Character Timeout flag

Definition at line 136 of file gr533x_ll_uart.h.

## ◆ LL_UART_IIR_MS

#define LL_UART_IIR_MS UART_IIR_IID_MS

Modem Status flag

Definition at line 131 of file gr533x_ll_uart.h.

## ◆ LL_UART_IIR_NIP

#define LL_UART_IIR_NIP UART_IIR_IID_NIP

No Interrupt Pending flag

Definition at line 132 of file gr533x_ll_uart.h.

## ◆ LL_UART_IIR_RDA

#define LL_UART_IIR_RDA UART_IIR_IID_RDA

Received Data Available flag

Definition at line 134 of file gr533x_ll_uart.h.

## ◆ LL_UART_IIR_RLS

#define LL_UART_IIR_RLS UART_IIR_IID_RLS

Receiver Line Status flag

Definition at line 135 of file gr533x_ll_uart.h.

## ◆ LL_UART_IIR_THRE

#define LL_UART_IIR_THRE UART_IIR_IID_THRE

THR Empty flag

Definition at line 133 of file gr533x_ll_uart.h.

## ◆ LL_UART_LSR_BI

#define LL_UART_LSR_BI UART_LSR_BI

Break detection flag

Definition at line 126 of file gr533x_ll_uart.h.

## ◆ LL_UART_LSR_FE

#define LL_UART_LSR_FE UART_LSR_FE

Framing error flag

Definition at line 125 of file gr533x_ll_uart.h.

## ◆ LL_UART_LSR_OE

#define LL_UART_LSR_OE UART_LSR_OE

Overrun error flag

Definition at line 123 of file gr533x_ll_uart.h.

## ◆ LL_UART_LSR_PE

#define LL_UART_LSR_PE UART_LSR_PE

Parity error flag

Definition at line 124 of file gr533x_ll_uart.h.

## ◆ LL_UART_LSR_RFE

#define LL_UART_LSR_RFE UART_LSR_RFE

Rx FIFO error flag

Definition at line 129 of file gr533x_ll_uart.h.

## ◆ LL_UART_LSR_TEMT

#define LL_UART_LSR_TEMT UART_LSR_TEMT

Transmitter empty flag

Definition at line 128 of file gr533x_ll_uart.h.

## ◆ LL_UART_LSR_THRE

#define LL_UART_LSR_THRE UART_LSR_THRE

Transmit holding register empty flag

Definition at line 127 of file gr533x_ll_uart.h.

## ◆ LL_UART_USR_RFF

#define LL_UART_USR_RFF UART_USR_RFF

Rx FIFO Full flag

Definition at line 138 of file gr533x_ll_uart.h.

## ◆ LL_UART_USR_RFNE

#define LL_UART_USR_RFNE UART_USR_RFNE

Rx FIFO Not Empty flag

Definition at line 139 of file gr533x_ll_uart.h.

## ◆ LL_UART_USR_TFE

#define LL_UART_USR_TFE UART_USR_TFE

Tx FIFO Empty flag

Definition at line 140 of file gr533x_ll_uart.h.

## ◆ LL_UART_USR_TFNF

#define LL_UART_USR_TFNF UART_USR_TFNF

Tx FIFO Not Full flag

Definition at line 141 of file gr533x_ll_uart.h.