Public Attributes | List of all members
ble_gap_dft_subrate_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Default Subrate command param. More...

`#include <ble_gapc.h>`

## Public Attributes
uint16_t | subrate_min
uint16_t | subrate_max
uint16_t | max_latency
uint16_t | continuation_num
uint16_t | superv_timeout

## Detailed Description

Default Subrate command param.

Definition at line 800 of file ble_gapc.h.

## Member Data Documentation

## ◆ continuation_num

uint16_t ble_gap_dft_subrate_param_t::continuation_num

Minimum number of underlying connection events to remain active.

Definition at line 805 of file ble_gapc.h.

## ◆ max_latency

uint16_t ble_gap_dft_subrate_param_t::max_latency

Maximum Peripheral latency allowed in requests by a Peripheral.

Definition at line 804 of file ble_gapc.h.

## ◆ subrate_max

uint16_t ble_gap_dft_subrate_param_t::subrate_max

Maximum subrate factor allowed in requests by a Peripheral(Range: 0x0001 - 0x01F4, Default: 0x0001).

Definition at line 803 of file ble_gapc.h.

## ◆ subrate_min

uint16_t ble_gap_dft_subrate_param_t::subrate_min

Minimum subrate factor allowed in requests by a Peripheral(Range: 0x0001 - 0x01F4, Default: 0x0001).

Definition at line 802 of file ble_gapc.h.

## ◆ superv_timeout

uint16_t ble_gap_dft_subrate_param_t::superv_timeout

Maximum supervision timeout allowed in requests by a Peripheral.

Definition at line 806 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h