Here is a list of all file members with links to the files they belong to:

### - r -

- RANDOM : ble_iso.h
- ras_ad_attr_idx_t : ras_ad.h
- RAS_AD_CP_MAX_LEN : ras_ad.h
- RAS_AD_DATA_MAX_LEN : ras_ad.h
- RAS_AD_DATA_OW_MAX_LEN : ras_ad.h
- RAS_AD_DATA_READY_MAX_LEN : ras_ad.h
- ras_ad_evt_handler_t : ras_ad.h
- RAS_AD_EVT_INVALID : ras_ad.h
- RAS_AD_EVT_SEND_NTI_IND_CMP : ras_ad.h
- RAS_AD_EVT_SET_CP_CCCD : ras_ad.h
- RAS_AD_EVT_SET_DATA_OW_CCCD : ras_ad.h
- RAS_AD_EVT_SET_DATA_READY_CCCD : ras_ad.h
- RAS_AD_EVT_SET_OD_DATA_CCCD : ras_ad.h
- RAS_AD_EVT_SET_RT_DATA_CCCD : ras_ad.h
- ras_ad_evt_type_t : ras_ad.h
- RAS_AD_EVT_WRITE_CP : ras_ad.h
- RAS_AD_FEA_MAX_LEN : ras_ad.h
- RAS_AD_IDX_CP_CCCD_CFG : ras_ad.h
- RAS_AD_IDX_CP_CHAR : ras_ad.h
- RAS_AD_IDX_CP_VAL : ras_ad.h
- RAS_AD_IDX_DATA_OW_CCCD_CFG : ras_ad.h
- RAS_AD_IDX_DATA_OW_CHAR : ras_ad.h
- RAS_AD_IDX_DATA_OW_VAL : ras_ad.h
- RAS_AD_IDX_DATA_READY_CCCD_CFG : ras_ad.h
- RAS_AD_IDX_DATA_READY_CHAR : ras_ad.h
- RAS_AD_IDX_DATA_READY_VAL : ras_ad.h
- RAS_AD_IDX_FEA_CHAR : ras_ad.h
- RAS_AD_IDX_FEA_VAL : ras_ad.h
- RAS_AD_IDX_NB : ras_ad.h
- RAS_AD_IDX_OD_DATA_CCCD_CFG : ras_ad.h
- RAS_AD_IDX_OD_DATA_CHAR : ras_ad.h
- RAS_AD_IDX_OD_DATA_VAL : ras_ad.h
- RAS_AD_IDX_RT_DATA_CCCD_CFG : ras_ad.h
- RAS_AD_IDX_RT_DATA_CHAR : ras_ad.h
- RAS_AD_IDX_RT_DATA_VAL : ras_ad.h
- RAS_AD_IDX_SVC : ras_ad.h
- ras_ad_init() : ras_ad.h
- RAS_AD_SEND_DATA_TYPE_INDICATE : ras_ad.h
- RAS_AD_SEND_DATA_TYPE_INVALID : ras_ad.h
- RAS_AD_SEND_DATA_TYPE_NOTIFY : ras_ad.h
- ras_ad_send_data_type_t : ras_ad.h
- ras_ad_send_noti_ind() : ras_ad.h
- RAS_ANT_PATH_BIT_MASK : ras_common.h
- RAS_ANTENNA_PATH_1_MASK : ras_common.h
- RAS_ANTENNA_PATH_2_MASK : ras_common.h
- RAS_ANTENNA_PATH_3_MASK : ras_common.h
- RAS_ANTENNA_PATH_4_MASK : ras_common.h
- RAS_C_AD_CHAR_HANDLE_CCCD_NB : ras_c_ad.h
- ras_c_ad_char_type_t : ras_c_ad.h
- ras_c_ad_disconnect_handler() : ras_c_ad.h
- RAS_C_AD_EVT_DISCOVER_COMPLETED : ras_c_ad.h
- RAS_C_AD_EVT_DISCOVER_FAILED : ras_c_ad.h
- ras_c_ad_evt_handler_t : ras_c_ad.h
- RAS_C_AD_EVT_INVALID : ras_c_ad.h
- RAS_C_AD_EVT_READ_RSP : ras_c_ad.h
- RAS_C_AD_EVT_SERVER_IND : ras_c_ad.h
- RAS_C_AD_EVT_SERVER_NOTIFY : ras_c_ad.h
- ras_c_ad_evt_type_t : ras_c_ad.h
- RAS_C_AD_EVT_WRITE_ERR : ras_c_ad.h
- RAS_C_AD_EVT_WRITE_RSP : ras_c_ad.h
- RAS_C_AD_HANDLE_ON_DEMAND_RA_DATA : ras_c_ad.h
- RAS_C_AD_HANDLE_ON_DEMAND_RA_DATA_IND_NTF_CFG : ras_c_ad.h
- RAS_C_AD_HANDLE_RA_DATA_OVERWRITE : ras_c_ad.h
- RAS_C_AD_HANDLE_RA_DATA_OVERWRITE_IND_NTF_CFG : ras_c_ad.h
- RAS_C_AD_HANDLE_RA_DATA_READY : ras_c_ad.h
- RAS_C_AD_HANDLE_RA_DATA_READY_IND_NTF_CFG : ras_c_ad.h
- RAS_C_AD_HANDLE_RAS_CP : ras_c_ad.h
- RAS_C_AD_HANDLE_RAS_CP_IND_NTF_CFG : ras_c_ad.h
- RAS_C_AD_HANDLE_RAS_FEATURES : ras_c_ad.h
- RAS_C_AD_HANDLE_RT_RA_DATA : ras_c_ad.h
- RAS_C_AD_HANDLE_RT_RA_DATA_IND_NTF_CFG : ras_c_ad.h
- ras_c_ad_init() : ras_c_ad.h
- ras_c_ad_read_char() : ras_c_ad.h
- ras_c_ad_start_discov_srvc() : ras_c_ad.h
- ras_c_ad_write_char() : ras_c_ad.h
- ras_c_cccd_value_type_t : ras_c.h
- ras_c_char_cccd_set() : ras_c.h
- ras_c_connect_handler() : ras_c.h
- RAS_C_DIS_NTF_IND : ras_c.h
- ras_c_disconnect_handler() : ras_c.h
- ras_c_discov_srvc_start() : ras_c.h
- RAS_C_EN_IND : ras_c.h
- RAS_C_EN_NTF : ras_c.h
- RAS_C_EN_NTF_IND : ras_c.h
- RAS_C_EVT_DISCOVER_COMPLETED : ras_c.h
- RAS_C_EVT_DISCOVER_FAILED : ras_c.h
- ras_c_evt_handler_t : ras_c.h
- RAS_C_EVT_INVALID : ras_c.h
- RAS_C_EVT_READ_RSP : ras_c.h
- RAS_C_EVT_SUBEVT_REPORT : ras_c.h
- ras_c_evt_type_t : ras_c.h
- RAS_C_EVT_WRITE_ERR : ras_c.h
- RAS_C_EVT_WRITE_RSP : ras_c.h
- ras_c_filter_policy_set() : ras_c.h
- ras_c_init() : ras_c.h
- ras_c_mtu_exch_handler() : ras_c.h
- ras_c_operation_abort() : ras_c.h
- RAS_C_READ_ON_DEMAND_RA_DATA_IND_NTF_CFG : ras_c.h
- RAS_C_READ_RA_DATA_OVERWRITE_IND_NTF_CFG : ras_c.h
- RAS_C_READ_RA_DATA_READY_IND_NTF_CFG : ras_c.h
- RAS_C_READ_RAS_CP_IND_NTF_CFG : ras_c.h
- RAS_C_READ_RAS_FEATURE : ras_c.h
- RAS_C_READ_RT_RA_DATA_IND_NTF_CFG : ras_c.h
- RAS_C_READ_TYPE_INVALID : ras_c.h
- ras_c_read_type_t : ras_c.h
- ras_c_set_remote_step_data_len() : ras_c.h
- RAS_C_WRITE_ON_DEMAND_RA_DATA_IND_NTF_CFG : ras_c.h
- RAS_C_WRITE_RA_DATA_OVERWRITE_IND_NTF_CFG : ras_c.h
- RAS_C_WRITE_RA_DATA_READY_IND_NTF_CFG : ras_c.h
- RAS_C_WRITE_RAS_CP : ras_c.h
- RAS_C_WRITE_RAS_CP_IND_NTF_CFG : ras_c.h
- RAS_C_WRITE_RT_RA_DATA_IND_NTF_CFG : ras_c.h
- RAS_C_WRITE_TYPE_INVALID : ras_c.h
- ras_c_write_type_t : ras_c.h
- RAS_CACHE_PROC_NUM : ras.h
- RAS_CCCD_LEN : ras_common.h
- RAS_CFG_ID_BIT_MASK : ras_common.h
- ras_connect_handler() : ras.h
- RAS_CONNECTION_MAX : ras_common.h
- RAS_CTRL_PT_CHAR_MAX_LEN : ras_common.h
- ras_ctrl_pt_cmd_opd_t : ras_common.h
- RAS_CTRL_PT_OPCODE_LEN : ras_common.h
- RAS_CTRL_PT_OPCODE_OFFSET : ras_common.h
- RAS_CTRL_PT_OPERAND_MAX_LEN : ras_common.h
- RAS_CTRL_PT_OPERAND_OFFSET : ras_common.h
- ras_ctrl_pt_rsp_opd_t : ras_common.h
- ras_disconnect_handler() : ras.h
- RAS_ERROR_PROC_ALREADY_IN_PROGRESS : ras_common.h
- RAS_FEA_ABORT_OPERATION_BIT_MASK : ras_common.h
- RAS_FEA_ALL_BIT_MASK : ras_common.h
- ras_fea_bit_mask_t : ras_common.h
- RAS_FEA_FILTER_RA_DATA_BIT_MASK : ras_common.h
- RAS_FEA_RETR_LOST_RA_DATA_SEG_BIT_MASK : ras_common.h
- RAS_FEA_RL_RA_DATA_BIT_MASK : ras_common.h
- RAS_FEATURE_CHAR_LEN : ras_common.h
- RAS_LOG_INFO : ras_common.h
- RAS_MAX_PROC_NUM_PER_LINK : ras_common.h
- RAS_MODE0_DATA_BIT_MASK : ras_common.h
- ras_mode0_data_bit_t : ras_common.h
- RAS_MODE1_DATA_BIT_MASK : ras_common.h
- ras_mode1_data_bit_t : ras_common.h
- RAS_MODE2_DATA_BIT_MASK : ras_common.h
- ras_mode2_data_bit_t : ras_common.h
- RAS_MODE3_DATA_BIT_MASK : ras_common.h
- ras_mode3_data_bit_t : ras_common.h
- RAS_MODE_0 : ras_common.h
- RAS_MODE_1 : ras_common.h
- RAS_MODE_2 : ras_common.h
- RAS_MODE_3 : ras_common.h
- RAS_MODE_NUM : ras_common.h
- RAS_MODE_TYPE_BIT_MASK : ras_common.h
- RAS_MODE_TYPE_BIT_OFFSET : ras_common.h
- ras_mode_type_t : ras_common.h
- ras_mtu_exch_handler() : ras.h
- RAS_OP_ABORT_OPERATION : ras_common.h
- RAS_OP_ACK_RA_DATA : ras_common.h
- RAS_OP_CMP_LOST_RA_DATA_SEG_RSP : ras_common.h
- RAS_OP_CMP_RA_DATA_RSP : ras_common.h
- RAS_OP_FILTER : ras_common.h
- RAS_OP_GET_RA_DATA : ras_common.h
- RAS_OP_RETR_LOST_RA_DATA_SEGMENTS : ras_common.h
- RAS_OP_RSP_CODE : ras_common.h
- RAS_PCT_FORMAT_BIT_MASK : ras_common.h
- RAS_PCT_FORMAT_MASK : ras_common.h
- ras_proc_disabled_handler() : ras.h
- RAS_RANGING_COUNTER_BIT_MASK : ras_common.h
- RAS_RANGING_HEADER_LEN : ras_common.h
- ras_rcv_subevt_data_handler() : ras.h
- RAS_ROLLING_SEGMENT_COUNTER_MAX : ras_common.h
- RAS_ROLLING_SEGMENT_COUNTER_MIN : ras_common.h
- RAS_RSP_ABORT_UNSUCCESSFUL : ras_common.h
- ras_rsp_code_val_t : ras_common.h
- RAS_RSP_INVALID_PARAM : ras_common.h
- RAS_RSP_NO_RECORDS_FOUND : ras_common.h
- RAS_RSP_OPCODE_NOT_SUPPORTED : ras_common.h
- RAS_RSP_PARAM_NOT_SUPPORTED : ras_common.h
- RAS_RSP_PROCEDURE_NOT_COMPLETED : ras_common.h
- RAS_RSP_SERVER_BUSY : ras_common.h
- RAS_RSP_SUCCESS : ras_common.h
- RAS_SEGMENT_HEADER_FIRST_SEG_BITMASK : ras_common.h
- RAS_SEGMENT_HEADER_LAST_SEG_BITMASK : ras_common.h
- RAS_SEGMENT_HEADER_LEN : ras_common.h
- RAS_SEGMENT_HEADER_ROLL_SEG_COUNT_BITMASK : ras_common.h
- ras_service_init() : ras.h
- ras_set_cache_data_info() : ras.h
- RAS_SUBEVENT_HEADER_FREQ_COMPENSATION_OFFSET : ras_common.h
- RAS_SUBEVENT_HEADER_LEN : ras_common.h
- RAS_SUBEVENT_HEADER_NUM_STEPS_REPORTED_OFFSET : ras_common.h
- RAS_SUBEVENT_HEADER_RANGING_DONE_STATUS_OFFSET : ras_common.h
- RAS_SUBEVENT_HEADER_REF_POWER_LEVEL_OFFSET : ras_common.h
- RAS_SUBEVENT_HEADER_START_ACL_CON_EVENT_OFFSET : ras_common.h
- RAS_SUBEVENT_HEADER_SUBEVENT_DONE_STATUS_OFFSET : ras_common.h
- ras_subevt_data_t : ras_common.h
- raw_log_send_cb_t : gr533x_sys_sdk.h
- RC_OSC_CLK : platform_sdk.h
- READ_CFG0_CFG : gr533x_ll_rtc.h
- reference_time_encode() : cts.h
- restore_sys_context() : gr533x_sys_sdk.h
- rng_handle_t : gr533x_hal_rng.h
- rng_init_t : gr533x_hal_rng.h
- RNG_LFSR_MODE_128BIT : gr533x_hal_rng.h
- RNG_LFSR_MODE_59BIT : gr533x_hal_rng.h
- RNG_OUTPUT_CYCLIC : gr533x_hal_rng.h
- RNG_OUTPUT_CYCLIC_PARITY : gr533x_hal_rng.h
- RNG_OUTPUT_FR0_S0 : gr533x_hal_rng.h
- RNG_OUTPUT_LFSR : gr533x_hal_rng.h
- RNG_OUTPUT_LFSR_RNG : gr533x_hal_rng.h
- RNG_POST_PRO_COUNTING : gr533x_hal_rng.h
- RNG_POST_PRO_NEUMANN : gr533x_hal_rng.h
- RNG_POST_PRO_NOT : gr533x_hal_rng.h
- RNG_POST_PRO_SKIPPING : gr533x_hal_rng.h
- RNG_PWR_ID : app_pwr_mgmt.h
- RNG_SEED_FR0_S0 : gr533x_hal_rng.h
- RNG_SEED_USER : gr533x_hal_rng.h
- RSCS_C_CONNECTION_MAX : rscs_c.h
- rscs_c_ctrl_pt_indicate_set() : rscs_c.h
- rscs_c_ctrl_pt_op_code_t : rscs_c.h
- RSCS_C_CTRL_PT_OP_REQ_SUP_LOC : rscs_c.h
- RSCS_C_CTRL_PT_OP_RESERVED : rscs_c.h
- RSCS_C_CTRL_PT_OP_RSP_CODE : rscs_c.h
- RSCS_C_CTRL_PT_OP_SET_CUMUL_VAL : rscs_c.h
- RSCS_C_CTRL_PT_OP_START_CALIB : rscs_c.h
- RSCS_C_CTRL_PT_OP_UPD_LOC : rscs_c.h
- RSCS_C_CTRL_PT_RSP_FAILED : rscs_c.h
- RSCS_C_CTRL_PT_RSP_INVALID_PARAM : rscs_c.h
- RSCS_C_CTRL_PT_RSP_NOT_SUP : rscs_c.h
- RSCS_C_CTRL_PT_RSP_RESERVED : rscs_c.h
- RSCS_C_CTRL_PT_RSP_SUCCESS : rscs_c.h
- rscs_c_ctrl_pt_rsp_t : rscs_c.h
- rscs_c_ctrl_pt_set() : rscs_c.h
- rscs_c_disc_srvc_start() : rscs_c.h
- RSCS_C_ERROR_CCCD_INVALID : rscs_c.h
- RSCS_C_ERROR_PROC_IN_PROGRESS : rscs_c.h
- RSCS_C_EVT_CTRL_PT_IND_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_CTRL_PT_RSP_RECEIVE : rscs_c.h
- RSCS_C_EVT_CTRL_PT_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_DISCOVERY_COMPLETE : rscs_c.h
- RSCS_C_EVT_DISCOVERY_FAIL : rscs_c.h
- rscs_c_evt_handler_t : rscs_c.h
- RSCS_C_EVT_INVALID : rscs_c.h
- RSCS_C_EVT_RSC_FEATURE_RECEIVE : rscs_c.h
- RSCS_C_EVT_RSC_MEAS_NTF_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_RSC_MEAS_VAL_RECEIVE : rscs_c.h
- RSCS_C_EVT_SENSOR_LOC_RECEIVE : rscs_c.h
- rscs_c_evt_type_t : rscs_c.h
- RSCS_C_EVT_WRITE_OP_ERR : rscs_c.h
- RSCS_C_FEAT_CALIBRATION_PROCEDURE_BIT : rscs_c.h
- RSCS_C_FEAT_INSTANT_STRIDE_LEN_BIT : rscs_c.h
- RSCS_C_FEAT_MULTIPLE_SENSORS_BIT : rscs_c.h
- RSCS_C_FEAT_RUNNING_OR_WALKING_STATUS_BIT : rscs_c.h
- RSCS_C_FEAT_TOTAL_DISTANCE_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_INST_STRIDE_LEN_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_RUNNING_OR_WALKING_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_TOTAL_DISTANCE_BIT : rscs_c.h
- RSCS_C_PT_RSP_LEN_MAX : rscs_c.h
- rscs_c_rsc_feature_read() : rscs_c.h
- rscs_c_rsc_meas_notify_set() : rscs_c.h
- RSCS_C_SENSOR_LOC_FRONT_HUB : rscs_c.h
- RSCS_C_SENSOR_LOC_FRONT_WHEEL : rscs_c.h
- RSCS_C_SENSOR_LOC_HIP : rscs_c.h
- RSCS_C_SENSOR_LOC_LEFT_PEDAL : rscs_c.h
- RSCS_C_SENSOR_LOC_OTHER : rscs_c.h
- rscs_c_sensor_loc_read() : rscs_c.h
- RSCS_C_SENSOR_LOC_RIGHT_PEDAL : rscs_c.h
- RSCS_C_SENSOR_LOC_SHOE_IN : rscs_c.h
- RSCS_C_SENSOR_LOC_SHOE_TOP : rscs_c.h
- RSCS_C_SENSOR_LOC_SUP_NB : rscs_c.h
- rscs_c_sensor_loc_t : rscs_c.h
- RSCS_CHAR_FULL : rscs.h
- RSCS_CHAR_MANDATORY : rscs.h
- RSCS_CHAR_SC_CTRL_POINT : rscs.h
- RSCS_CHAR_SENSOR_LOC_SUP : rscs.h
- rscs_client_init() : rscs_c.h
- RSCS_CONNECTION_MAX : rscs.h
- rscs_ctrl_pt_op_code_t : rscs.h
- RSCS_CTRL_PT_OP_REQ_SUP_LOC : rscs.h
- RSCS_CTRL_PT_OP_RESERVED : rscs.h
- RSCS_CTRL_PT_OP_RSP_CODE : rscs.h
- RSCS_CTRL_PT_OP_SET_CUMUL_VAL : rscs.h
- RSCS_CTRL_PT_OP_START_CALIB : rscs.h
- RSCS_CTRL_PT_OP_UPD_LOC : rscs.h
- RSCS_CTRL_PT_RSP_FAILED : rscs.h
- RSCS_CTRL_PT_RSP_INVALID_PARAM : rscs.h
- RSCS_CTRL_PT_RSP_LEN_MIN : rscs.h
- RSCS_CTRL_PT_RSP_NOT_SUP : rscs.h
- RSCS_CTRL_PT_RSP_RESERVED : rscs.h
- rscs_ctrl_pt_rsp_send() : rscs.h
- RSCS_CTRL_PT_RSP_SUCCESS : rscs.h
- rscs_ctrl_pt_rsp_t : rscs.h
- RSCS_CTRL_PT_VAL_LEN_MAX : rscs.h
- RSCS_ERROR_CCCD_INVALID : rscs.h
- RSCS_ERROR_PROC_IN_PROGRESS : rscs.h
- RSCS_EVT_CTRL_POINT_INDICATION_DISABLE : rscs.h
- RSCS_EVT_CTRL_POINT_INDICATION_ENABLE : rscs.h
- RSCS_EVT_CTRL_POINT_RSP_CPLT : rscs.h
- RSCS_EVT_CUMUL_VAL_SET : rscs.h
- rscs_evt_handler_t : rscs.h
- RSCS_EVT_INVALID : rscs.h
- RSCS_EVT_RSC_MEAS_NOTIFICATION_DISABLE : rscs.h
- RSCS_EVT_RSC_MEAS_NOTIFICATION_ENABLE : rscs.h
- RSCS_EVT_RSC_MEAS_SEND_CPLT : rscs.h
- RSCS_EVT_SEBSOR_CALIBRATION : rscs.h
- RSCS_EVT_SEBSOR_LOC_UPD : rscs.h
- RSCS_EVT_SUP_SEBSOR_LOC_REQ : rscs.h
- rscs_evt_type_t : rscs.h
- RSCS_FEAR_FULL_BIT : rscs.h
- RSCS_FEAT_CALIBRATION_PROCEDURE_BIT : rscs.h
- RSCS_FEAT_INSTANT_STRIDE_LEN_BIT : rscs.h
- RSCS_FEAT_MULTIPLE_SENSORS_BIT : rscs.h
- RSCS_FEAT_RUNNING_OR_WALKING_STATUS_BIT : rscs.h
- RSCS_FEAT_TOTAL_DISTANCE_BIT : rscs.h
- RSCS_FEAT_VAL_LEN_MAX : rscs.h
- RSCS_MEAS_FLAG_INST_STRIDE_LEN_BIT : rscs.h
- RSCS_MEAS_FLAG_RUNNING_OR_WALKING_BIT : rscs.h
- RSCS_MEAS_FLAG_TOTAL_DISTANCE_BIT : rscs.h
- RSCS_MEAS_VAL_LEN_MAX : rscs.h
- rscs_measurement_send() : rscs.h
- RSCS_SENSOR_LOC_FRONT_HUB : rscs.h
- RSCS_SENSOR_LOC_FRONT_WHEEL : rscs.h
- RSCS_SENSOR_LOC_HIP : rscs.h
- RSCS_SENSOR_LOC_LEFT_PEDAL : rscs.h
- RSCS_SENSOR_LOC_OTHER : rscs.h
- RSCS_SENSOR_LOC_RIGHT_PEDAL : rscs.h
- RSCS_SENSOR_LOC_SHOE_IN : rscs.h
- RSCS_SENSOR_LOC_SHOE_TOP : rscs.h
- RSCS_SENSOR_LOC_SUP_NB : rscs.h
- rscs_sensor_loc_t : rscs.h
- rscs_sensor_loc_update() : rscs.h
- RSCS_SENSOR_LOC_VAL_LEN_MAX : rscs.h
- rscs_service_init() : rscs.h
- rtc_alarm_state_t : gr533x_hal_rtc.h
- RTC_DIV_128 : gr533x_hal_rtc.h
- RTC_DIV_16 : gr533x_hal_rtc.h
- RTC_DIV_2 : gr533x_hal_rtc.h
- RTC_DIV_32 : gr533x_hal_rtc.h
- RTC_DIV_4 : gr533x_hal_rtc.h
- RTC_DIV_64 : gr533x_hal_rtc.h
- RTC_DIV_8 : gr533x_hal_rtc.h
- RTC_DIV_NONE : gr533x_hal_rtc.h
- RTC_FLAG_ALARM : gr533x_hal_rtc.h
- RTC_FLAG_TICK : gr533x_hal_rtc.h
- RTC_FLAG_WRAP : gr533x_hal_rtc.h
- rtc_handle_t : gr533x_hal_rtc.h
- rtc_init_t : gr533x_hal_rtc.h
- RTC_IT_ALARM : gr533x_hal_rtc.h
- RTC_IT_TICK : gr533x_hal_rtc.h
- RTC_IT_WRAP : gr533x_hal_rtc.h
- RTC_OSC_CLK : platform_sdk.h
- rtc_tick_state_t : gr533x_hal_rtc.h
- RTUS_CHAR_FULL : rtus.h
- RTUS_CONNECTION_MAX : rtus.h
- RTUS_CTRL_PT_CANCEL_UPDATE : rtus.h
- RTUS_CTRL_PT_GET_UPDATE : rtus.h
- rtus_ctrl_pt_t : rtus.h
- RTUS_CTRL_PT_VAL_LEN : rtus.h
- RTUS_CUR_STATE_IDLE : rtus.h
- RTUS_CUR_STATE_PENDING : rtus.h
- rtus_cur_state_t : rtus.h
- rtus_current_state_set() : rtus.h
- RTUS_EVT_CANCEL_UPDATE : rtus.h
- RTUS_EVT_GET_UPDATE : rtus.h
- rtus_evt_handler_t : rtus.h
- RTUS_EVT_INVALID : rtus.h
- rtus_evt_type_t : rtus.h
- rtus_service_init() : rtus.h
- RTUS_UPDATE_RESULT_CANCELED : rtus.h
- RTUS_UPDATE_RESULT_NO_ATTEMPTED : rtus.h
- RTUS_UPDATE_RESULT_NO_CONN_TO_REF : rtus.h
- RTUS_UPDATE_RESULT_REP_ERROR : rtus.h
- RTUS_UPDATE_RESULT_SCCESSFUL : rtus.h
- rtus_update_result_set() : rtus.h
- rtus_update_result_t : rtus.h
- RTUS_UPDATE_RESULT_TIMEOUT : rtus.h
- RTUS_UPDATE_STATE_VAL_LEN : rtus.h
- rx_done_cb_t : ble_lcp.h
- rx_handler_cb_t : ble_lcp.h