### - f -

- fast_ldo_prep : boot_timing_params_t
- fat_free_mass : bcs_meas_val_t
- fat_free_mass_present : bcs_meas_flag_t
- feature : __attribute__ , bcs_init_t , bms_init_t , cgms_init_t , cscs_init_t , gls_init_t , rscs_init_t , wss_init_t
- feature_report : hids_init_t
- feature_report_sup : hids_init_t
- features : ble_gap_peer_features_ind_t
- filter : gls_racp_req_t
- filter_param : cgms_racp_req_t , ras_ctr_pt_operation_t
- filter_pol : ble_gap_adv_param_t , ble_gap_ext_adv_param_t
- filter_type : cgms_racp_req_t
- first_name_present : uds_chars_flag_t
- flag : ams_c_attr_info_t , wechat_pedo_meas_t , wechat_pedo_target_t
- flags : ble_gap_evt_remote_tx_pwr_read_ind_t , ble_gap_evt_tx_pwr_change_report_t , ble_gap_remote_tx_pwr_read_ind_t , ble_gap_tx_pwr_change_report_t , cgms_meas_rec_t , gls_meas_ctx_t , gls_meas_val_t , hids_hid_info_t
- flash : __attribute__
- flash_manufacturer : __attribute__
- flash_otp_addr1 : __attribute__
- flash_otp_addr2 : __attribute__
- flash_size : __attribute__
- flash_tDP : __attribute__ , _exflash_timing_param
- flash_tERS : __attribute__ , _exflash_timing_param
- flash_tESL : __attribute__ , _exflash_timing_param
- flash_tPRS : __attribute__ , _exflash_timing_param
- flash_tPSL : __attribute__ , _exflash_timing_param
- flash_tRDINT : __attribute__ , _exflash_timing_param
- flash_tRES2 : __attribute__ , _exflash_timing_param
- flash_tVSL : __attribute__ , _exflash_timing_param
- flickerstop_lvl : _ll_pwm_none_coding_channel_init_t
- force_clk : _cgc_init
- format : prf_char_pres_fmt_t
- fractions_256 : cts_c_exact_time_256_t , cts_exact_time_256_t
- frame_buf : dfu_buf_table_t
- frame_size : dfu_buf_table_t
- framing : iso_big_info_report_evt_t , iso_create_big_t , iso_set_cig_param_t
- freq : pwm_none_coding_init_t
- freq_mhz : gdx_lcp_config_t
- fstoplvl : pwm_none_coding_channel_init_t
- ft_m2s : iso_cis_est_evt_t
- ft_s2m : iso_cis_est_evt_t
- fw_rev_str : dis_init_t