Macros
AON_GPIO mode
Peripheral Driver » HAL Driver » AON_GPIO » Defines » AON_GPIO Exported Constants

AON_GPIO Configuration Mode Elements values convention: 0x000000YX. More...

## Macros
#define | AON_GPIO_MODE_NONE (LL_AON_GPIO_MODE_NONE)
#define | AON_GPIO_MODE_INPUT (LL_AON_GPIO_MODE_INPUT)
#define | AON_GPIO_MODE_OUTPUT (LL_AON_GPIO_MODE_OUTPUT)
#define | AON_GPIO_MODE_INOUT (LL_AON_GPIO_MODE_INOUT)
#define | AON_GPIO_MODE_MUX (LL_AON_GPIO_MODE_INOUT)
#define | AON_GPIO_MODE_IT_RISING (LL_AON_GPIO_TRIGGER_RISING << 4 | AON_GPIO_MODE_INPUT)
#define | AON_GPIO_MODE_IT_FALLING (LL_AON_GPIO_TRIGGER_FALLING << 4 | AON_GPIO_MODE_INPUT)
#define | AON_GPIO_MODE_IT_HIGH (LL_AON_GPIO_TRIGGER_HIGH << 4 | AON_GPIO_MODE_INPUT)
#define | AON_GPIO_MODE_IT_LOW (LL_AON_GPIO_TRIGGER_LOW << 4 | AON_GPIO_MODE_INPUT)
#define | AON_GPIO_MODE_IT_BOTH_EDGE (LL_AON_GPIO_TRIGGER_BOTH_EDGE << 4 | AON_GPIO_MODE_INPUT)

## Detailed Description

AON_GPIO Configuration Mode Elements values convention: 0x000000YX.

- X : IO Direction mode (Input, Output, Mux)
- Y : IT trigger detection

## Macro Definition Documentation

## ◆ AON_GPIO_MODE_INOUT

#define AON_GPIO_MODE_INOUT (LL_AON_GPIO_MODE_INOUT)

Input andoutput Mode

Definition at line 169 of file hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_INPUT

#define AON_GPIO_MODE_INPUT (LL_AON_GPIO_MODE_INPUT)

Input Mode

Definition at line 167 of file hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_IT_BOTH_EDGE

#define AON_GPIO_MODE_IT_BOTH_EDGE (LL_AON_GPIO_TRIGGER_BOTH_EDGE << 4 | AON_GPIO_MODE_INPUT)

Interrupt Mode with Rising and Falling edge trigger detection

Definition at line 175 of file hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_IT_FALLING

#define AON_GPIO_MODE_IT_FALLING (LL_AON_GPIO_TRIGGER_FALLING << 4 | AON_GPIO_MODE_INPUT)

Interrupt Mode with Falling edge trigger detection

Definition at line 172 of file hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_IT_HIGH

#define AON_GPIO_MODE_IT_HIGH (LL_AON_GPIO_TRIGGER_HIGH << 4 | AON_GPIO_MODE_INPUT)

Interrupt Mode with High-level trigger detection

Definition at line 173 of file hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_IT_LOW

#define AON_GPIO_MODE_IT_LOW (LL_AON_GPIO_TRIGGER_LOW << 4 | AON_GPIO_MODE_INPUT)

Interrupt Mode with Low-level trigger detection

Definition at line 174 of file hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_IT_RISING

#define AON_GPIO_MODE_IT_RISING (LL_AON_GPIO_TRIGGER_RISING << 4 | AON_GPIO_MODE_INPUT)

Interrupt Mode with Rising edge trigger detection

Definition at line 171 of file hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_MUX

#define AON_GPIO_MODE_MUX (LL_AON_GPIO_MODE_INOUT)

Mux Mode

Definition at line 170 of file hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_NONE

#define AON_GPIO_MODE_NONE (LL_AON_GPIO_MODE_NONE)

Disable input and output

Definition at line 166 of file hal_aon_gpio.h.

## ◆ AON_GPIO_MODE_OUTPUT

#define AON_GPIO_MODE_OUTPUT (LL_AON_GPIO_MODE_OUTPUT)

Output Mode

Definition at line 168 of file hal_aon_gpio.h.