Here is a list of all file members with links to the files they belong to:

### - x -

- XIP_16M : platform_sdk.h
- XIP_24M : platform_sdk.h
- XIP_32M : platform_sdk.h
- XIP_48M : platform_sdk.h
- XIP_64M : platform_sdk.h
- XIP_XO16M : platform_sdk.h
- XO_REQUEST_DEVICE_NUM_BLE : hal_clock.h
- XO_REQUEST_DEVICE_NUM_CALIBRATION : hal_clock.h
- XO_REQUEST_DEVICE_NUM_DCDC : hal_clock.h
- XO_REQUEST_DEVICE_NUM_DDVS : hal_clock.h
- XO_REQUEST_DEVICE_NUM_USER : hal_clock.h
- xo_request_device_number_t : hal_clock.h
- XQSPI_ADDRSIZE_00_BITS : hal_xqspi.h
- XQSPI_ADDRSIZE_08_BITS : hal_xqspi.h
- XQSPI_ADDRSIZE_16_BITS : hal_xqspi.h
- XQSPI_ADDRSIZE_24_BITS : hal_xqspi.h
- XQSPI_ADDRSIZE_32_BITS : hal_xqspi.h
- XQSPI_BAUD_RATE_16M : hal_xqspi.h
- XQSPI_BAUD_RATE_24M : hal_xqspi.h
- XQSPI_BAUD_RATE_32M : hal_xqspi.h
- XQSPI_BAUD_RATE_48M : hal_xqspi.h
- XQSPI_BAUD_RATE_64M : hal_xqspi.h
- XQSPI_CACHE_DIRECT_MAP_DIS : hal_xqspi.h
- XQSPI_CACHE_DIRECT_MAP_EN : hal_xqspi.h
- XQSPI_CACHE_FLUSH_DIS : hal_xqspi.h
- XQSPI_CACHE_FLUSH_EN : hal_xqspi.h
- XQSPI_CACHE_MODE_DIS : hal_xqspi.h
- XQSPI_CACHE_MODE_EN : hal_xqspi.h
- XQSPI_CLOCK_MODE_0 : hal_xqspi.h
- XQSPI_CLOCK_MODE_1 : hal_xqspi.h
- XQSPI_CLOCK_MODE_2 : hal_xqspi.h
- XQSPI_CLOCK_MODE_3 : hal_xqspi.h
- xqspi_command_t : hal_xqspi.h
- XQSPI_DATA_MODE_DUALSPI : hal_xqspi.h
- XQSPI_DATA_MODE_QUADSPI : hal_xqspi.h
- XQSPI_DATA_MODE_SPI : hal_xqspi.h
- XQSPI_DISABLE_PRESENT : hal_xqspi.h
- XQSPI_ENABLE_PRESENT : hal_xqspi.h
- XQSPI_FIFO_DEPTH : hal_xqspi.h
- XQSPI_FIFO_THRESHOLD_1_2 : hal_xqspi.h
- XQSPI_FIFO_THRESHOLD_1_4 : hal_xqspi.h
- XQSPI_FIFO_THRESHOLD_1_8 : hal_xqspi.h
- XQSPI_FIFO_THRESHOLD_3_4 : hal_xqspi.h
- XQSPI_FLAG_BUSY : hal_xqspi.h
- XQSPI_FLAG_RFE : hal_xqspi.h
- XQSPI_FLAG_RFF : hal_xqspi.h
- XQSPI_FLAG_RFTF : hal_xqspi.h
- XQSPI_FLAG_TFE : hal_xqspi.h
- XQSPI_FLAG_TFF : hal_xqspi.h
- XQSPI_FLAG_TFTF : hal_xqspi.h
- xqspi_handle_t : hal_xqspi.h
- XQSPI_HP_MODE_DIS : hal_xqspi.h
- XQSPI_HP_MODE_EN : hal_xqspi.h
- xqspi_init_t : hal_xqspi.h
- XQSPI_INST_ADDR_ALL_IN_SPI : hal_xqspi.h
- XQSPI_INST_ADDR_ALL_IN_SPIFRF : hal_xqspi.h
- XQSPI_INST_IN_SPI_ADDR_IN_SPIFRF : hal_xqspi.h
- XQSPI_INSTSIZE_00_BITS : hal_xqspi.h
- XQSPI_INSTSIZE_08_BITS : hal_xqspi.h
- XQSPI_INSTSIZE_16_BITS : hal_xqspi.h
- XQSPI_READ_CMD_DUAL_IO_READ : hal_xqspi.h
- XQSPI_READ_CMD_DUAL_OUT_READ : hal_xqspi.h
- XQSPI_READ_CMD_FAST_READ : hal_xqspi.h
- XQSPI_READ_CMD_QUAD_IO_READ : hal_xqspi.h
- XQSPI_READ_CMD_QUAD_OUT_READ : hal_xqspi.h
- XQSPI_READ_CMD_READ : hal_xqspi.h
- XQSPI_WORK_MODE_QSPI : hal_xqspi.h
- XQSPI_WORK_MODE_XIP : hal_xqspi.h