Macros
ADC Input Channel Select
Peripheral Driver » HAL Driver » ADC » Defines » ADC Exported Constants

## Macros
#define | ADC_INPUT_SRC_IO0 LL_ADC_INPUT_SRC_IO0
#define | ADC_INPUT_SRC_IO1 LL_ADC_INPUT_SRC_IO1
#define | ADC_INPUT_SRC_IO2 LL_ADC_INPUT_SRC_IO2
#define | ADC_INPUT_SRC_IO3 LL_ADC_INPUT_SRC_IO3
#define | ADC_INPUT_SRC_IO4 LL_ADC_INPUT_SRC_IO4
#define | ADC_INPUT_SRC_IO5 LL_ADC_INPUT_SRC_IO5
#define | ADC_INPUT_SRC_IO6 LL_ADC_INPUT_SRC_IO6
#define | ADC_INPUT_SRC_IO7 LL_ADC_INPUT_SRC_IO7
#define | ADC_INPUT_SRC_TMP LL_ADC_INPUT_SRC_TMP
#define | ADC_INPUT_SRC_BAT LL_ADC_INPUT_SRC_BAT
#define | ADC_INPUT_SRC_REF LL_ADC_INPUT_SRC_REF

## Detailed Description

## Macro Definition Documentation

## ◆ ADC_INPUT_SRC_BAT

#define ADC_INPUT_SRC_BAT LL_ADC_INPUT_SRC_BAT

Select Vbattery as input

Definition at line 221 of file hal_adc.h.

## ◆ ADC_INPUT_SRC_IO0

#define ADC_INPUT_SRC_IO0 LL_ADC_INPUT_SRC_IO0

Select MSIO0 as input

Definition at line 212 of file hal_adc.h.

## ◆ ADC_INPUT_SRC_IO1

#define ADC_INPUT_SRC_IO1 LL_ADC_INPUT_SRC_IO1

Select MSIO1 as input

Definition at line 213 of file hal_adc.h.

## ◆ ADC_INPUT_SRC_IO2

#define ADC_INPUT_SRC_IO2 LL_ADC_INPUT_SRC_IO2

Select MSIO2 as input

Definition at line 214 of file hal_adc.h.

## ◆ ADC_INPUT_SRC_IO3

#define ADC_INPUT_SRC_IO3 LL_ADC_INPUT_SRC_IO3

Select MSIO3 as input

Definition at line 215 of file hal_adc.h.

## ◆ ADC_INPUT_SRC_IO4

#define ADC_INPUT_SRC_IO4 LL_ADC_INPUT_SRC_IO4

Select MSIO4 as input

Definition at line 216 of file hal_adc.h.

## ◆ ADC_INPUT_SRC_IO5

#define ADC_INPUT_SRC_IO5 LL_ADC_INPUT_SRC_IO5

Select MSIO5 as input

Definition at line 217 of file hal_adc.h.

## ◆ ADC_INPUT_SRC_IO6

#define ADC_INPUT_SRC_IO6 LL_ADC_INPUT_SRC_IO6

Select MSIO6 as input

Definition at line 218 of file hal_adc.h.

## ◆ ADC_INPUT_SRC_IO7

#define ADC_INPUT_SRC_IO7 LL_ADC_INPUT_SRC_IO7

Select MSIO7 as input

Definition at line 219 of file hal_adc.h.

## ◆ ADC_INPUT_SRC_REF

#define ADC_INPUT_SRC_REF LL_ADC_INPUT_SRC_REF

Select reference as input

Definition at line 222 of file hal_adc.h.

## ◆ ADC_INPUT_SRC_TMP

#define ADC_INPUT_SRC_TMP LL_ADC_INPUT_SRC_TMP

Select temperature as input

Definition at line 220 of file hal_adc.h.