Macros
Mode defines
Peripheral Driver » LL Driver » LL Clock Calibration » Defines

## Macros
#define | LL_DDVS_RINGO_0_EN (1<<0U)
#define | LL_DDVS_RINGO_1_EN (1<<1U)
#define | LL_DDVS_RINGO_2_EN (1<<2U)
#define | LL_DDVS_RINGO_3_EN (1<<3U)
#define | LL_DDVS_RINGO_ALL_EN (0xFU)
#define | LL_DDVS_RINGO_ALL_DIS (0x0U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_DDVS_RINGO_0_EN

#define LL_DDVS_RINGO_0_EN (1<<0U)

DDVS Ringo_0 Enable

Definition at line 83 of file ll_ddvs.h.

## ◆ LL_DDVS_RINGO_1_EN

#define LL_DDVS_RINGO_1_EN (1<<1U)

DDVS Ringo_1 Enable

Definition at line 84 of file ll_ddvs.h.

## ◆ LL_DDVS_RINGO_2_EN

#define LL_DDVS_RINGO_2_EN (1<<2U)

DDVS Ringo_2 Enable

Definition at line 85 of file ll_ddvs.h.

## ◆ LL_DDVS_RINGO_3_EN

#define LL_DDVS_RINGO_3_EN (1<<3U)

DDVS Ringo_3 Enable

Definition at line 86 of file ll_ddvs.h.

## ◆ LL_DDVS_RINGO_ALL_DIS

#define LL_DDVS_RINGO_ALL_DIS (0x0U)

DDVS All Ringos Disable

Definition at line 88 of file ll_ddvs.h.

## ◆ LL_DDVS_RINGO_ALL_EN

#define LL_DDVS_RINGO_ALL_EN (0xFU)

DDVS All Ringos Enable

Definition at line 87 of file ll_ddvs.h.