Public Attributes | List of all members
ble_gap_set_conn_cte_rcv_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Set connection CTE receive parameters info. More...

`#include <ble_gapc.h>`

## Public Attributes
bool | sampling_enable
uint8_t | slot_durations
uint8_t | num_antenna
uint8_t * | antenna_id

## Detailed Description

Set connection CTE receive parameters info.

Definition at line 534 of file ble_gapc.h.

## Member Data Documentation

## ◆ antenna_id

uint8_t* ble_gap_set_conn_cte_rcv_param_t::antenna_id

List of Antenna IDs in the pattern.

Definition at line 539 of file ble_gapc.h.

## ◆ num_antenna

uint8_t ble_gap_set_conn_cte_rcv_param_t::num_antenna

The number of Antenna IDs in the pattern, range 0x02 to 0x4B.

Definition at line 538 of file ble_gapc.h.

## ◆ sampling_enable

bool ble_gap_set_conn_cte_rcv_param_t::sampling_enable

Wheter to sample IQ from the CTE.

Definition at line 536 of file ble_gapc.h.

## ◆ slot_durations

uint8_t ble_gap_set_conn_cte_rcv_param_t::slot_durations

The slot for sample IQ from the CTE, see ble_gap_switching_sampling_type_t.

Definition at line 537 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h