Macros
ADC Buffered Internal Reference Value
Peripheral Driver » LL Driver » ADC » Defines » ADC Exported Constants

## Macros
#define | LL_ADC_REF_VALUE_0P8 (0x3UL << AON_PMU_SNSADC_CFG_REF_VALUE_Pos)
#define | LL_ADC_REF_VALUE_1P2 (0x7UL << AON_PMU_SNSADC_CFG_REF_VALUE_Pos)
#define | LL_ADC_REF_VALUE_1P6 (0xAUL << AON_PMU_SNSADC_CFG_REF_VALUE_Pos)
#define | LL_ADC_REF_VALUE_2P0 (0xFUL << AON_PMU_SNSADC_CFG_REF_VALUE_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_ADC_REF_VALUE_0P8

#define LL_ADC_REF_VALUE_0P8 (0x3UL << AON_PMU_SNSADC_CFG_REF_VALUE_Pos)

Reference = 0.85 V

Definition at line 141 of file ll_adc.h.

## ◆ LL_ADC_REF_VALUE_1P2

#define LL_ADC_REF_VALUE_1P2 (0x7UL << AON_PMU_SNSADC_CFG_REF_VALUE_Pos)

Reference = 1.28 V

Definition at line 142 of file ll_adc.h.

## ◆ LL_ADC_REF_VALUE_1P6

#define LL_ADC_REF_VALUE_1P6 (0xAUL << AON_PMU_SNSADC_CFG_REF_VALUE_Pos)

Reference = 1.60 V

Definition at line 143 of file ll_adc.h.

## ◆ LL_ADC_REF_VALUE_2P0

#define LL_ADC_REF_VALUE_2P0 (0xFUL << AON_PMU_SNSADC_CFG_REF_VALUE_Pos)

Reference = 2.00 V

Definition at line 144 of file ll_adc.h.