Macros
Serial Protocol
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_SPI_PROTOCOL_MOTOROLA 0x00000000UL
#define | LL_SPI_PROTOCOL_TI (1UL << SPI_CTRL0_FRAME_FORMAT_POS)
#define | LL_SPI_PROTOCOL_MICROWIRE (2UL << SPI_CTRL0_FRAME_FORMAT_POS)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SPI_PROTOCOL_MICROWIRE

#define LL_SPI_PROTOCOL_MICROWIRE (2UL << SPI_CTRL0_FRAME_FORMAT_POS)

Microwire mode

Definition at line 286 of file ll_spi.h.

## ◆ LL_SPI_PROTOCOL_MOTOROLA

#define LL_SPI_PROTOCOL_MOTOROLA 0x00000000UL

Motorola mode. Used as default value

Definition at line 284 of file ll_spi.h.

## ◆ LL_SPI_PROTOCOL_TI

#define LL_SPI_PROTOCOL_TI (1UL << SPI_CTRL0_FRAME_FORMAT_POS)

TI mode

Definition at line 285 of file ll_spi.h.