Macros
InitStruct default configuartion
Peripheral Driver » LL Driver » AON_GPIO » Defines » AON_GPIO Private Macros

## Macros
#define | LL_AON_GPIO_DEFAULT_CONFIG
| LL AON_GPIO InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_AON_GPIO_DEFAULT_CONFIG

#define LL_AON_GPIO_DEFAULT_CONFIG

Value:
{ \
.pin = LL_AON_GPIO_PIN_ALL, \
.mode = LL_AON_GPIO_MODE_INPUT, \
.pull = LL_AON_GPIO_PULL_DOWN, \
.mux = IO_MUX_GPIO, \
.speed = LL_AON_GPIO_SPEED_MEDIUM, \
.strength = LL_AON_GPIO_STRENGTH_MEDIUM, \
.input_type = LL_AON_GPIO_INPUT_TYPE_CMOS, \
.trigger = LL_AON_GPIO_TRIGGER_NONE, \
}

LL AON_GPIO InitStrcut default configuartion.

Definition at line 262 of file ll_aon_gpio.h.

LL_AON_GPIO_PIN_ALL
#define LL_AON_GPIO_PIN_ALL
Definition: ll_aon_gpio.h:151
LL_AON_GPIO_TRIGGER_NONE
#define LL_AON_GPIO_TRIGGER_NONE
Definition: ll_aon_gpio.h:199
IO_MUX_GPIO
#define IO_MUX_GPIO
Definition: hal_gpio.h:179
LL_AON_GPIO_STRENGTH_MEDIUM
#define LL_AON_GPIO_STRENGTH_MEDIUM
Definition: ll_aon_gpio.h:184
LL_AON_GPIO_INPUT_TYPE_CMOS
#define LL_AON_GPIO_INPUT_TYPE_CMOS
Definition: ll_aon_gpio.h:192
LL_AON_GPIO_PULL_DOWN
#define LL_AON_GPIO_PULL_DOWN
Definition: ll_aon_gpio.h:169
LL_AON_GPIO_MODE_INPUT
#define LL_AON_GPIO_MODE_INPUT
Definition: ll_aon_gpio.h:158
LL_AON_GPIO_SPEED_MEDIUM
#define LL_AON_GPIO_SPEED_MEDIUM
Definition: ll_aon_gpio.h:176