Macros
DMA Peripheral type
Peripheral Driver » LL Driver » DMA » Defines » DMA Exported Constants

## Macros
#define | LL_DMA0_PERIPH_MEM ((uint32_t)0x0000000BU)
#define | LL_DMA0_PERIPH_CTE ((uint32_t)0x00000000U)
#define | LL_DMA0_PERIPH_PWM0 ((uint32_t)0x00000001U)
#define | LL_DMA0_PERIPH_SPIM_TX ((uint32_t)0x00000002U)
#define | LL_DMA0_PERIPH_SPIM_RX ((uint32_t)0x00000003U)
#define | LL_DMA0_PERIPH_SPIS_TX ((uint32_t)0x00000004U)
#define | LL_DMA0_PERIPH_SPIS_RX ((uint32_t)0x00000005U)
#define | LL_DMA0_PERIPH_UART0_TX ((uint32_t)0x00000006U)
#define | LL_DMA0_PERIPH_UART0_RX ((uint32_t)0x00000007U)
#define | LL_DMA0_PERIPH_UART1_TX ((uint32_t)0x00000008U)
#define | LL_DMA0_PERIPH_UART1_RX ((uint32_t)0x00000009U)
#define | LL_DMA0_PERIPH_SNSADC ((uint32_t)0x0000000AU)
#define | LL_DMA0_PERIPH_I2C0_TX ((uint32_t)0x0000000CU)
#define | LL_DMA0_PERIPH_I2C0_RX ((uint32_t)0x0000000DU)
#define | LL_DMA0_PERIPH_I2C1_TX ((uint32_t)0x0000000EU)
#define | LL_DMA0_PERIPH_I2C1_RX ((uint32_t)0x0000000FU)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_DMA0_PERIPH_CTE

#define LL_DMA0_PERIPH_CTE ((uint32_t)0x00000000U)

DMA Peripheral type is CTE

Definition at line 290 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_I2C0_RX

#define LL_DMA0_PERIPH_I2C0_RX ((uint32_t)0x0000000DU)

DMA peripheral type is I2C0 RX

Definition at line 302 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_I2C0_TX

#define LL_DMA0_PERIPH_I2C0_TX ((uint32_t)0x0000000CU)

DMA peripheral type is I2C0 TX

Definition at line 301 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_I2C1_RX

#define LL_DMA0_PERIPH_I2C1_RX ((uint32_t)0x0000000FU)

DMA peripheral type is I2C1 RX

Definition at line 304 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_I2C1_TX

#define LL_DMA0_PERIPH_I2C1_TX ((uint32_t)0x0000000EU)

DMA peripheral type is I2C1 TX

Definition at line 303 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_MEM

#define LL_DMA0_PERIPH_MEM ((uint32_t)0x0000000BU)

DMA peripheral type is Memory

Definition at line 287 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_PWM0

#define LL_DMA0_PERIPH_PWM0 ((uint32_t)0x00000001U)

DMA Peripheral type is PWM0

Definition at line 291 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_SNSADC

#define LL_DMA0_PERIPH_SNSADC ((uint32_t)0x0000000AU)

DMA peripheral type is SNSADC

Definition at line 300 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_SPIM_RX

#define LL_DMA0_PERIPH_SPIM_RX ((uint32_t)0x00000003U)

DMA Peripheral type is SPIM RX

Definition at line 293 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_SPIM_TX

#define LL_DMA0_PERIPH_SPIM_TX ((uint32_t)0x00000002U)

DMA Peripheral type is SPIM TX

Definition at line 292 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_SPIS_RX

#define LL_DMA0_PERIPH_SPIS_RX ((uint32_t)0x00000005U)

DMA Peripheral type is SPIS RX

Definition at line 295 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_SPIS_TX

#define LL_DMA0_PERIPH_SPIS_TX ((uint32_t)0x00000004U)

DMA Peripheral type is SPIS TX

Definition at line 294 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART0_RX

#define LL_DMA0_PERIPH_UART0_RX ((uint32_t)0x00000007U)

DMA Peripheral type is UART0 RX

Definition at line 297 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART0_TX

#define LL_DMA0_PERIPH_UART0_TX ((uint32_t)0x00000006U)

DMA Peripheral type is UART0 TX

Definition at line 296 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART1_RX

#define LL_DMA0_PERIPH_UART1_RX ((uint32_t)0x00000009U)

DMA Peripheral type is UART1 RX

Definition at line 299 of file ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART1_TX

#define LL_DMA0_PERIPH_UART1_TX ((uint32_t)0x00000008U)

DMA Peripheral type is UART1 TX

Definition at line 298 of file ll_dma.h.