Macros
QSPI Clock Phase
Peripheral Driver » LL Driver » Defines » XQSPI Exported Constants

## Macros
#define | LL_XQSPI_SCPHA_1EDGE 0
#define | LL_XQSPI_SCPHA_2EDGE 1

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_SCPHA_1EDGE

#define LL_XQSPI_SCPHA_1EDGE 0

First clock transition is the first data capture edge

Definition at line 296 of file ll_xqspi.h.

## ◆ LL_XQSPI_SCPHA_2EDGE

#define LL_XQSPI_SCPHA_2EDGE 1

Second clock transition is the first data capture edge

Definition at line 297 of file ll_xqspi.h.