Functions
Initialization and de-initialization functions
Peripheral Driver » LL Driver » AON_GPIO » Functions

## Functions
void | ll_aon_gpio_init (ll_aon_gpio_init_t const p_aon_gpio_init)
| Initialize AON_GPIO registers according to the specified. parameters in p_aon_gpio_init. More...

## Detailed Description

## Function Documentation

## ◆ ll_aon_gpio_init()

void ll_aon_gpio_init | ( | ll_aon_gpio_init_t const | p_aon_gpio_init | ) |

Initialize AON_GPIO registers according to the specified. parameters in p_aon_gpio_init.

Parameters

  p_aon_gpio_init | Pointer to a ll_aon_gpio_init_t structure that contains the configuration information for the specified AON_GPIO peripheral.

Return values

  None |