### - p -

- PASS_ALERT_STATUS_VAL_LEN : pass.h
- PASS_ALL_STATE_ACTIVE : pass.h
- PASS_C_ALL_STATE_ACTIVE : pass_c.h
- PASS_C_CONNECTION_MAX : pass_c.h
- PASS_C_DISPLAY_ALERT_ACTIVE : pass_c.h
- PASS_C_NO_STATE_ACTIVE : pass_c.h
- PASS_C_RINGER_ACTIVE : pass_c.h
- PASS_C_RINGER_CTRL_PT_VAL_LEN : pass_c.h
- PASS_C_RINGER_SET_NORMAL : pass_c.h
- PASS_C_RINGER_SET_SILENT : pass_c.h
- PASS_C_VIBRATE_ACTIVE : pass_c.h
- PASS_CHAR_FULL : pass.h
- PASS_CHAR_MANDATORY : pass.h
- PASS_CHAR_RING_CTRL_PT_SUP : pass.h
- PASS_CONNECTION_MAX : pass.h
- PASS_DISPLAY_ALERT_ACTIVE : pass.h
- PASS_NO_STATE_ACTIVE : pass.h
- PASS_RINGER_ACTIVE : pass.h
- PASS_RINGER_CTRL_PT_VAL_LEN : pass.h
- PASS_RINGER_SET_NORMAL : pass.h
- PASS_RINGER_SET_SILENT : pass.h
- PASS_RINGER_SET_VAL_LEN : pass.h
- PASS_VIBRATE_ACTIVE : pass.h
- PAWR_MAX_SENT_DATA_LEN : esls.h
- PAWR_SENT_DATA_LEN_OFFSET : esls.h
- PAWR_SENT_DATA_TYPE_OFFSET : esls.h
- PCS_CONNECTION_MAX : pcs.h
- PCS_MAX_DATA_LEN : pcs.h
- PCS_SERVICE_UUID : pcs.h
- PCS_SET_ADV_DATA_10B : pcs.h
- PCS_SET_ADV_DATA_17B : pcs.h
- PCS_SET_ADV_DATA_24B : pcs.h
- PCS_SET_ADV_DATA_31B : pcs.h
- PCS_SET_ADV_DATA_3B : pcs.h
- PCS_SET_PARAM_FAIL : pcs.h
- PCS_SET_PARAM_SUCCESS : pcs.h
- PKC_BIGMULTI_BITS_LENGTH_MAX : hal_pkc.h
- PKC_BITS_LENGTH_MAX : hal_pkc.h
- PKC_BITS_LENGTH_MIN : hal_pkc.h
- PKC_FLAG_BUSY : hal_pkc.h
- PKC_IT_DONE : hal_pkc.h
- PKC_IT_ERR : hal_pkc.h
- PKC_IT_OVF : hal_pkc.h
- PKC_OPERATION_MODE_ADD : hal_pkc.h
- PKC_OPERATION_MODE_BIGADD : hal_pkc.h
- PKC_OPERATION_MODE_BIGMULTI : hal_pkc.h
- PKC_OPERATION_MODE_CMP : hal_pkc.h
- PKC_OPERATION_MODE_INVER : hal_pkc.h
- PKC_OPERATION_MODE_LSHIFT : hal_pkc.h
- PKC_OPERATION_MODE_MULTI : hal_pkc.h
- PKC_OPERATION_MODE_SUB : hal_pkc.h
- PKC_SECURE_MODE_DISABLE : hal_pkc.h
- PKC_SECURE_MODE_ENABLE : hal_pkc.h
- PKC_SPRAM_BASE_ADDR : hal_pkc.h
- PKC_SPRAM_SIZE : hal_pkc.h
- PMR_MGMT_FAIL : gr5405_pwr.h
- PMR_MGMT_SUCCESS : gr5405_pwr.h
- POL_SET : ll_gpio.h
- PRF_CHAR_PRES_FMT_SIZE : ble_prf_types.h
- PRF_INVALID_HANDLE : ble_prf_types.h
- PWM_ACTIONEVENT_CLEAR : hal_pwm.h
- PWM_ACTIONEVENT_NONE : hal_pwm.h
- PWM_ACTIONEVENT_SET : hal_pwm.h
- PWM_ACTIONEVENT_TOGGLE : hal_pwm.h
- PWM_ALIGNED_CENTER : hal_pwm.h
- PWM_ALIGNED_EDGE : hal_pwm.h
- PWM_CODING_CHANNEL_A : hal_pwm.h
- PWM_CODING_CHANNEL_ALL : hal_pwm.h
- PWM_DRIVEPOLARITY_NEGATIVE : hal_pwm.h
- PWM_DRIVEPOLARITY_POSITIVE : hal_pwm.h
- PWM_STOP_LVL_HIGH : hal_pwm.h
- PWM_STOP_LVL_LOW : hal_pwm.h
- PWM_WAITING_TIME_LVL_HIGH : hal_pwm.h
- PWM_WAITING_TIME_LVL_LOW : hal_pwm.h
- PWR_MEM_POWER_FULL : hal_pwr.h
- PWR_MEM_POWER_OFF : hal_pwr.h
- PWR_MEM_POWER_RETENTION : hal_pwr.h
- PWR_MGMT_BB_CHECK_FAIL : gr5405_pwr.h
- PWR_MGMT_MODE_CHECK_FAIL : gr5405_pwr.h
- PWR_SLP_TIMER_MODE_NORMAL : hal_sleep_timer.h
- PWR_SLP_TIMER_MODE_RELOAD : hal_sleep_timer.h
- PWR_SLP_TIMER_MODE_SINGLE : hal_sleep_timer.h
- PWR_TIMER_TYPE_AON_WDT : hal_pwr.h
- PWR_TIMER_TYPE_AON_WDT_TIMER : hal_pwr.h
- PWR_TIMER_TYPE_CAL_ALARM : hal_pwr.h
- PWR_TIMER_TYPE_CAL_TIMER : hal_pwr.h
- PWR_TIMER_TYPE_SLP_TIMER : hal_pwr.h
- PWR_WKUP_COND_ALL : hal_pwr.h
- PWR_WKUP_COND_AON_WDT : hal_pwr.h
- PWR_WKUP_COND_AUSB : hal_pwr.h
- PWR_WKUP_COND_BLE : hal_pwr.h
- PWR_WKUP_COND_CLDR : hal_pwr.h
- PWR_WKUP_COND_CLDR_TICK : hal_pwr.h
- PWR_WKUP_COND_DUSB : hal_pwr.h
- PWR_WKUP_COND_EXT : hal_pwr.h
- PWR_WKUP_COND_MSIO_COMP : hal_pwr.h
- PWR_WKUP_COND_TIMER : hal_pwr.h