Public Attributes | List of all members
ble_gap_adv_period_cfg_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Configuration for periodic advertising. More...

`#include <ble_gapm.h>`

## Public Attributes
uint16_t | adv_intv_min
uint16_t | adv_intv_max
bool | inc_adi_flag

## Detailed Description

Configuration for periodic advertising.

Definition at line 616 of file ble_gapm.h.

## Member Data Documentation

## ◆ adv_intv_max

uint16_t ble_gap_adv_period_cfg_t::adv_intv_max

Maximum advertising interval (in unit of 1.25 ms). Must be greater than 20 ms.

Definition at line 619 of file ble_gapm.h.

## ◆ adv_intv_min

uint16_t ble_gap_adv_period_cfg_t::adv_intv_min

Minimum advertising interval (in unit of 1.25 ms). Must be greater than 20 ms.

Definition at line 618 of file ble_gapm.h.

## ◆ inc_adi_flag

bool ble_gap_adv_period_cfg_t::inc_adi_flag

Flag for include the ADI field in AUX_SYNC_IND PDUs.

Definition at line 620 of file ble_gapm.h.

The documentation for this struct was generated from the following file:

- ble_gapm.h