### - a -

- adv_rf_phy_freq_modify() : ble.h
- ags_non_stream_send() : ags.h
- ags_service_init() : ags.h
- ags_stream_send() : ags.h
- ams_c_attr_display_set() : ams_c.h
- ams_c_attr_focus_set() : ams_c.h
- ams_c_attr_update_notify_set() : ams_c.h
- ams_c_client_init() : ams_c.h
- ams_c_cmd_enable_check() : ams_c.h
- ams_c_cmd_notify_set() : ams_c.h
- ams_c_cmd_send() : ams_c.h
- ams_c_cplt_attr_read() : ams_c.h
- ams_c_disc_srvc_start() : ams_c.h
- ancs_action_perform() : ancs_protocol.h
- ancs_c_client_init() : ancs_c.h
- ancs_c_data_source_notify_set() : ancs_c.h
- ancs_c_discovery_service() : ancs_c.h
- ancs_c_ntf_source_notify_set() : ancs_c.h
- ancs_c_write_control_point() : ancs_c.h
- ancs_decode_data_source() : ancs_protocol.h
- ancs_decode_notification_source() : ancs_protocol.h
- ancs_get_uid() : ancs_protocol.h
- ancs_notify_attr_get() : ancs_protocol.h
- ans_c_ctrl_point_set() : ans_c.h
- ans_c_disc_srvc_start() : ans_c.h
- ans_c_new_alert_notify_set() : ans_c.h
- ans_c_sup_new_alert_cat_read() : ans_c.h
- ans_c_sup_unread_alert_cat_read() : ans_c.h
- ans_c_unread_alert_notify_set() : ans_c.h
- ans_client_init() : ans_c.h
- ans_new_alert_send() : ans.h
- ans_service_init() : ans.h
- ans_unread_alert_send() : ans.h
- app_adc_conversion_async() : app_adc.h
- app_adc_conversion_sync() : app_adc.h
- app_adc_deinit() : app_adc.h
- app_adc_dma_deinit() : app_adc_dma.h
- app_adc_dma_init() : app_adc_dma.h
- app_adc_get_handle() : app_adc.h
- app_adc_init() : app_adc.h
- app_adc_multi_channel_conversion_async() : app_adc.h
- app_adc_temperature_conv() : app_adc.h
- app_adc_vbat_conv() : app_adc.h
- app_adc_voltage_intern() : app_adc.h
- app_aon_wdt_deinit() : app_aon_wdt.h
- app_aon_wdt_init() : app_aon_wdt.h
- app_aon_wdt_refresh() : app_aon_wdt.h
- app_bod_deinit() : app_bod.h
- app_bod_enable() : app_bod.h
- app_bod_event_enable() : app_bod.h
- app_bod_event_set_level() : app_bod.h
- app_bod_init() : app_bod.h
- app_bod_static_mode_enable() : app_bod.h
- app_comp_deinit() : app_comp.h
- app_comp_get_handle() : app_comp.h
- app_comp_init() : app_comp.h
- app_comp_start() : app_comp.h
- app_comp_stop() : app_comp.h
- app_dma_deinit() : app_dma.h
- app_dma_get_handle() : app_dma.h
- app_dma_init() : app_dma.h
- app_dma_start() : app_dma.h
- app_dual_tim_deinit() : app_dual_tim.h
- app_dual_tim_get_handle() : app_dual_tim.h
- app_dual_tim_init() : app_dual_tim.h
- app_dual_tim_set_background_reload() : app_dual_tim.h
- app_dual_tim_set_params() : app_dual_tim.h
- app_dual_tim_start() : app_dual_tim.h
- app_dual_tim_stop() : app_dual_tim.h
- app_gpiote_config() : app_gpiote.h
- app_gpiote_deinit() : app_gpiote.h
- app_gpiote_init() : app_gpiote.h
- app_i2c_deinit() : app_i2c.h
- app_i2c_dma_deinit() : app_i2c_dma.h
- app_i2c_dma_init() : app_i2c_dma.h
- app_i2c_dma_mem_read_async() : app_i2c_dma.h
- app_i2c_dma_mem_write_async() : app_i2c_dma.h
- app_i2c_dma_receive_async() : app_i2c_dma.h
- app_i2c_dma_transmit_async() : app_i2c_dma.h
- app_i2c_get_handle() : app_i2c.h
- app_i2c_init() : app_i2c.h
- app_i2c_master_abort_it() : app_i2c.h
- app_i2c_mem_read_async() : app_i2c.h
- app_i2c_mem_read_sync() : app_i2c.h
- app_i2c_mem_write_async() : app_i2c.h
- app_i2c_mem_write_sync() : app_i2c.h
- app_i2c_receive_async() : app_i2c.h
- app_i2c_receive_sync() : app_i2c.h
- app_i2c_transmit_async() : app_i2c.h
- app_i2c_transmit_sync() : app_i2c.h
- app_io_deinit() : app_io.h
- app_io_event_register_cb() : app_io.h
- app_io_event_unregister() : app_io.h
- app_io_init() : app_io.h
- app_io_read_pin() : app_io.h
- app_io_set_intput_type() : app_io.h
- app_io_set_speed() : app_io.h
- app_io_set_strength() : app_io.h
- app_io_toggle_pin() : app_io.h
- app_io_write_pin() : app_io.h
- app_pwm_config_channel() : app_pwm.h
- app_pwm_deinit() : app_pwm.h
- app_pwm_get_handle() : app_pwm.h
- app_pwm_inactive_channel() : app_pwm.h
- app_pwm_init() : app_pwm.h
- app_pwm_start() : app_pwm.h
- app_pwm_stop() : app_pwm.h
- app_pwm_update_freq() : app_pwm.h
- app_pwr_mgmt_init() : app_pwr_mgmt.h
- app_rng_deinit() : app_rng.h
- app_rng_gen_async() : app_rng.h
- app_rng_gen_sync() : app_rng.h
- app_rng_get_handle() : app_rng.h
- app_rng_init() : app_rng.h
- app_rtc_deinit() : app_rtc.h
- app_rtc_disable_event() : app_rtc.h
- app_rtc_get_time() : app_rtc.h
- app_rtc_init() : app_rtc.h
- app_rtc_init_time() : app_rtc.h
- app_rtc_setup_alarm() : app_rtc.h
- app_rtc_setup_tick() : app_rtc.h
- app_spi_abort() : app_spi.h
- app_spi_deinit() : app_spi.h
- app_spi_dma_deinit() : app_spi_dma.h
- app_spi_dma_init() : app_spi_dma.h
- app_spi_dma_read_eeprom_async() : app_spi_dma.h
- app_spi_dma_receive_async() : app_spi_dma.h
- app_spi_dma_transmit_async() : app_spi_dma.h
- app_spi_dma_transmit_receive_async() : app_spi_dma.h
- app_spi_get_handle() : app_spi.h
- app_spi_init() : app_spi.h
- app_spi_read_eeprom_async() : app_spi.h
- app_spi_read_eeprom_sync() : app_spi.h
- app_spi_receive_async() : app_spi.h
- app_spi_receive_sync() : app_spi.h
- app_spi_transmit_async() : app_spi.h
- app_spi_transmit_receive_async() : app_spi.h
- app_spi_transmit_receive_sync() : app_spi.h
- app_spi_transmit_sync() : app_spi.h
- app_spim_dma_receive_with_ia() : app_spi_dma.h
- app_spim_dma_transmit_with_ia() : app_spi_dma.h
- app_spim_receive_with_ia() : app_spi.h
- app_spim_transmit_with_ia() : app_spi.h
- app_tim_deinit() : app_tim.h
- app_tim_get_handle() : app_tim.h
- app_tim_init() : app_tim.h
- app_tim_start() : app_tim.h
- app_tim_stop() : app_tim.h
- app_uart_abort() : app_uart.h
- app_uart_abort_receive() : app_uart.h
- app_uart_abort_transmit() : app_uart.h
- app_uart_assert_flush() : app_uart.h
- app_uart_deinit() : app_uart.h
- app_uart_dma_deinit() : app_uart_dma.h
- app_uart_dma_init() : app_uart_dma.h
- app_uart_dma_receive_async() : app_uart_dma.h
- app_uart_dma_transmit_async() : app_uart_dma.h
- app_uart_flush() : app_uart.h
- app_uart_get_handle() : app_uart.h
- app_uart_init() : app_uart.h
- app_uart_receive_async() : app_uart.h
- app_uart_receive_sync() : app_uart.h
- app_uart_transmit_async() : app_uart.h
- app_uart_transmit_sync() : app_uart.h