Macros
COMP
Peripheral Driver » LL Driver » COMP » Defines » COMP Exported Constants

## Macros
#define | LL_COMP_HYST_POSITIVE (1UL << AON_PMU_COMP_REG_0_POSITIVE_HYS_EN_Pos )
#define | LL_COMP_HYST_NEGATIVE (1UL << AON_PMU_COMP_REG_0_NEGATIVE_HYS_EN_Pos )

## Detailed Description

## Macro Definition Documentation

## ◆ LL_COMP_HYST_NEGATIVE

#define LL_COMP_HYST_NEGATIVE (1UL << AON_PMU_COMP_REG_0_NEGATIVE_HYS_EN_Pos )

Set negative side of hysteresis for the comparator

Definition at line 153 of file ll_comp.h.

## ◆ LL_COMP_HYST_POSITIVE

#define LL_COMP_HYST_POSITIVE (1UL << AON_PMU_COMP_REG_0_POSITIVE_HYS_EN_Pos )

Set positive side of hysteresis for the comparator

Definition at line 152 of file ll_comp.h.