Macros
InitStrcut default configuartion
Peripheral Driver » LL Driver » Defines » XQSPI Exported Constants » XQSPI Cache direct map enable

## Macros
#define | LL_XQSPI_DEFAULT_CONFIG
| LL XQSPI InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_DEFAULT_CONFIG

#define LL_XQSPI_DEFAULT_CONFIG

Value:
{ \
.mode = LL_XQSPI_MODE_QSPI, \
.cache_mode = LL_XQSPI_CACHE_EN, \
.read_cmd = LL_XQSPI_XIP_CMD_READ, \
.data_size = LL_XQSPI_QSPI_DATASIZE_8BIT, \
.data_order = LL_XQSPI_QSPI_MSB, \
.clock_polarity = LL_XQSPI_SCPOL_HIGH, \
.clock_phase = LL_XQSPI_SCPHA_2EDGE, \
.baud_rate = LL_XQSPI_BAUD_RATE_16M, \
.cache_direct_map_en= LL_XQSPI_CACHE_DIRECT_MAP_DIS, \
.cache_flush = LL_XQSPI_CACHE_FLUSH_EN, \
}

LL XQSPI InitStrcut default configuartion.

Definition at line 352 of file ll_xqspi.h.

LL_XQSPI_MODE_QSPI
#define LL_XQSPI_MODE_QSPI
Definition: ll_xqspi.h:167
LL_XQSPI_SCPOL_HIGH
#define LL_XQSPI_SCPOL_HIGH
Definition: ll_xqspi.h:304
LL_XQSPI_QSPI_MSB
#define LL_XQSPI_QSPI_MSB
Definition: ll_xqspi.h:277
LL_XQSPI_BAUD_RATE_16M
#define LL_XQSPI_BAUD_RATE_16M
Definition: ll_xqspi.h:314
LL_XQSPI_CACHE_EN
#define LL_XQSPI_CACHE_EN
Definition: ll_xqspi.h:208
LL_XQSPI_QSPI_DATASIZE_8BIT
#define LL_XQSPI_QSPI_DATASIZE_8BIT
Definition: ll_xqspi.h:284
LL_XQSPI_XIP_CMD_READ
#define LL_XQSPI_XIP_CMD_READ
Definition: ll_xqspi.h:173
LL_XQSPI_CACHE_FLUSH_EN
#define LL_XQSPI_CACHE_FLUSH_EN
Definition: ll_xqspi.h:327
LL_XQSPI_CACHE_DIRECT_MAP_DIS
#define LL_XQSPI_CACHE_DIRECT_MAP_DIS
Definition: ll_xqspi.h:320
LL_XQSPI_SCPHA_2EDGE
#define LL_XQSPI_SCPHA_2EDGE
Definition: ll_xqspi.h:297