Macros
Defines
Peripheral Driver » APP DRIVER » DRIVER CONFIG

## Macros
#define | APP_DRIVER_ADC_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
| APP driver peripheral priority define. More...
#define | APP_DRIVER_AES_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID
#define | APP_DRIVER_COMP_WAKEUP_PRIORITY WAKEUP_PRIORITY_LOW
#define | APP_DRIVER_DUAL_TIM_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID
#define | APP_DRIVER_DMA_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
#define | APP_DRIVER_UART_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
#define | APP_DRIVER_HMAC_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID
#define | APP_DRIVER_I2C_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
#define | APP_DRIVER_I2S_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
#define | APP_DRIVER_QSPI_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
#define | APP_DRIVER_RNG_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID
#define | APP_DRIVER_SPI_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
#define | APP_DRIVER_TIM_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID
#define | APP_DRIVER_PWM_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID
#define | APP_DRIVER_ISO7816_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
#define | APP_DRIVER_PKC_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
#define | APP_DRIVER_DSPI_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
#define | APP_DRIVER_PDM_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
#define | APP_DRIVER_CAN_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH
#define | APP_DRIVER_LIN_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

## Detailed Description

## Macro Definition Documentation

## ◆ APP_DRIVER_ADC_WAKEUP_PRIORITY

#define APP_DRIVER_ADC_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

APP driver peripheral priority define.

ADC Wakeup priority High

Definition at line 414 of file app_drv_config.h.

## ◆ APP_DRIVER_AES_WAKEUP_PRIORITY

#define APP_DRIVER_AES_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID

AES Wakeup priority Mid

Definition at line 418 of file app_drv_config.h.

## ◆ APP_DRIVER_CAN_WAKEUP_PRIORITY

#define APP_DRIVER_CAN_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

CAN Wakeup priority High

Definition at line 486 of file app_drv_config.h.

## ◆ APP_DRIVER_COMP_WAKEUP_PRIORITY

#define APP_DRIVER_COMP_WAKEUP_PRIORITY WAKEUP_PRIORITY_LOW

COMP Wakeup priority Low

Definition at line 422 of file app_drv_config.h.

## ◆ APP_DRIVER_DMA_WAKEUP_PRIORITY

#define APP_DRIVER_DMA_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

DMA Wakeup priority High

Definition at line 430 of file app_drv_config.h.

## ◆ APP_DRIVER_DSPI_WAKEUP_PRIORITY

#define APP_DRIVER_DSPI_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

DSPI Wakeup priority High

Definition at line 478 of file app_drv_config.h.

## ◆ APP_DRIVER_DUAL_TIM_WAKEUP_PRIORITY

#define APP_DRIVER_DUAL_TIM_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID

DUAL TIM Wakeup priority Mid

Definition at line 426 of file app_drv_config.h.

## ◆ APP_DRIVER_HMAC_WAKEUP_PRIORITY

#define APP_DRIVER_HMAC_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID

Hmac Wakeup priority Mid

Definition at line 438 of file app_drv_config.h.

## ◆ APP_DRIVER_I2C_WAKEUP_PRIORITY

#define APP_DRIVER_I2C_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

I2C Wakeup priority High

Definition at line 442 of file app_drv_config.h.

## ◆ APP_DRIVER_I2S_WAKEUP_PRIORITY

#define APP_DRIVER_I2S_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

I2S Wakeup priority High

Definition at line 446 of file app_drv_config.h.

## ◆ APP_DRIVER_ISO7816_WAKEUP_PRIORITY

#define APP_DRIVER_ISO7816_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

ISO7816 Wakeup priority High

Definition at line 470 of file app_drv_config.h.

## ◆ APP_DRIVER_LIN_WAKEUP_PRIORITY

#define APP_DRIVER_LIN_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

LIN Wakeup priority High

Definition at line 490 of file app_drv_config.h.

## ◆ APP_DRIVER_PDM_WAKEUP_PRIORITY

#define APP_DRIVER_PDM_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

PDM Wakeup priority High

Definition at line 482 of file app_drv_config.h.

## ◆ APP_DRIVER_PKC_WAKEUP_PRIORITY

#define APP_DRIVER_PKC_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

PKC Wakeup priority High

Definition at line 474 of file app_drv_config.h.

## ◆ APP_DRIVER_PWM_WAKEUP_PRIORITY

#define APP_DRIVER_PWM_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID

PWM Wakeup priority Mid

Definition at line 466 of file app_drv_config.h.

## ◆ APP_DRIVER_QSPI_WAKEUP_PRIORITY

#define APP_DRIVER_QSPI_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

QSPI Wakeup priority High

Definition at line 450 of file app_drv_config.h.

## ◆ APP_DRIVER_RNG_WAKEUP_PRIORITY

#define APP_DRIVER_RNG_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID

RNG Wakeup priority Mid

Definition at line 454 of file app_drv_config.h.

## ◆ APP_DRIVER_SPI_WAKEUP_PRIORITY

#define APP_DRIVER_SPI_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

SPI Wakeup priority High

Definition at line 458 of file app_drv_config.h.

## ◆ APP_DRIVER_TIM_WAKEUP_PRIORITY

#define APP_DRIVER_TIM_WAKEUP_PRIORITY WAKEUP_PRIORITY_MID

TIM Wakeup priority Mid

Definition at line 462 of file app_drv_config.h.

## ◆ APP_DRIVER_UART_WAKEUP_PRIORITY

#define APP_DRIVER_UART_WAKEUP_PRIORITY WAKEUP_PRIORITY_HIGH

Uart Wakeup priority High

Definition at line 434 of file app_drv_config.h.