### - l -

- L2CC_NB_DEPRECATED_MSG : ble_id.h
- LL_ADC_CLK_16K : ll_adc.h
- LL_ADC_CLK_16M : ll_adc.h
- LL_ADC_CLK_1M : ll_adc.h
- LL_ADC_CLK_4K : ll_adc.h
- LL_ADC_CLK_4M : ll_adc.h
- LL_ADC_CLK_8K : ll_adc.h
- LL_ADC_CLK_8M : ll_adc.h
- LL_ADC_CLK_NONE : ll_adc.h
- LL_ADC_DEFAULT_CONFIG : ll_adc.h
- LL_ADC_INPUT_DIFFERENTIAL : ll_adc.h
- LL_ADC_INPUT_SINGLE : ll_adc.h
- LL_ADC_INPUT_SRC_BAT : ll_adc.h
- LL_ADC_INPUT_SRC_IO0 : ll_adc.h
- LL_ADC_INPUT_SRC_IO1 : ll_adc.h
- LL_ADC_INPUT_SRC_IO2 : ll_adc.h
- LL_ADC_INPUT_SRC_IO3 : ll_adc.h
- LL_ADC_INPUT_SRC_IO4 : ll_adc.h
- LL_ADC_INPUT_SRC_IO5 : ll_adc.h
- LL_ADC_INPUT_SRC_IO6 : ll_adc.h
- LL_ADC_INPUT_SRC_IO7 : ll_adc.h
- LL_ADC_INPUT_SRC_REF : ll_adc.h
- LL_ADC_INPUT_SRC_TMP : ll_adc.h
- LL_ADC_ReadReg : ll_adc.h
- LL_ADC_REF_SRC_BUF_INT : ll_adc.h
- LL_ADC_REF_SRC_IO0 : ll_adc.h
- LL_ADC_REF_SRC_IO1 : ll_adc.h
- LL_ADC_REF_SRC_IO2 : ll_adc.h
- LL_ADC_REF_SRC_IO3 : ll_adc.h
- LL_ADC_REF_VALUE_0P8 : ll_adc.h
- LL_ADC_REF_VALUE_1P2 : ll_adc.h
- LL_ADC_REF_VALUE_1P6 : ll_adc.h
- LL_ADC_REF_VALUE_2P0 : ll_adc.h
- LL_ADC_WriteReg : ll_adc.h
- LL_AES_DMA_TRANSIZE_MAX : ll_aes.h
- LL_AES_DMA_TRANSIZE_MIN : ll_aes.h
- LL_AES_FLAG_DATAREADY : ll_aes.h
- LL_AES_FLAG_DMA_DONE : ll_aes.h
- LL_AES_FLAG_DMA_ERR : ll_aes.h
- LL_AES_FLAG_KEY_VALID : ll_aes.h
- LL_AES_KEY_SIZE_128 : ll_aes.h
- LL_AES_KEY_SIZE_192 : ll_aes.h
- LL_AES_KEY_SIZE_256 : ll_aes.h
- LL_AES_KEYMODE_KEYWRAP : ll_aes.h
- LL_AES_KEYMODE_NORMAL : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_0 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_1 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_10 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_11 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_12 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_13 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_14 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_15 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_2 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_3 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_4 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_5 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_6 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_7 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_8 : ll_aes.h
- LL_AES_KEYRAM_KEYSLOT_9 : ll_aes.h
- LL_AES_KEYTYPE_AHB : ll_aes.h
- LL_AES_KEYTYPE_KRAM : ll_aes.h
- LL_AES_KEYTYPE_MCU : ll_aes.h
- LL_AES_OPERATION_MODE_CBC : ll_aes.h
- LL_AES_OPERATION_MODE_ECB : ll_aes.h
- LL_AES_ReadReg : ll_aes.h
- LL_AES_WriteReg : ll_aes.h
- LL_AON_GPIO_DEFAULT_CONFIG : ll_aon_gpio.h
- LL_AON_GPIO_INPUT_TYPE_CMOS : ll_aon_gpio.h
- LL_AON_GPIO_INPUT_TYPE_SCHMITT : ll_aon_gpio.h
- LL_AON_GPIO_MODE_INOUT : ll_aon_gpio.h
- LL_AON_GPIO_MODE_INPUT : ll_aon_gpio.h
- LL_AON_GPIO_MODE_INPUT_POS : ll_aon_gpio.h
- LL_AON_GPIO_MODE_NONE : ll_aon_gpio.h
- LL_AON_GPIO_MODE_OUTPUT : ll_aon_gpio.h
- LL_AON_GPIO_MODE_OUTPUT_POS : ll_aon_gpio.h
- LL_AON_GPIO_PIN_0 : ll_aon_gpio.h
- LL_AON_GPIO_PIN_1 : ll_aon_gpio.h
- LL_AON_GPIO_PIN_2 : ll_aon_gpio.h
- LL_AON_GPIO_PIN_3 : ll_aon_gpio.h
- LL_AON_GPIO_PIN_4 : ll_aon_gpio.h
- LL_AON_GPIO_PIN_5 : ll_aon_gpio.h
- LL_AON_GPIO_PIN_6 : ll_aon_gpio.h
- LL_AON_GPIO_PIN_7 : ll_aon_gpio.h
- LL_AON_GPIO_PIN_ALL : ll_aon_gpio.h
- LL_AON_GPIO_PULL_DOWN : ll_aon_gpio.h
- LL_AON_GPIO_PULL_NO : ll_aon_gpio.h
- LL_AON_GPIO_PULL_UP : ll_aon_gpio.h
- LL_AON_GPIO_ReadReg : ll_aon_gpio.h
- LL_AON_GPIO_SPEED_HIGH : ll_aon_gpio.h
- LL_AON_GPIO_SPEED_MEDIUM : ll_aon_gpio.h
- LL_AON_GPIO_STRENGTH_DS0_MASK : ll_aon_gpio.h
- LL_AON_GPIO_STRENGTH_DS0_POS : ll_aon_gpio.h
- LL_AON_GPIO_STRENGTH_DS1_MASK : ll_aon_gpio.h
- LL_AON_GPIO_STRENGTH_DS1_POS : ll_aon_gpio.h
- LL_AON_GPIO_STRENGTH_HIGH : ll_aon_gpio.h
- LL_AON_GPIO_STRENGTH_LOW : ll_aon_gpio.h
- LL_AON_GPIO_STRENGTH_MEDIUM : ll_aon_gpio.h
- LL_AON_GPIO_STRENGTH_ULTRA : ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_BOTH_EDGE : ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_FALLING : ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_HIGH : ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_LOW : ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_NONE : ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_RISING : ll_aon_gpio.h
- LL_AON_GPIO_WriteReg : ll_aon_gpio.h
- LL_AON_SLOW_CLK_256K : ll_clk.h
- LL_AON_SLOW_CLK_32K : ll_clk.h
- LL_BOD_BOD2_AUTO_POWER_BYPASS_DISABLE : ll_bod.h
- LL_BOD_BOD2_AUTO_POWER_BYPASS_ENABLE : ll_bod.h
- LL_BOD_BOD2_DISABLE : ll_bod.h
- LL_BOD_BOD2_ENABLE : ll_bod.h
- LL_BOD_BOD2_LEVEL_0 : ll_bod.h
- LL_BOD_BOD2_LEVEL_1 : ll_bod.h
- LL_BOD_BOD2_LEVEL_2 : ll_bod.h
- LL_BOD_BOD2_LEVEL_3 : ll_bod.h
- LL_BOD_BOD2_LEVEL_4 : ll_bod.h
- LL_BOD_BOD2_LEVEL_5 : ll_bod.h
- LL_BOD_BOD2_LEVEL_6 : ll_bod.h
- LL_BOD_BOD2_LEVEL_7 : ll_bod.h
- LL_BOD_BOD_DISABLE : ll_bod.h
- LL_BOD_BOD_ENABLE : ll_bod.h
- LL_BOD_STATIC_DISABLE : ll_bod.h
- LL_BOD_STATIC_ENABLE : ll_bod.h
- LL_CALENDAR_DIV_128 : ll_calendar.h
- LL_CALENDAR_DIV_16 : ll_calendar.h
- LL_CALENDAR_DIV_2 : ll_calendar.h
- LL_CALENDAR_DIV_32 : ll_calendar.h
- LL_CALENDAR_DIV_4 : ll_calendar.h
- LL_CALENDAR_DIV_64 : ll_calendar.h
- LL_CALENDAR_DIV_8 : ll_calendar.h
- LL_CALENDAR_DIV_NONE : ll_calendar.h
- LL_CGC_FRC_ALL_HCLK0 : ll_cgc.h
- LL_CGC_FRC_ALL_HCLK1 : ll_cgc.h
- LL_CGC_FRC_ALL_HCLK2 : ll_cgc.h
- LL_CGC_FRC_APB_SUB_HCLK : ll_cgc.h
- LL_CGC_FRC_BLE_BRG_HCLK : ll_cgc.h
- LL_CGC_FRC_GPIO_HCLK : ll_cgc.h
- LL_CGC_FRC_HTB_HCLK : ll_cgc.h
- LL_CGC_FRC_I2C0_PCLK : ll_cgc.h
- LL_CGC_FRC_I2C1_PCLK : ll_cgc.h
- LL_CGC_FRC_PWM_0_PCLK : ll_cgc.h
- LL_CGC_FRC_PWM_1_PCLK : ll_cgc.h
- LL_CGC_FRC_ROM_HCLK : ll_cgc.h
- LL_CGC_FRC_SECU_HCLK : ll_cgc.h
- LL_CGC_FRC_SERIAL_HCLK : ll_cgc.h
- LL_CGC_FRC_SERIALS_HCLK2 : ll_cgc.h
- LL_CGC_FRC_SNSADC_HCLK : ll_cgc.h
- LL_CGC_FRC_SPI_M_PCLK : ll_cgc.h
- LL_CGC_FRC_SPI_S_PCLK : ll_cgc.h
- LL_CGC_FRC_SRAM_HCLK : ll_cgc.h
- LL_CGC_FRC_UART0_PCLK : ll_cgc.h
- LL_CGC_FRC_UART1_PCLK : ll_cgc.h
- LL_CGC_FRC_XF_XQSPI_HCLK : ll_cgc.h
- LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN : ll_cgc.h
- LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN : ll_cgc.h
- LL_CGC_MCU_MISC_CLK : ll_cgc.h
- LL_CGC_MCU_MISC_CLK_DEFAULT : ll_cgc.h
- LL_CGC_MCU_MISC_DMA_CLK : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_DEFAULT : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_EN : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_SYNC_EN : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_AHB_BUS_LP_EN : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_PCLK_EN : ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_SCLK_EN : ll_cgc.h
- LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL : ll_cgc.h
- LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF : ll_cgc.h
- LL_CGC_MCU_PERIPH_SLP_CG_DEFAULT : ll_cgc.h
- LL_CGC_MCU_SECU_FRC_OFF_ALL : ll_cgc.h
- LL_CGC_MCU_SECU_FRC_OFF_HCLK : ll_cgc.h
- LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK : ll_cgc.h
- LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN : ll_cgc.h
- LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN : ll_cgc.h
- LL_CGC_MCU_SUBSYS_DEFAULT_CLK : ll_cgc.h
- LL_CGC_MCU_SUBSYS_DEFAULT_WFI_CLK0 : ll_cgc.h
- LL_CGC_MCU_SUBSYS_DEFAULT_WFI_CLK1 : ll_cgc.h
- LL_CGC_WFI_ALL_HCLK0 : ll_cgc.h
- LL_CGC_WFI_ALL_HCLK1 : ll_cgc.h
- LL_CGC_WFI_AON_MCUSUB_HCLK : ll_cgc.h
- LL_CGC_WFI_APB_SUB_HCLK : ll_cgc.h
- LL_CGC_WFI_BLE_BRG_HCLK : ll_cgc.h
- LL_CGC_WFI_GPIO_HCLK : ll_cgc.h
- LL_CGC_WFI_HTB_HCLK : ll_cgc.h
- LL_CGC_WFI_ROM_HCLK : ll_cgc.h
- LL_CGC_WFI_SECU_HCLK : ll_cgc.h
- LL_CGC_WFI_SERIAL_HCLK : ll_cgc.h
- LL_CGC_WFI_SNSADC_HCLK : ll_cgc.h
- LL_CGC_WFI_SRAM_HCLK : ll_cgc.h
- LL_CGC_WFI_XF_XQSPI_HCLK : ll_cgc.h
- LL_CLDR_TIMER_TICK : ll_calendar.h
- LL_CLDR_TIMER_TICK_TYPE_AUTO : ll_calendar.h
- LL_CLDR_TIMER_TICK_TYPE_SINGLE : ll_calendar.h
- LL_CLK_CAL_CLK_SOURCE_RNG_32K : ll_clk_cal.h
- LL_CLK_CAL_CLK_SOURCE_RNG_40K : ll_clk_cal.h
- LL_CLK_CAL_CLK_SOURCE_RTC_32K : ll_clk_cal.h
- LL_CLK_CPLL_S16M_CLK : ll_clk.h
- LL_CLK_CPLL_S64M_CLK : ll_clk.h
- LL_CLK_CPLL_T32M_CLK : ll_clk.h
- LL_CLK_RC_OSC_CLK : ll_aon_gpio.h
- LL_CLK_RNG_OSC_250K : ll_aon_gpio.h
- LL_CLK_RNG_OSC_32K : ll_aon_gpio.h
- LL_CLK_RTC_CLK : ll_aon_gpio.h
- LL_CLK_SEL_SOURCE_CPLL_CLK : ll_clk.h
- LL_CLK_SEL_SOURCE_HF_OSC_CLK : ll_clk.h
- LL_CLK_XO_PLL_HF_STAT : ll_clk.h
- LL_CLK_XO_PLL_PLL_STAT : ll_clk.h
- LL_CLK_XO_PLL_XO_STAT : ll_clk.h
- LL_CLK_XO_S16M_CLK : ll_clk.h
- LL_COMP_DEFAULT_CONFIG : ll_comp.h
- LL_COMP_HYST_NEGATIVE : ll_comp.h
- LL_COMP_HYST_POSITIVE : ll_comp.h
- LL_COMP_INPUT_SRC_IO0 : ll_comp.h
- LL_COMP_INPUT_SRC_IO1 : ll_comp.h
- LL_COMP_INPUT_SRC_IO2 : ll_comp.h
- LL_COMP_INPUT_SRC_IO3 : ll_comp.h
- LL_COMP_INPUT_SRC_IO4 : ll_comp.h
- LL_COMP_INPUT_SRC_IO5 : ll_comp.h
- LL_COMP_INPUT_SRC_IO6 : ll_comp.h
- LL_COMP_INPUT_SRC_IO7 : ll_comp.h
- LL_COMP_INPUT_SRC_VBAT : ll_comp.h
- LL_COMP_INPUT_SRC_VREF : ll_comp.h
- LL_COMP_ReadReg : ll_comp.h
- LL_COMP_REF_SRC_IO0 : ll_comp.h
- LL_COMP_REF_SRC_IO1 : ll_comp.h
- LL_COMP_REF_SRC_IO2 : ll_comp.h
- LL_COMP_REF_SRC_IO3 : ll_comp.h
- LL_COMP_REF_SRC_IO4 : ll_comp.h
- LL_COMP_REF_SRC_IO5 : ll_comp.h
- LL_COMP_REF_SRC_IO6 : ll_comp.h
- LL_COMP_REF_SRC_IO7 : ll_comp.h
- LL_COMP_REF_SRC_VBAT : ll_comp.h
- LL_COMP_REF_SRC_VREF : ll_comp.h
- LL_COMP_RES_DEGENERATION_NEGATIVE : ll_comp.h
- LL_COMP_RES_DEGENERATION_POSITIVE : ll_comp.h
- LL_COMP_WAKEUP_EDGE_BOTH : ll_comp.h
- LL_COMP_WAKEUP_EDGE_FALLING : ll_comp.h
- LL_COMP_WAKEUP_EDGE_RISING : ll_comp.h
- LL_COMP_WriteReg : ll_comp.h
- LL_DDVS_AUTO_MODE : ll_ddvs.h
- LL_DDVS_CLK_DIS : ll_ddvs.h
- LL_DDVS_CLK_EN : ll_ddvs.h
- LL_DDVS_CLK_SEL_SYS_16M : ll_ddvs.h
- LL_DDVS_CLK_SEL_SYS_32M : ll_ddvs.h
- LL_DDVS_CLK_SEL_XO_16M : ll_ddvs.h
- LL_DDVS_CLK_SEL_XO_32M : ll_ddvs.h
- LL_DDVS_DIS : ll_ddvs.h
- LL_DDVS_DIVIDE_FACTOR_16K : ll_ddvs.h
- LL_DDVS_DIVIDE_FACTOR_4K : ll_ddvs.h
- LL_DDVS_DIVIDE_FACTOR_8K : ll_ddvs.h
- LL_DDVS_EN : ll_ddvs.h
- LL_DDVS_MALNUAL_MODE : ll_ddvs.h
- LL_DDVS_RINGO_0_EN : ll_ddvs.h
- LL_DDVS_RINGO_1_EN : ll_ddvs.h
- LL_DDVS_RINGO_2_EN : ll_ddvs.h
- LL_DDVS_RINGO_3_EN : ll_ddvs.h
- LL_DDVS_RINGO_ALL_DIS : ll_ddvs.h
- LL_DDVS_RINGO_ALL_EN : ll_ddvs.h
- LL_DMA0_PERIPH_CTE : ll_dma.h
- LL_DMA0_PERIPH_I2C0_RX : ll_dma.h
- LL_DMA0_PERIPH_I2C0_TX : ll_dma.h
- LL_DMA0_PERIPH_I2C1_RX : ll_dma.h
- LL_DMA0_PERIPH_I2C1_TX : ll_dma.h
- LL_DMA0_PERIPH_MEM : ll_dma.h
- LL_DMA0_PERIPH_PWM0 : ll_dma.h
- LL_DMA0_PERIPH_SNSADC : ll_dma.h
- LL_DMA0_PERIPH_SPIM_RX : ll_dma.h
- LL_DMA0_PERIPH_SPIM_TX : ll_dma.h
- LL_DMA0_PERIPH_SPIS_RX : ll_dma.h
- LL_DMA0_PERIPH_SPIS_TX : ll_dma.h
- LL_DMA0_PERIPH_UART0_RX : ll_dma.h
- LL_DMA0_PERIPH_UART0_TX : ll_dma.h
- LL_DMA0_PERIPH_UART1_RX : ll_dma.h
- LL_DMA0_PERIPH_UART1_TX : ll_dma.h
- LL_DMA_CHANNEL_0 : ll_dma.h
- LL_DMA_CHANNEL_1 : ll_dma.h
- LL_DMA_CHANNEL_2 : ll_dma.h
- LL_DMA_CHANNEL_3 : ll_dma.h
- LL_DMA_CHANNEL_4 : ll_dma.h
- LL_DMA_CHANNEL_ALL : ll_dma.h
- LL_DMA_DDATAALIGN_BYTE : ll_dma.h
- LL_DMA_DDATAALIGN_HALFWORD : ll_dma.h
- LL_DMA_DDATAALIGN_WORD : ll_dma.h
- LL_DMA_DHANDSHAKING_HW : ll_dma.h
- LL_DMA_DHANDSHAKING_SW : ll_dma.h
- LL_DMA_DIRECTION_MEMORY_TO_MEMORY : ll_dma.h
- LL_DMA_DIRECTION_MEMORY_TO_PERIPH : ll_dma.h
- LL_DMA_DIRECTION_PERIPH_TO_MEMORY : ll_dma.h
- LL_DMA_DIRECTION_PERIPH_TO_PERIPH : ll_dma.h
- LL_DMA_DST_BURST_LENGTH_1 : ll_dma.h
- LL_DMA_DST_BURST_LENGTH_128 : ll_dma.h
- LL_DMA_DST_BURST_LENGTH_16 : ll_dma.h
- LL_DMA_DST_BURST_LENGTH_256 : ll_dma.h
- LL_DMA_DST_BURST_LENGTH_32 : ll_dma.h
- LL_DMA_DST_BURST_LENGTH_4 : ll_dma.h
- LL_DMA_DST_BURST_LENGTH_64 : ll_dma.h
- LL_DMA_DST_BURST_LENGTH_8 : ll_dma.h
- LL_DMA_DST_DECREMENT : ll_dma.h
- LL_DMA_DST_INCREMENT : ll_dma.h
- LL_DMA_DST_NO_CHANGE : ll_dma.h
- LL_DMA_LOCK_BUS_DSIBALE : ll_dma.h
- LL_DMA_LOCK_BUS_ENABLE : ll_dma.h
- LL_DMA_LOCK_BUS_LEVEL_BLK : ll_dma.h
- LL_DMA_LOCK_BUS_LEVEL_TFR : ll_dma.h
- LL_DMA_LOCK_BUS_LEVEL_TRANS : ll_dma.h
- LL_DMA_LOCK_CH_DSIBALE : ll_dma.h
- LL_DMA_LOCK_CH_ENABLE : ll_dma.h
- LL_DMA_LOCK_CH_LEVEL_BLK : ll_dma.h
- LL_DMA_LOCK_CH_LEVEL_TFR : ll_dma.h
- LL_DMA_LOCK_CH_LEVEL_TRANS : ll_dma.h
- LL_DMA_PRIORITY_0 : ll_dma.h
- LL_DMA_PRIORITY_1 : ll_dma.h
- LL_DMA_PRIORITY_2 : ll_dma.h
- LL_DMA_PRIORITY_3 : ll_dma.h
- LL_DMA_PRIORITY_4 : ll_dma.h
- LL_DMA_PRIORITY_5 : ll_dma.h
- LL_DMA_PRIORITY_6 : ll_dma.h
- LL_DMA_PRIORITY_7 : ll_dma.h
- LL_DMA_ReadReg : ll_dma.h
- LL_DMA_SDATAALIGN_BYTE : ll_dma.h
- LL_DMA_SDATAALIGN_HALFWORD : ll_dma.h
- LL_DMA_SDATAALIGN_WORD : ll_dma.h
- LL_DMA_SHANDSHAKING_HW : ll_dma.h
- LL_DMA_SHANDSHAKING_SW : ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_1 : ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_128 : ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_16 : ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_256 : ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_32 : ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_4 : ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_64 : ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_8 : ll_dma.h
- LL_DMA_SRC_DECREMENT : ll_dma.h
- LL_DMA_SRC_INCREMENT : ll_dma.h
- LL_DMA_SRC_NO_CHANGE : ll_dma.h
- LL_DMA_WriteReg : ll_dma.h
- LL_DUAL_TIMER_COUNTERSIZE_16 : ll_dual_tim.h
- LL_DUAL_TIMER_COUNTERSIZE_32 : ll_dual_tim.h
- LL_DUAL_TIMER_FREERUNNING_MODE : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_ACT_PERIOD : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_ACT_START : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_ACT_STOP : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_BLEPULSE1 : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_BLEPULSE2 : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_COUNTDONE : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_IOA_ACT_C1 : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_IOA_ACT_C2 : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_IOB_ACT_C1 : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_IOB_ACT_C2 : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_IOC_ACT_C1 : ll_dual_tim.h
- LL_DUAL_TIMER_INTSTAT_IOC_ACT_C2 : ll_dual_tim.h
- LL_DUAL_TIMER_IO_ACTION_NONE : ll_dual_tim.h
- LL_DUAL_TIMER_IO_ACTION_RESET : ll_dual_tim.h
- LL_DUAL_TIMER_IO_ACTION_SET : ll_dual_tim.h
- LL_DUAL_TIMER_IO_ACTION_TOGGLE : ll_dual_tim.h
- LL_DUAL_TIMER_IO_INIT_RESET : ll_dual_tim.h
- LL_DUAL_TIMER_IO_INIT_SET : ll_dual_tim.h
- LL_DUAL_TIMER_PERIODIC_MODE : ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV0 : ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV16 : ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV256 : ll_dual_tim.h
- LL_DUAL_TIMER_ReadReg : ll_dual_tim.h
- LL_DUAL_TIMER_WriteReg : ll_dual_tim.h
- LL_ECC_CURVE_DEFAULT_CONFIG : ll_pkc.h
- LL_ECC_CURVE_SECP256K1_CONFIG : ll_pkc.h
- LL_ECC_CURVE_SECP256R1_CONFIG : ll_pkc.h
- LL_EFUSE_INIT_CHECK : ll_efuse.h
- LL_EFUSE_INIT_CHECK_DONE : ll_efuse.h
- LL_EFUSE_INIT_CHECK_SUCCESS : ll_efuse.h
- LL_EFUSE_PWR_CTL_DIS_DONE : ll_efuse.h
- LL_EFUSE_PWR_CTL_EN_DONE : ll_efuse.h
- LL_EFUSE_ReadReg : ll_efuse.h
- LL_EFUSE_WRITE_DONE : ll_efuse.h
- LL_EFUSE_WriteReg : ll_efuse.h
- LL_GPIO_DEFAULT_CONFIG : ll_gpio.h
- LL_GPIO_GET_DPAD_POS : ll_gpio.h
- LL_GPIO_GET_REG_MUX_CTRL_0_7 : ll_gpio.h
- LL_GPIO_GET_REG_MUX_CTRL_8_15 : ll_gpio.h
- LL_GPIO_GET_RESISTOR_POS : ll_gpio.h
- LL_GPIO_INPUT_TYPE_CMOS : ll_gpio.h
- LL_GPIO_INPUT_TYPE_SCHMITT : ll_gpio.h
- LL_GPIO_MODE_INOUT : ll_gpio.h
- LL_GPIO_MODE_INPUT : ll_gpio.h
- LL_GPIO_MODE_INPUT_POS : ll_gpio.h
- LL_GPIO_MODE_NONE : ll_gpio.h
- LL_GPIO_MODE_OUTPUT : ll_gpio.h
- LL_GPIO_MODE_OUTPUT_POS : ll_gpio.h
- LL_GPIO_PIN_0 : ll_gpio.h
- LL_GPIO_PIN_1 : ll_gpio.h
- LL_GPIO_PIN_10 : ll_gpio.h
- LL_GPIO_PIN_11 : ll_gpio.h
- LL_GPIO_PIN_12 : ll_gpio.h
- LL_GPIO_PIN_13 : ll_gpio.h
- LL_GPIO_PIN_2 : ll_gpio.h
- LL_GPIO_PIN_3 : ll_gpio.h
- LL_GPIO_PIN_4 : ll_gpio.h
- LL_GPIO_PIN_5 : ll_gpio.h
- LL_GPIO_PIN_6 : ll_gpio.h
- LL_GPIO_PIN_7 : ll_gpio.h
- LL_GPIO_PIN_8 : ll_gpio.h
- LL_GPIO_PIN_9 : ll_gpio.h
- LL_GPIO_PIN_ALL : ll_gpio.h
- LL_GPIO_PULL_DOWN : ll_gpio.h
- LL_GPIO_PULL_NO : ll_gpio.h
- LL_GPIO_PULL_UP : ll_gpio.h
- LL_GPIO_ReadReg : ll_gpio.h
- LL_GPIO_SPEED_HIGH : ll_gpio.h
- LL_GPIO_SPEED_MEDIUM : ll_gpio.h
- LL_GPIO_STRENGTH_DS0_MASK : ll_gpio.h
- LL_GPIO_STRENGTH_DS0_POS : ll_gpio.h
- LL_GPIO_STRENGTH_DS1_MASK : ll_gpio.h
- LL_GPIO_STRENGTH_DS1_POS : ll_gpio.h
- LL_GPIO_STRENGTH_HIGH : ll_gpio.h
- LL_GPIO_STRENGTH_LOW : ll_gpio.h
- LL_GPIO_STRENGTH_MEDIUM : ll_gpio.h
- LL_GPIO_STRENGTH_ULTRA : ll_gpio.h
- LL_GPIO_TRIGGER_BOTH_EDGE : ll_gpio.h
- LL_GPIO_TRIGGER_FALLING : ll_gpio.h
- LL_GPIO_TRIGGER_HIGH : ll_gpio.h
- LL_GPIO_TRIGGER_LOW : ll_gpio.h
- LL_GPIO_TRIGGER_NONE : ll_gpio.h
- LL_GPIO_TRIGGER_RISING : ll_gpio.h
- LL_GPIO_WriteReg : ll_gpio.h
- LL_HMAC_CALCULATETYPE_HMAC : ll_hmac.h
- LL_HMAC_CALCULATETYPE_SHA : ll_hmac.h
- LL_HMAC_DMA_TRANSIZE_MAX : ll_hmac.h
- LL_HMAC_DMA_TRANSIZE_MIN : ll_hmac.h
- LL_HMAC_FLAG_DATAREADY_HMAC : ll_hmac.h
- LL_HMAC_FLAG_DATAREADY_SHA : ll_hmac.h
- LL_HMAC_FLAG_DMA_DONE : ll_hmac.h
- LL_HMAC_FLAG_DMA_ERR : ll_hmac.h
- LL_HMAC_FLAG_DMA_MESSAGEDONE : ll_hmac.h
- LL_HMAC_FLAG_KEY_VALID : ll_hmac.h
- LL_HMAC_HASH_STANDARD : ll_hmac.h
- LL_HMAC_HASH_USER : ll_hmac.h
- LL_HMAC_KEYTYPE_AHB : ll_hmac.h
- LL_HMAC_KEYTYPE_KRAM : ll_hmac.h
- LL_HMAC_KEYTYPE_MCU : ll_hmac.h
- LL_HMAC_ReadReg : ll_hmac.h
- LL_HMAC_WriteReg : ll_hmac.h
- LL_I2C_ABRT_10ADDR1_NOACK : ll_i2c.h
- LL_I2C_ABRT_10ADDR2_NOACK : ll_i2c.h
- LL_I2C_ABRT_10B_RD_NORSTRT : ll_i2c.h
- LL_I2C_ABRT_7B_ADDR_NOACK : ll_i2c.h
- LL_I2C_ABRT_ARB_LOST : ll_i2c.h
- LL_I2C_ABRT_GCALL_NOACK : ll_i2c.h
- LL_I2C_ABRT_GCALL_READ : ll_i2c.h
- LL_I2C_ABRT_HS_ACKDET : ll_i2c.h
- LL_I2C_ABRT_HS_NORSTRT : ll_i2c.h
- LL_I2C_ABRT_MST_DIS : ll_i2c.h
- LL_I2C_ABRT_SBYTE_ACKDET : ll_i2c.h
- LL_I2C_ABRT_SBYTE_NORSTRT : ll_i2c.h
- LL_I2C_ABRT_SDA_STUCK_AT_LOW : ll_i2c.h
- LL_I2C_ABRT_SLV_ARBLOST : ll_i2c.h
- LL_I2C_ABRT_SLVFLUSH_TXFIFO : ll_i2c.h
- LL_I2C_ABRT_SLVRD_INTX : ll_i2c.h
- LL_I2C_ABRT_TX_FLUSH_CNT : ll_i2c.h
- LL_I2C_ABRT_TXDATA_NOACK : ll_i2c.h
- LL_I2C_ABRT_USER_ABRT : ll_i2c.h
- LL_I2C_ADDRESSING_MODE_10BIT : ll_i2c.h
- LL_I2C_ADDRESSING_MODE_7BIT : ll_i2c.h
- LL_I2C_CMD_MST_GEN_RESTART : ll_i2c.h
- LL_I2C_CMD_MST_GEN_STOP : ll_i2c.h
- LL_I2C_CMD_MST_READ : ll_i2c.h
- LL_I2C_CMD_MST_WRITE : ll_i2c.h
- LL_I2C_CMD_SLV_NONE : ll_i2c.h
- LL_I2C_DEFAULT_CONFIG : ll_i2c.h
- LL_I2C_INTR_MASK_ACTIVITY : ll_i2c.h
- LL_I2C_INTR_MASK_ALL : ll_i2c.h
- LL_I2C_INTR_MASK_GEN_CALL : ll_i2c.h
- LL_I2C_INTR_MASK_MST_ON_HOLD : ll_i2c.h
- LL_I2C_INTR_MASK_RD_REQ : ll_i2c.h
- LL_I2C_INTR_MASK_RESTART_DET : ll_i2c.h
- LL_I2C_INTR_MASK_RX_DONE : ll_i2c.h
- LL_I2C_INTR_MASK_RX_FULL : ll_i2c.h
- LL_I2C_INTR_MASK_RX_OVER : ll_i2c.h
- LL_I2C_INTR_MASK_RX_UNDER : ll_i2c.h
- LL_I2C_INTR_MASK_SCL_STUCK_AT_LOW : ll_i2c.h
- LL_I2C_INTR_MASK_START_DET : ll_i2c.h
- LL_I2C_INTR_MASK_STOP_DET : ll_i2c.h
- LL_I2C_INTR_MASK_TX_ABRT : ll_i2c.h
- LL_I2C_INTR_MASK_TX_EMPTY : ll_i2c.h
- LL_I2C_INTR_MASK_TX_OVER : ll_i2c.h
- LL_I2C_INTR_STAT_ACTIVITY : ll_i2c.h
- LL_I2C_INTR_STAT_GEN_CALL : ll_i2c.h
- LL_I2C_INTR_STAT_MST_ON_HOLD : ll_i2c.h
- LL_I2C_INTR_STAT_RD_REQ : ll_i2c.h
- LL_I2C_INTR_STAT_RESTART_DET : ll_i2c.h
- LL_I2C_INTR_STAT_RX_DONE : ll_i2c.h
- LL_I2C_INTR_STAT_RX_FULL : ll_i2c.h
- LL_I2C_INTR_STAT_RX_OVER : ll_i2c.h
- LL_I2C_INTR_STAT_RX_UNDER : ll_i2c.h
- LL_I2C_INTR_STAT_SCL_STUCK_AT_LOW : ll_i2c.h
- LL_I2C_INTR_STAT_START_DET : ll_i2c.h
- LL_I2C_INTR_STAT_STOP_DET : ll_i2c.h
- LL_I2C_INTR_STAT_TX_ABRT : ll_i2c.h
- LL_I2C_INTR_STAT_TX_EMPTY : ll_i2c.h
- LL_I2C_INTR_STAT_TX_OVER : ll_i2c.h
- LL_I2C_OWNADDRESS_10BIT : ll_i2c.h
- LL_I2C_OWNADDRESS_7BIT : ll_i2c.h
- LL_I2C_ReadReg : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_1 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_10 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_11 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_12 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_13 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_14 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_15 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_16 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_17 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_18 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_19 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_2 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_20 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_21 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_22 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_23 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_24 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_25 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_26 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_27 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_28 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_29 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_3 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_30 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_31 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_32 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_4 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_5 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_6 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_7 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_8 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_9 : ll_i2c.h
- LL_I2C_RX_FIFO_TH_FULL : ll_i2c.h
- LL_I2C_SPEED_1000K : ll_i2c.h
- LL_I2C_SPEED_100K : ll_i2c.h
- LL_I2C_SPEED_2000K : ll_i2c.h
- LL_I2C_SPEED_400K : ll_i2c.h
- LL_I2C_SPEED_MODE_FAST : ll_i2c.h
- LL_I2C_SPEED_MODE_HIGH : ll_i2c.h
- LL_I2C_SPEED_MODE_STANDARD : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_1 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_10 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_11 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_12 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_13 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_14 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_15 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_16 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_17 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_18 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_19 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_2 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_20 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_21 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_22 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_23 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_24 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_25 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_26 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_27 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_28 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_29 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_3 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_30 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_31 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_32 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_4 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_5 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_6 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_7 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_8 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_9 : ll_i2c.h
- LL_I2C_TX_FIFO_TH_EMPTY : ll_i2c.h
- LL_I2C_WriteReg : ll_i2c.h
- LL_MSIO_DEFAULT_CONFIG : ll_msio.h
- LL_MSIO_DIRECTION_INOUT : ll_msio.h
- LL_MSIO_DIRECTION_INPUT : ll_msio.h
- LL_MSIO_DIRECTION_NONE : ll_msio.h
- LL_MSIO_DIRECTION_OUTPUT : ll_msio.h
- LL_MSIO_INPUT_POS : ll_msio.h
- LL_MSIO_INPUT_TYPE_CMOS : ll_msio.h
- LL_MSIO_INPUT_TYPE_SCHMITT : ll_msio.h
- LL_MSIO_MODE_ANALOG : ll_msio.h
- LL_MSIO_MODE_DIGITAL : ll_msio.h
- LL_MSIO_OUTPUT_POS : ll_msio.h
- LL_MSIO_PIN_0 : ll_msio.h
- LL_MSIO_PIN_1 : ll_msio.h
- LL_MSIO_PIN_2 : ll_msio.h
- LL_MSIO_PIN_3 : ll_msio.h
- LL_MSIO_PIN_4 : ll_msio.h
- LL_MSIO_PIN_5 : ll_msio.h
- LL_MSIO_PIN_6 : ll_msio.h
- LL_MSIO_PIN_7 : ll_msio.h
- LL_MSIO_PIN_8 : ll_msio.h
- LL_MSIO_PIN_9 : ll_msio.h
- LL_MSIO_PIN_ALL : ll_msio.h
- LL_MSIO_PULL_DOWN : ll_msio.h
- LL_MSIO_PULL_NO : ll_msio.h
- LL_MSIO_PULL_UP : ll_msio.h
- LL_MSIO_ReadReg : ll_msio.h
- LL_MSIO_SPEED_HIGH : ll_msio.h
- LL_MSIO_SPEED_MEDIUM : ll_msio.h
- LL_MSIO_STRENGTH_DS0_MASK : ll_msio.h
- LL_MSIO_STRENGTH_DS0_POS : ll_msio.h
- LL_MSIO_STRENGTH_DS1_MASK : ll_msio.h
- LL_MSIO_STRENGTH_DS1_POS : ll_msio.h
- LL_MSIO_STRENGTH_HIGH : ll_msio.h
- LL_MSIO_STRENGTH_LOW : ll_msio.h
- LL_MSIO_STRENGTH_MEDIUM : ll_msio.h
- LL_MSIO_STRENGTH_ULTRA : ll_msio.h
- LL_MSIO_WriteReg : ll_msio.h
- LL_PKC_BIGMULTI_BITS_LENGTH_MAX : ll_pkc.h
- LL_PKC_BITS_LENGTH_MAX : ll_pkc.h
- LL_PKC_BITS_LENGTH_MIN : ll_pkc.h
- LL_PKC_INTEN_BAOVF : ll_pkc.h
- LL_PKC_INTEN_DONE : ll_pkc.h
- LL_PKC_INTEN_ERR : ll_pkc.h
- LL_PKC_operation_mode_ADD : ll_pkc.h
- LL_PKC_operation_mode_BIGINTEGERADD : ll_pkc.h
- LL_PKC_operation_mode_BIGINTEGERMULTIPLY : ll_pkc.h
- LL_PKC_operation_mode_COMPARE : ll_pkc.h
- LL_PKC_operation_mode_INVERTION : ll_pkc.h
- LL_PKC_operation_mode_LEFTSHIFT : ll_pkc.h
- LL_PKC_operation_mode_MULTIPLY : ll_pkc.h
- LL_PKC_operation_mode_SUB : ll_pkc.h
- LL_PKC_ReadReg : ll_pkc.h
- LL_PKC_WORKSTAT_BUSY : ll_pkc.h
- LL_PKC_WriteReg : ll_pkc.h
- LL_PWM_ACTIONEVENT_CLEAR : ll_pwm.h
- LL_PWM_ACTIONEVENT_NONE : ll_pwm.h
- LL_PWM_ACTIONEVENT_SET : ll_pwm.h
- LL_PWM_ACTIONEVENT_TOGGLE : ll_pwm.h
- LL_PWM_BREATH_PRESCALER_UNIT : ll_pwm.h
- LL_PWM_CENTER_ALIGNED : ll_pwm.h
- LL_PWM_CODING_CHANNEL_A : ll_pwm.h
- LL_PWM_CODING_CHANNEL_ALL : ll_pwm.h
- LL_PWM_CODING_CHANNEL_DEFAULT_CONFIG : ll_pwm.h
- LL_PWM_CODING_DEFAULT_CONFIG : ll_pwm.h
- LL_PWM_DEFAULT_CONFIG : ll_pwm.h
- LL_PWM_DRIVEPOLARITY_NEGATIVE : ll_pwm.h
- LL_PWM_DRIVEPOLARITY_POSITIVE : ll_pwm.h
- LL_PWM_EDGE_ALIGNED : ll_pwm.h
- LL_PWM_HOLD_PRESCALER_UNIT : ll_pwm.h
- LL_PWM_NONE_CODING_CHANNEL_DEFAULT_CONFIG : ll_pwm.h
- LL_PWM_NONE_CODING_DEFAULT_CONFIG : ll_pwm.h
- LL_PWM_PRESCALER_UNIT : ll_pwm.h
- LL_PWM_ReadReg : ll_pwm.h
- LL_PWM_STOP_LVL_HIGH : ll_pwm.h
- LL_PWM_STOP_LVL_LOW : ll_pwm.h
- LL_PWM_WAITING_TIME_LVL_HIGH : ll_pwm.h
- LL_PWM_WAITING_TIME_LVL_LOW : ll_pwm.h
- LL_PWM_WriteReg : ll_pwm.h
- LL_PWR_AON_IRQ_EN_ALL : ll_pwr.h
- LL_PWR_AON_IRQ_EN_BLE_MAC : ll_pwr.h
- LL_PWR_AON_IRQ_EN_BLE_PWR_DN : ll_pwr.h
- LL_PWR_AON_IRQ_EN_BLE_PWR_ON : ll_pwr.h
- LL_PWR_AON_IRQ_EN_BOD_FALL : ll_pwr.h
- LL_PWR_AON_IRQ_EN_BOD_RISE : ll_pwr.h
- LL_PWR_AON_IRQ_EN_CPLL_DN : ll_pwr.h
- LL_PWR_AON_IRQ_EN_SLP_FAIL : ll_pwr.h
- LL_PWR_AON_IRQ_EVT_ALL : ll_pwr.h
- LL_PWR_AON_IRQ_EVT_BLE_MAC : ll_pwr.h
- LL_PWR_AON_IRQ_EVT_BLE_PWR_DN : ll_pwr.h
- LL_PWR_AON_IRQ_EVT_BLE_PWR_ON : ll_pwr.h
- LL_PWR_AON_IRQ_EVT_BOD_FALL : ll_pwr.h
- LL_PWR_AON_IRQ_EVT_BOD_RISE : ll_pwr.h
- LL_PWR_AON_IRQ_EVT_CPLL_DN : ll_pwr.h
- LL_PWR_AON_IRQ_EVT_SLP_FAIL : ll_pwr.h
- LL_PWR_DPAD_LE_OFF : ll_pwr.h
- LL_PWR_DPAD_LE_ON : ll_pwr.h
- LL_PWR_WKUP_COND_ALL : ll_pwr.h
- LL_PWR_WKUP_COND_AON_WDT : ll_pwr.h
- LL_PWR_WKUP_COND_BLE : ll_pwr.h
- LL_PWR_WKUP_COND_CLDR : ll_pwr.h
- LL_PWR_WKUP_COND_COMP_FALL : ll_pwr.h
- LL_PWR_WKUP_COND_COMP_RISE : ll_pwr.h
- LL_PWR_WKUP_COND_EXT : ll_pwr.h
- LL_PWR_WKUP_COND_TIMER : ll_pwr.h
- LL_PWR_WKUP_EVENT_ALL : ll_pwr.h
- LL_PWR_WKUP_EVENT_BLE : ll_pwr.h
- LL_PWR_WKUP_EVENT_CLDR : ll_pwr.h
- LL_PWR_WKUP_EVENT_COMP_FALL : ll_pwr.h
- LL_PWR_WKUP_EVENT_COMP_RISE : ll_pwr.h
- LL_PWR_WKUP_EVENT_EXT : ll_pwr.h
- LL_PWR_WKUP_EVENT_TIMER : ll_pwr.h
- LL_PWR_WKUP_EVENT_WDT : ll_pwr.h
- LL_RNG_IT_DISABLE : ll_rng.h
- LL_RNG_IT_ENABLE : ll_rng.h
- LL_RNG_LFSR_MODE_128BIT : ll_rng.h
- LL_RNG_LFSR_MODE_59BIT : ll_rng.h
- LL_RNG_OUTPUT_CYCLIC : ll_rng.h
- LL_RNG_OUTPUT_CYCLIC_PARITY : ll_rng.h
- LL_RNG_OUTPUT_FR0_S0 : ll_rng.h
- LL_RNG_OUTPUT_LFSR : ll_rng.h
- LL_RNG_OUTPUT_LFSR_RNG : ll_rng.h
- LL_RNG_POST_PRO_COUNTING : ll_rng.h
- LL_RNG_POST_PRO_NEUMANN : ll_rng.h
- LL_RNG_POST_PRO_NOT : ll_rng.h
- LL_RNG_POST_PRO_SKIPPING : ll_rng.h
- LL_RNG_ReadReg : ll_rng.h
- LL_RNG_SEED_FR0_S0 : ll_rng.h
- LL_RNG_SEED_USER : ll_rng.h
- LL_RNG_WriteReg : ll_rng.h
- LL_RTC_DIV_128 : ll_rtc.h
- LL_RTC_DIV_16 : ll_rtc.h
- LL_RTC_DIV_2 : ll_rtc.h
- LL_RTC_DIV_32 : ll_rtc.h
- LL_RTC_DIV_4 : ll_rtc.h
- LL_RTC_DIV_64 : ll_rtc.h
- LL_RTC_DIV_8 : ll_rtc.h
- LL_RTC_DIV_NONE : ll_rtc.h
- LL_RTC_TIMER_TICK_TYPE_AUTO : ll_rtc.h
- LL_RTC_TIMER_TICK_TYPE_SINGLE : ll_rtc.h
- LL_SLEEP_TIMER_AUTO_MODE : ll_sleep_timer.h
- LL_SLEEP_TIMER_SINGLE_MODE_0 : ll_sleep_timer.h
- LL_SLEEP_TIMER_SINGLE_MODE_1 : ll_sleep_timer.h
- LL_SLOW_CLK_RC : ll_clk.h
- LL_SLOW_CLK_RNG : ll_clk.h
- LL_SLOW_CLK_RTC : ll_clk.h
- LL_SLP_TIMER_ReadReg : ll_sleep_timer.h
- LL_SLP_TIMER_WriteReg : ll_sleep_timer.h
- LL_SPI_DATASIZE_10BIT : ll_spi.h
- LL_SPI_DATASIZE_11BIT : ll_spi.h
- LL_SPI_DATASIZE_12BIT : ll_spi.h
- LL_SPI_DATASIZE_13BIT : ll_spi.h
- LL_SPI_DATASIZE_14BIT : ll_spi.h
- LL_SPI_DATASIZE_15BIT : ll_spi.h
- LL_SPI_DATASIZE_16BIT : ll_spi.h
- LL_SPI_DATASIZE_17BIT : ll_spi.h
- LL_SPI_DATASIZE_18BIT : ll_spi.h
- LL_SPI_DATASIZE_19BIT : ll_spi.h
- LL_SPI_DATASIZE_20BIT : ll_spi.h
- LL_SPI_DATASIZE_21BIT : ll_spi.h
- LL_SPI_DATASIZE_22BIT : ll_spi.h
- LL_SPI_DATASIZE_23BIT : ll_spi.h
- LL_SPI_DATASIZE_24BIT : ll_spi.h
- LL_SPI_DATASIZE_25BIT : ll_spi.h
- LL_SPI_DATASIZE_26BIT : ll_spi.h
- LL_SPI_DATASIZE_27BIT : ll_spi.h
- LL_SPI_DATASIZE_28BIT : ll_spi.h
- LL_SPI_DATASIZE_29BIT : ll_spi.h
- LL_SPI_DATASIZE_30BIT : ll_spi.h
- LL_SPI_DATASIZE_31BIT : ll_spi.h
- LL_SPI_DATASIZE_32BIT : ll_spi.h
- LL_SPI_DATASIZE_4BIT : ll_spi.h
- LL_SPI_DATASIZE_5BIT : ll_spi.h
- LL_SPI_DATASIZE_6BIT : ll_spi.h
- LL_SPI_DATASIZE_7BIT : ll_spi.h
- LL_SPI_DATASIZE_8BIT : ll_spi.h
- LL_SPI_DATASIZE_9BIT : ll_spi.h
- LL_SPI_DMA_RX_DIS : ll_spi.h
- LL_SPI_DMA_RX_EN : ll_spi.h
- LL_SPI_DMA_TX_DIS : ll_spi.h
- LL_SPI_DMA_TX_EN : ll_spi.h
- LL_SPI_FULL_DUPLEX : ll_spi.h
- LL_SPI_IM_MST : ll_spi.h
- LL_SPI_IM_RXF : ll_spi.h
- LL_SPI_IM_RXO : ll_spi.h
- LL_SPI_IM_RXU : ll_spi.h
- LL_SPI_IM_TXE : ll_spi.h
- LL_SPI_IM_TXO : ll_spi.h
- LL_SPI_IS_MST : ll_spi.h
- LL_SPI_IS_RXF : ll_spi.h
- LL_SPI_IS_RXO : ll_spi.h
- LL_SPI_IS_RXU : ll_spi.h
- LL_SPI_IS_TXE : ll_spi.h
- LL_SPI_IS_TXO : ll_spi.h
- LL_SPI_M_FIFO_DEPTH : ll_spi.h
- LL_SPI_MICROWIRE_HANDSHAKE_DIS : ll_spi.h
- LL_SPI_MICROWIRE_HANDSHAKE_EN : ll_spi.h
- LL_SPI_MICROWIRE_NON_SEQUENTIAL : ll_spi.h
- LL_SPI_MICROWIRE_RX : ll_spi.h
- LL_SPI_MICROWIRE_SEQUENTIAL : ll_spi.h
- LL_SPI_MICROWIRE_TX : ll_spi.h
- LL_SPI_MW_CMDSIZE_10BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_11BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_12BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_13BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_14BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_15BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_16BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_1BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_2BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_3BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_4BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_5BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_6BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_7BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_8BIT : ll_spi.h
- LL_SPI_MW_CMDSIZE_9BIT : ll_spi.h
- LL_SPI_NORMAL_MODE : ll_spi.h
- LL_SPI_PROTOCOL_MICROWIRE : ll_spi.h
- LL_SPI_PROTOCOL_MOTOROLA : ll_spi.h
- LL_SPI_PROTOCOL_TI : ll_spi.h
- LL_SPI_READ_EEPROM : ll_spi.h
- LL_SPI_ReadReg : ll_spi.h
- LL_SPI_RIS_MST : ll_spi.h
- LL_SPI_RIS_RXF : ll_spi.h
- LL_SPI_RIS_RXO : ll_spi.h
- LL_SPI_RIS_RXU : ll_spi.h
- LL_SPI_RIS_TXE : ll_spi.h
- LL_SPI_RIS_TXO : ll_spi.h
- LL_SPI_S_FIFO_DEPTH : ll_spi.h
- LL_SPI_SCPHA_1EDGE : ll_spi.h
- LL_SPI_SCPHA_2EDGE : ll_spi.h
- LL_SPI_SCPOL_HIGH : ll_spi.h
- LL_SPI_SCPOL_LOW : ll_spi.h
- LL_SPI_SIMPLEX_RX : ll_spi.h
- LL_SPI_SIMPLEX_TX : ll_spi.h
- LL_SPI_SLAVE0 : ll_spi.h
- LL_SPI_SLAVE1 : ll_spi.h
- LL_SPI_SLAVE_OUTDIS : ll_spi.h
- LL_SPI_SLAVE_OUTEN : ll_spi.h
- LL_SPI_SR_BUSY : ll_spi.h
- LL_SPI_SR_DCOL : ll_spi.h
- LL_SPI_SR_RFF : ll_spi.h
- LL_SPI_SR_RFNE : ll_spi.h
- LL_SPI_SR_TFE : ll_spi.h
- LL_SPI_SR_TFNF : ll_spi.h
- LL_SPI_SR_TXE : ll_spi.h
- LL_SPI_TEST_MODE : ll_spi.h
- LL_SPI_WriteReg : ll_spi.h
- LL_SPIM_DEFAULT_CONFIG : ll_spi.h
- LL_SPIS_DEFAULT_CONFIG : ll_spi.h
- LL_TIMER_INTSTAT_BLEPULSE1 : ll_tim.h
- LL_TIMER_INTSTAT_BLEPULSE2 : ll_tim.h
- LL_TIMER_INTSTAT_CH0 : ll_tim.h
- LL_TIMER_INTSTAT_CH1 : ll_tim.h
- LL_TIMER_INTSTAT_CH2 : ll_tim.h
- LL_TIMER_INTSTAT_CH3 : ll_tim.h
- LL_TIMER_INTSTAT_COUNTDONE : ll_tim.h
- LL_TIMER_ReadReg : ll_tim.h
- LL_TIMER_WriteReg : ll_tim.h
- LL_UART_CTSPIN_STATE_ACTIVE : ll_uart.h
- LL_UART_CTSPIN_STATE_INACTIVE : ll_uart.h
- LL_UART_DATABITS_5B : ll_uart.h
- LL_UART_DATABITS_6B : ll_uart.h
- LL_UART_DATABITS_7B : ll_uart.h
- LL_UART_DATABITS_8B : ll_uart.h
- LL_UART_DEFAULT_CONFIG : ll_uart.h
- LL_UART_HWCONTROL_NONE : ll_uart.h
- LL_UART_HWCONTROL_RTS_CTS : ll_uart.h
- LL_UART_IER_MS : ll_uart.h
- LL_UART_IER_RDA : ll_uart.h
- LL_UART_IER_RLS : ll_uart.h
- LL_UART_IER_THRE : ll_uart.h
- LL_UART_IIR_CTO : ll_uart.h
- LL_UART_IIR_MS : ll_uart.h
- LL_UART_IIR_NIP : ll_uart.h
- LL_UART_IIR_RDA : ll_uart.h
- LL_UART_IIR_RLS : ll_uart.h
- LL_UART_IIR_THRE : ll_uart.h
- LL_UART_LSR_BI : ll_uart.h
- LL_UART_LSR_FE : ll_uart.h
- LL_UART_LSR_OE : ll_uart.h
- LL_UART_LSR_PE : ll_uart.h
- LL_UART_LSR_RFE : ll_uart.h
- LL_UART_LSR_TEMT : ll_uart.h
- LL_UART_LSR_THRE : ll_uart.h
- LL_UART_PARITY_EVEN : ll_uart.h
- LL_UART_PARITY_NONE : ll_uart.h
- LL_UART_PARITY_ODD : ll_uart.h
- LL_UART_PARITY_SP0 : ll_uart.h
- LL_UART_PARITY_SP1 : ll_uart.h
- LL_UART_ReadReg : ll_uart.h
- LL_UART_RTSPIN_STATE_ACTIVE : ll_uart.h
- LL_UART_RTSPIN_STATE_INACTIVE : ll_uart.h
- LL_UART_RX_FIFO_TH_CHAR_1 : ll_uart.h
- LL_UART_RX_FIFO_TH_FULL_2 : ll_uart.h
- LL_UART_RX_FIFO_TH_HALF_FULL : ll_uart.h
- LL_UART_RX_FIFO_TH_QUARTER_FULL : ll_uart.h
- LL_UART_STOPBITS_1 : ll_uart.h
- LL_UART_STOPBITS_1_5 : ll_uart.h
- LL_UART_STOPBITS_2 : ll_uart.h
- LL_UART_TX_FIFO_TH_CHAR_2 : ll_uart.h
- LL_UART_TX_FIFO_TH_EMPTY : ll_uart.h
- LL_UART_TX_FIFO_TH_HALF_FULL : ll_uart.h
- LL_UART_TX_FIFO_TH_QUARTER_FULL : ll_uart.h
- LL_UART_USR_RFF : ll_uart.h
- LL_UART_USR_RFNE : ll_uart.h
- LL_UART_USR_TFE : ll_uart.h
- LL_UART_USR_TFNF : ll_uart.h
- LL_UART_WriteReg : ll_uart.h
- LL_XQSPI_BAUD_RATE_16M : ll_xqspi.h
- LL_XQSPI_BAUD_RATE_24M : ll_xqspi.h
- LL_XQSPI_BAUD_RATE_32M : ll_xqspi.h
- LL_XQSPI_BAUD_RATE_48M : ll_xqspi.h
- LL_XQSPI_BAUD_RATE_64M : ll_xqspi.h
- LL_XQSPI_CACHE_DIRECT_MAP_DIS : ll_xqspi.h
- LL_XQSPI_CACHE_DIRECT_MAP_EN : ll_xqspi.h
- LL_XQSPI_CACHE_DIS : ll_xqspi.h
- LL_XQSPI_CACHE_EN : ll_xqspi.h
- LL_XQSPI_CACHE_FIFO_CLEAR : ll_xqspi.h
- LL_XQSPI_CACHE_FIFO_NORMAL : ll_xqspi.h
- LL_XQSPI_CACHE_FLUSH_DIS : ll_xqspi.h
- LL_XQSPI_CACHE_FLUSH_EN : ll_xqspi.h
- LL_XQSPI_CACHE_HITMISS_CLEAR : ll_xqspi.h
- LL_XQSPI_CACHE_HITMISS_NORMAL : ll_xqspi.h
- LL_XQSPI_DEFAULT_CONFIG : ll_xqspi.h
- LL_XQSPI_DISABLE_PRESENT : ll_xqspi.h
- LL_XQSPI_ENABLE_PRESENT : ll_xqspi.h
- LL_XQSPI_FLASH_WRITE_128BIT : ll_xqspi.h
- LL_XQSPI_FLASH_WRITE_32BIT : ll_xqspi.h
- LL_XQSPI_HP_MODE_DIS : ll_xqspi.h
- LL_XQSPI_HP_MODE_EN : ll_xqspi.h
- LL_XQSPI_MODE_QSPI : ll_xqspi.h
- LL_XQSPI_MODE_XIP : ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_12BIT : ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_16BIT : ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_20BIT : ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_24BIT : ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_28BIT : ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_32BIT : ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_4BIT : ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_8BIT : ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_DEPTH : ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_2 : ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_4 : ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_8 : ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_3_4 : ll_xqspi.h
- LL_XQSPI_QSPI_FRF_DUALSPI : ll_xqspi.h
- LL_XQSPI_QSPI_FRF_QUADSPI : ll_xqspi.h
- LL_XQSPI_QSPI_FRF_SPI : ll_xqspi.h
- LL_XQSPI_QSPI_IM_DONE : ll_xqspi.h
- LL_XQSPI_QSPI_IM_RFF : ll_xqspi.h
- LL_XQSPI_QSPI_IM_RFTF : ll_xqspi.h
- LL_XQSPI_QSPI_IM_TFE : ll_xqspi.h
- LL_XQSPI_QSPI_IM_TFTF : ll_xqspi.h
- LL_XQSPI_QSPI_IS_DONE : ll_xqspi.h
- LL_XQSPI_QSPI_IS_RFF : ll_xqspi.h
- LL_XQSPI_QSPI_IS_RFTF : ll_xqspi.h
- LL_XQSPI_QSPI_IS_TFE : ll_xqspi.h
- LL_XQSPI_QSPI_IS_TFTF : ll_xqspi.h
- LL_XQSPI_QSPI_LSB : ll_xqspi.h
- LL_XQSPI_QSPI_MSB : ll_xqspi.h
- LL_XQSPI_QSPI_STAT_BUSY : ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFE : ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFF : ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFTF : ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFE : ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFF : ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFTF : ll_xqspi.h
- LL_XQSPI_ReadReg : ll_xqspi.h
- LL_XQSPI_SCPHA_1EDGE : ll_xqspi.h
- LL_XQSPI_SCPHA_2EDGE : ll_xqspi.h
- LL_XQSPI_SCPOL_HIGH : ll_xqspi.h
- LL_XQSPI_SCPOL_LOW : ll_xqspi.h
- LL_XQSPI_WriteReg : ll_xqspi.h
- LL_XQSPI_XIP_ADDR_3BYTES : ll_xqspi.h
- LL_XQSPI_XIP_ADDR_4BYTES : ll_xqspi.h
- LL_XQSPI_XIP_CMD_DUAL_IO_READ : ll_xqspi.h
- LL_XQSPI_XIP_CMD_DUAL_OUT_READ : ll_xqspi.h
- LL_XQSPI_XIP_CMD_FAST_READ : ll_xqspi.h
- LL_XQSPI_XIP_CMD_QUAD_IO_READ : ll_xqspi.h
- LL_XQSPI_XIP_CMD_QUAD_OUT_READ : ll_xqspi.h
- LL_XQSPI_XIP_CMD_READ : ll_xqspi.h
- LL_XQSPI_XIP_ENDIAN_BIG : ll_xqspi.h
- LL_XQSPI_XIP_ENDIAN_LITTLE : ll_xqspi.h
- LL_XQSPI_XIP_SS0 : ll_xqspi.h
- LL_XQSPI_XIP_SS1 : ll_xqspi.h
- LL_XQSPI_XIP_SS2 : ll_xqspi.h
- LL_XQSPI_XIP_SS3 : ll_xqspi.h
- LLS_C_CONNECTION_MAX : lls_c.h
- LMS_CONNECTION_MAX : lms.h
- LMS_MAX_DATA_LEN : lms.h
- LMS_PATTERN_VALUE : lms.h
- LMS_SERVICE_UUID : lms.h
- LNS_CONNECTION_MAX : lns.h
- LNS_LOG_CTRL_PT_VAL_LEN : lns.h
- LNS_LOG_INFO_VAL_LEN : lns.h
- LNS_SERVICE_UUID : lns.h
- LOCAL_INT_DISABLE : gr_common.h
- LOCAL_INT_RESTORE : gr_common.h
- LOW_POWER_MODE_ENABLE : gr5405_feat.h