Data Structures
Here are the classes, structs, unions and interfaces with brief descriptions:
[detail level 1 2]

C__attribute__ |
C_adc_handle | ADC handle Structure definition
C_aes_handle | AES handle Structure definition
C_aes_init | AES Init Structure definition
C_alarm_handle_t | Alarm handle params
C_aon_gpio_init | AON_GPIO init structure definition
C_aon_wdt_handle | AON_WDT handle Structure definition
C_aon_wdt_init | AON_WDT_Configuration init structure definition
C_bod_handle | BOD handle Structure definition
C_calendar_alarm | CALENDAR alarm structure definition
C_calendar_handle | CALENDAR handle structure definition
C_calendar_time | CALENDAR time structure definition
C_cgc_init | CGC init structure definition
C_comp_handle | COMP handle Structure definition
C_dma_handle | DMA handle Structure definition
C_dma_init | DMA Configuration Structure definition
C_dma_lock_config | DMA LOCK Structure definition
C_dual_timer_handle | DUAL_TIMER handle Structure definition
C_dual_timer_init | DUAL TIMER init Structure definition
C_dual_timer_io_ctrl_cfg | DUAL TIMER io crtl config Structure definition
C_efuse_handle | EFuse handle Structure definition
C_exflash_timing_param | ExFlash AC characteristics
C_hal_adc_callback | HAL ADC Callback function definition
C_hal_aes_callback | HAL AES Callback function definition
C_hal_aon_gpio_callback | HAL AON_GPIO Callback function definition
C_hal_aon_wdt_callback | HAL_AON_WDT Callback function definition
C_hal_bod_callback | HAL BOD Callback function definition
C_hal_calendar_callback | CALENDAR callback function definition
C_hal_comp_callback | HAL COMP Callback function definition
C_hal_dual_timer_callback | HAL_DUAL_TIMER Callback function definition
C_hal_efuse_callback | HAL_EFUSE Callback function definition
C_hal_hmac_callback | HAL_HMAC Callback function definition
C_hal_i2c_callback | HAL_I2C Callback function definition
C_hal_msio_callback | HAL_MSIO Callback function definition
C_hal_pkc_callback | HAL_PKC Callback function definition
C_hal_pwm_callback | HAL_PWM Callback function definition
C_hal_rng_callback | HAL_RNG Callback function definition
C_hal_rtc_callback | HAL_RTC Callback function definition
C_hal_spi_callback | HAL_SPI Callback function definition
C_hal_timer_base_callback | HAL_TIMER Callback function definition
C_hal_timer_capture_channel_init | TIMER capture channel Structure definition
C_hal_uart_callback | HAL_UART Callback function definition
C_hal_xqspi_callback | HAL_XQSPI Callback function definition
C_hmac_handle | HMAC handle Structure definition
C_hmac_init | HMAC init Structure definition
C_i2c_handle | I2C handle Structure definition
C_i2c_init | I2C Configuration Structure definition
C_ll_adc_init | LL ADC init Structure definition
C_ll_aes_init | LL AES Init Structure definition
C_ll_aon_gpio_init | LL AON_GPIO init Structure definition
C_ll_bod_init | LL BOD init Structure definition
C_ll_comp_init | LL COMP init Structure definition
C_ll_dma_init | LL DMA init Structure definition
C_ll_ecc_curve_init | LL PKC ECC P-256 Elliptic Curve Init Structure definition
C_ll_ecc_point | LL PKC ECC Point Structure definition
C_ll_gpio_init | LL GPIO init configuration definition
C_ll_hmac_init_t | LL HMAC Init Structure definition
C_ll_i2c_init | LL I2C init Structure definition
C_ll_pkc_init | LL PKC Init Structure definition
C_ll_pwm_coding_channel_init_t | LL PWM Output Channel init Structure definition
C_ll_pwm_coding_mode_init_t | LL PWM coding mode Structure definition
C_ll_pwm_init_t | LL PWM init Structure definition
C_ll_pwm_none_coding_channel_init_t | LL PWM Output Channel init Structure definition
C_ll_pwm_none_coding_mode_init_t | LL PWM none coding mode Structure definition
C_ll_spim_init_t | LL SPIM init structures definition
C_ll_spis_init_t | SPIS init structures definition
C_ll_timer_capture_channel_init | LL TIMER capture channel Structure definition
C_ll_timer_init_t | LL TIMER init Structure definition
C_ll_uart_init_t | LL UART init Structure definition
C_ll_xqspi_hp_init_t | XQSPI High Performance mode init structures definition
C_ll_xqspi_init_t | XQSPI init structures definition
C_pkc_big_number_add | PKC Big Number Addition expression input
C_pkc_big_number_multi | PKC Big Number Multiplication expression input
C_pkc_ecc_point_multi | PKC ECC Point Multiplication expression input
C_pkc_handle | PKC handle Structure definition
C_pkc_modular_add | PKC Modular Addition expression input
C_pkc_modular_compare | PKC Modular Comparison expression input
C_pkc_modular_shift | PKC Modular Left Shift expression input
C_pkc_modular_sub | PKC Modular Subtraction expression input
C_pkc_montgomery_inversion | PKC Montgomery Inversion expression input
C_pkc_montgomery_multi | PKC Montgomery Modular Multiplication expression input
C_pkc_rsa_modular_exponent | PKC RSA Modular Exponentiation expression input
C_pwr_handler | PWR callback handle Structure definition
C_rng_handle | RNG handle Structure definition
C_rng_init | RNG init structure definition
C_rtc_handle_t | Rtc handle definition
C_spi_handle | SPI handle Structure definition
C_spi_init | SPI init Structure definition
C_timer_handle | TIMER handle Structure definition
C_timer_init | TIMER init Structure definition
C_uart_handle | UART handle Structure definition
C_uart_init | UART init structure definition
C_xqspi_command_t | XQSPI command Structure definition
C_xqspi_handle_t | XQSPI handle Structure definition
C_xqspi_init_t | XQSPI init Structure definition
C adc_env_t | ADC device structure definition
C adc_trim_info_t | ADC trim parameter information definition
C ags_ack_packet_t | Alexa Gadget Service ACK packet
C ags_evt_t | Alexa Gadget Service event
C ags_header_base_t | Alexa Gadget Service base part of data packet header
C ags_header_first_ext_t | Alexa Gadget Service extended version of header in first packet
C ags_header_first_t | Alexa Gadget Service header in first packet
C ags_header_subs_ext_t | Alexa Gadget Service extended version of header in subsequent packets
C ags_header_subs_t | Alexa Gadget Service header in subsequent packets
C ags_init_t | Alexa Gadget Service init stucture. This contains all option and data needed for initialization of the service
C ags_stream_env_t | Alexa Gadget Service gadget stream enviorenment variable
C ams_c_attr_info_t | Structure that stores attribute information
C ams_c_cmd_list_t | Structure that stores new command list
C ams_c_cplt_attr_data_t | Complete attribution's value
C ams_c_ett_attr_id_t | Structure that stores the attribute to be concerned or to display completely
C ams_c_evt_t | Apple Media Service Client event
C ams_c_handles_t | Handles on the connected peer device needed to interact with it
C ancs_c_att_handles_t | Ancs handle structure
C ancs_c_evt_t | ANCS Client event
C ancs_ntf_flags_t | Notification flags that can be performed for iOS notifications
C ans_c_ctrl_pt_t | Alert Notification Service Client Control Point value
C ans_c_evt_t | Alert Notification Service Client event
C ans_c_handles_t | Handles on the connected peer device needed to interact with it
C ans_c_new_alert_t | Alert Notification Service Client decoded New Alert value
C ans_c_unread_alert_t | Alert Notification Service Client decoded Unread Alert Status value
C ans_ctrl_pt_t | Alert Notification Service Control Point value
C ans_evt_t | Alert Notification Service event
C ans_init_t | Alert Notification Service init stucture. This contains all options and data needed for initialization of the service
C ans_new_alert_t | Alert Notification Service New Alert value
C ans_unread_alert_t | Alert Notification Service Unread Alert Status value
C aon_aon_wdt_env_t | AON_WDT device structure definition
C app_adc_dma_cfg_t | ADC DMA configuration Structures
C app_adc_evt_t | ADC event structure definition
C app_adc_params_t | ADC parameters structure definition
C app_adc_pin_cfg_t | ADC pins config Structures
C app_adc_pin_t | ADC pins Structures
C app_aon_wdt_params_t | AON_WDT parameters structure definition
C app_bod_evt_t | BOD event structure definition
C app_bod_params_t | BOD parameters structure definition
C app_comp_params_t | COMP parameters structure definition
C app_comp_pin_cfg_t | COMP pins config Structures
C app_comp_pin_t | COMP pins Structures
C app_dma_params_t | DMA parameters structure definition
C app_dual_tim_params_t | DUAL_TIM parameters structure definition
C app_gpiote_param_t | GPIOTE Interrupt parameters structure definition
C app_i2c_dma_cfg_t | I2C operate mode Enumerations definition
C app_i2c_evt_t | I2C event structure definition
C app_i2c_params_t | I2C parameters structure definition
C app_i2c_pin_cfg_t | I2C pins config Structures
C app_i2c_pin_t | I2C pins Structures
C app_io_evt_t | GPIO Interrupt event Structure definition
C app_io_init_t | GPIO parameter structure definition
C app_pwm_channel_init_t | PWM Channel init Structure definition
C app_pwm_params_t | PWM parameters structure definition
C app_pwm_pin_cfg_t | PWM configuration Structures
C app_pwm_pin_t | PWM IO configuration Structures
C app_rng_evt_t | RNG event structure definition
C app_rng_params_t | RNG parameters structure definition
C app_rtc_evt_t | RTC event structure definition
C app_sleep_callbacks_t | PWR sleep check function Structure
C app_spi_dma_cfg_t | SPI configuration definition
C app_spi_evt_t | SPI event structure definition
C app_spi_params_t | SPI parameters structure definition
C app_spi_pin_cfg_t | SPI IO configuration Structures
C app_spi_pin_t | SPI IO Structures
C app_spi_screen_config_t | SPI SCreen Config Structures
C app_tim_params_t | TIM parameters structure definition
C app_uart_dma_cfg_t | UART DMA configuration structure definition
C app_uart_evt_t | UART event structure definition
C app_uart_params_t | UART parameters structure definition
C app_uart_pin_cfg_t | UART pins config Structures
C app_uart_pin_t | UART pins Structures
C app_uart_tx_buf_t | UART buffer structure definition
C bas_c_evt_t | Battery Service Client event
C bas_c_handles_t | Handles on the connected peer device needed to interact with it
C bas_evt_t | Battery Service event
C bas_init_t | Battery Service init structure. This contains all options and data needed for initialization of the service
C bcs_evt_t | Body Composition Service event
C bcs_init_t | Body Composition Service Init variable
C bcs_meas_flag_t | Body composition Measurement flag data
C bcs_meas_val_t | Body composition Measurement data
C birth_date_t | UDS Characteristic - birthdate's structure
C ble_dis_c_read_rsp_t | Device Information Service Client Read Response encode structure
C ble_evt_t | BLE Event Information
C ble_ext_llcp_cb_func_t | Extended LLCP
C ble_gap_addr_t | The struct of address
C ble_gap_adv_param_t | Advertising parameters for legacy advertising
C ble_gap_adv_period_cfg_t | Configuration for periodic advertising
C ble_gap_adv_prim_cfg_t | Configuration for advertising on primary channel
C ble_gap_adv_second_cfg_t | Configuration for advertising on secondary channel
C ble_gap_adv_time_param_t | Advertising timing parameter
C ble_gap_bdaddr_t | The struct of broadcast address with broadcast type
C ble_gap_bond_dev_list_t | Bonded device list
C ble_gap_chnl_map_t | Channel map structure
C ble_gap_con_plan_tag_t | The Structure for BLE Connection Arrangement
C ble_gap_conn_info_param_t | The info of connecting operation
C ble_gap_conn_info_t | Connection info
C ble_gap_conn_iq_report_t | Connection IQ Report info
C ble_gap_conn_param_t | The parameter of connection
C ble_gap_conn_update_cmp_t | Connection parameter used to update connection parameters
C ble_gap_conn_update_param_t | The parameter of update connection
C ble_gap_connless_iq_report_t | Connectionless IQ Report info
C ble_gap_connless_iq_sample_param_t | Set connectionless IQ sampling enable parameter
C ble_gap_dev_name_ind_t | GAP Device name struct
C ble_gap_evt_adv_report_t | Advertising report event for BLE_GAPM_EVT_ADV_REPORT
C ble_gap_evt_adv_stop_t | Advertising Stop info
C ble_gap_evt_conn_info_t | Get Connection info event for BLE_GAPC_EVT_CONN_INFO_GOT
C ble_gap_evt_conn_iq_report_t | Connection IQ Report info event for BLE_GAPC_EVT_CONNECT_IQ_REPORT
C ble_gap_evt_conn_param_update_req_t | Connection parameter update request event for BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ
C ble_gap_evt_conn_param_updated_t | Connection parameter updated event for BLE_GAPC_EVT_CONN_PARAM_UPDATED
C ble_gap_evt_connected_t | Connection complete event for BLE_GAPC_EVT_CONNECTED
C ble_gap_evt_connless_iq_report_t | Connectionless IQ Report info event for BLE_GAPC_EVT_CONNECTLESS_IQ_REPORT
C ble_gap_evt_data_length_t | Data Length Updated event for BLE_GAPC_EVT_DATA_LENGTH_UPDATED
C ble_gap_evt_dev_info_set_t | Device Information set event for BLE_GAPC_EVT_DEV_INFO_SET
C ble_gap_evt_disconnected_t | Disconnection event for BLE_GAPC_EVT_DISCONNECTED
C ble_gap_evt_dtm_test_end_report_t |
C ble_gap_evt_iden_addr_report_t | Identity address report event for BLE_GAPM_EVT_IDEN_ADDR_REPORT
C ble_gap_evt_le_event_noti_report_t | Le event notification reporting info event for BLE_GAPC_EVT_LE_EVT_NOTI_REPORT
C ble_gap_evt_peer_info_t | Get peer info event for BLE_GAPC_EVT_PEER_INFO_GOT
C ble_gap_evt_peer_name_get_t | Name of peer device indication event for BLE_GAPC_EVT_PEER_NAME_GOT
C ble_gap_evt_phy_update_t | PHY update event for BLE_GAPC_EVT_PHY_UPDATED
C ble_gap_evt_rslv_addr_report_t | Resolvable address report event for BLE_GAPM_EVT_RSLV_ADDR_REPORT
C ble_gap_evt_scan_req_t | Scan request info
C ble_gap_evt_scan_stop_t | Scan Stop info struct
C ble_gap_evt_sync_established_t | Sync established event for BLE_GAPM_EVT_SYNC_ESTABLISH
C ble_gap_ext_adv_param_t | Advertising parameters for extended advertising and periodic advertising
C ble_gap_ext_adv_report_ind_t | APP receives the extended advertising report indication info struct
C ble_gap_ext_conn_param_t | Connection parameters
C ble_gap_ext_init_param_t | Extended initiating parameters
C ble_gap_ext_scan_param_t | Parameters for extended scanning
C ble_gap_init_param_t | Legacy initiating parameters
C ble_gap_le_phy_ind_t | PHY info
C ble_gap_le_pkt_size_ind_t | Supported data length size Indication
C ble_gap_lepsm_register_t | LE Protocol/Service Multiplexer information
C ble_gap_peer_features_ind_t | LE features info
C ble_gap_peer_info_param_t | Get peer info operation struct
C ble_gap_peer_info_t | LE peer info
C ble_gap_peer_version_ind_t | Peer version info
C ble_gap_per_sync_param_t | Periodic advertising synchronization parameters
C ble_gap_per_sync_trans_param_t | Default periodic advertising synchronization transfer parameters
C ble_gap_period_adv_addr_cfg_t | Periodic advertising information
C ble_gap_period_adv_list_t | Periodic advertising list
C ble_gap_ral_dev_info_t | RPA list item info
C ble_gap_ral_dev_list_t | RPA list info
C ble_gap_scan_param_t | Parameters for legacy scanning
C ble_gap_scan_wd_op_param_t | Scan Window operation parameters
C ble_gap_sec_key_t | Security key
C ble_gap_set_conn_cte_rcv_param_t | Set connection CTE receive parameters info
C ble_gap_set_conn_cte_req_enable_t | Set connection CTE Request enable info
C ble_gap_set_conn_cte_trans_param_t | Set connection CTE transmit parameters info
C ble_gap_set_path_loss_report_param_t | Set path loss reporting parameter info
C ble_gap_set_pref_slave_evt_dur_param_t | Set preference slave event duration
C ble_gap_sync_established_ind_t | Sync established indication
C ble_gap_white_list_t | White list
C ble_gapc_evt_t | BLE GAPC event structure
C ble_gapc_set_dev_info_t | Device information data struct
C ble_gapm_evt_t | BLE GAPM event structure
C ble_gatt_common_evt_mtu_exchange_t | GATT MTU Exchange event for BLE_GATT_COMMON_EVT_MTU_EXCHANGE
C ble_gatt_common_evt_prf_reg_t | GATT Server Profile Register event for BLE_GATT_COMMON_EVT_PRF_REGISTER
C ble_gatt_common_evt_t | GATT Common structure
C ble_gattc_browse_attr_char_t | GATTC Browse information about Characteristic
C ble_gattc_browse_attr_info | GATTC Browse attribute information
C ble_gattc_browse_attr_t | GATTC Browse information about Attribute
C ble_gattc_browse_inc_srvc_t | GATTC Browse information about Included Service
C ble_gattc_browse_srvc_t | GATTC Browse service(s) indication
C ble_gattc_char_desc_disc_t | GATT characteristic descriptor discovery
C ble_gattc_char_disc_t | GATT characteristic discovery
C ble_gattc_char_t | GATT characteristic
C ble_gattc_desc_t | GATT descriptor
C ble_gattc_disc_char_t | GATTC discovery characteristic structure
C ble_gattc_evt_browse_srvc_t | GATTC Browse service(s) event for BLE_GATTC_EVT_SRVC_BROWSE
C ble_gattc_evt_char_desc_disc_t | GATT characteristic descriptor discovery event for BLE_GATTC_EVT_CHAR_DESC_DISC
C ble_gattc_evt_char_disc_t | GATT characteristic discovery event for BLE_GATTC_EVT_CHAR_DISC
C ble_gattc_evt_incl_disc_t | GATT include discovery event for BLE_GATTC_EVT_INCLUDE_SRVC_DISC
C ble_gattc_evt_ntf_ind_t | GATTC Notification and Indication event for BLE_GATTC_EVT_NTF_IND
C ble_gattc_evt_prf_reg_t | GATTC profile register event for BLE_GATTC_EVT_PRIMARY_SRVC_DISC
C ble_gattc_evt_read_t | GATT Client Read response event for BLE_GATTC_EVT_READ_RSP
C ble_gattc_evt_srvc_disc_t | GATT service discovery event for BLE_GATTC_EVT_PRIMARY_SRVC_DISC
C ble_gattc_evt_t | BLE GATTC event structure
C ble_gattc_evt_write_t | GATT Client Write Response event for BLE_GATTC_EVT_WRITE_RSP
C ble_gattc_incl_disc_t | GATT include discovery
C ble_gattc_include_t | GATT include
C ble_gattc_multiple_att_t | Read Multiple Handles
C ble_gattc_ntf_ind_t | GATTC Notification and Indication value indication
C ble_gattc_read_by_uuid_t | GATTC read by characteristic UUID structure
C ble_gattc_read_multiple_t | GATTC Read Multiple
C ble_gattc_read_rsp_t | GATT value Read response
C ble_gattc_read_value_t | GATT Client Read value
C ble_gattc_service_t | GATT service
C ble_gattc_srvc_disc_t | GATT service discovery
C ble_gattc_write_attr_value_t | GATTC write attribute value structure
C ble_gattc_write_no_resp_t | GATTC write without response structure
C ble_gattc_write_t | GATT Client Write
C ble_gatts_attm_desc_128_t | Service(128 bits UUID) description
C ble_gatts_attm_desc_t | Service(16-bit UUID) description
►C ble_gatts_create_db_t | Parameter of Added service description
C attribute_table |
C ble_gatts_evt_cccd_rec_t | Gatt cccd recovery event for BLE_GATTS_EVT_CCCD_RECOVERY
C ble_gatts_evt_inited_ind_t | GATTS Database Inited Indication event structure
C ble_gatts_evt_ntf_ind_t | Gatt Notification or indication event for BLE_GATTS_EVT_NTF_IND
C ble_gatts_evt_prep_write_t | GATT prepare write request event for BLE_GATTS_EVT_PREP_WRITE_REQUEST
C ble_gatts_evt_read_t | GATT read request event for BLE_GATTS_EVT_READ_REQUEST
C ble_gatts_evt_t | BLE GATTS event structure
C ble_gatts_evt_write_t | GATT write request event for BLE_GATTS_EVT_WRITE_REQUEST
C ble_gatts_noti_ind_t | GATT sending Notification or Indication event param description
C ble_gatts_ntf_ind_t | GATTS Operation Complete event structure
C ble_gatts_prep_write_cfm_t | GATT prepare write result description
C ble_gatts_read_cfm_t | GATT read attribute result description
C ble_gatts_write_cfm_t | GATT write attribute result description
C ble_hci_rx_channel_t | BLE HCI RX Channel (Host send packet to controller)
C ble_l2cap_evt_add_credits_cplt_t | L2cap Credits Add Completed event for BLE_L2CAP_EVT_ADD_CREDITS_CPLT
C ble_l2cap_evt_add_credits_ind_t | L2cap Credits Add Indicate event for BLE_L2CAP_EVT_ADD_CREDITS_IND
C ble_l2cap_evt_conn_ind_t | L2cap Connected Indicate event for BLE_L2CAP_EVT_CONN_IND
C ble_l2cap_evt_conn_req_t | L2cap Connect Request event for BLE_L2CAP_EVT_CONN_REQ
C ble_l2cap_evt_disconnect_t | L2cap disconnect event for BLE_L2CAP_EVT_DISCONNECTED
C ble_l2cap_evt_sdu_recv_t | L2cap SDU Receive event for BLE_L2CAP_EVT_SDU_RECV
C ble_l2cap_evt_sdu_send_t | L2cap SDU Send event for BLE_L2CAP_EVT_SDU_SEND
C ble_l2cap_evt_t | BLE L2CAP event structure
C ble_l2cap_lecb_add_credits_t | LE flow control credit packet parameter
C ble_l2cap_lecb_cfm_conn_t | LE credit based connection confirm parameter
C ble_l2cap_lecb_conn_req_t | The parameter of LE credit based connection request packet sending
C ble_l2cap_lecb_sdu_t | Sdu parameter
C ble_prf_manager_cbs_t | Profile manager callbacks
C ble_sch_config_t | BLE Scheduler configure defination
C ble_sec_cfm_enc_data_t | SEC Confirm encryption data
C ble_sec_cfm_enc_t | SEC Confirm encryption
C ble_sec_enc_req_data_t | SEC encryption request data
C ble_sec_enc_req_t | SEC encryption request
C ble_sec_evt_enc_ind_t | Link Encrypted event for BLE_SEC_EVT_LINK_ENCRYPTED
C ble_sec_evt_enc_req_t | Link Encrypte Request event for BLE_SEC_EVT_LINK_ENC_REQUEST
C ble_sec_evt_key_missing_t | Key Missing event for BLE_SEC_EVT_KEY_MISSING
C ble_sec_evt_keypress_notify_t | Key Press Notify event for BLE_SEC_EVT_KEY_PRESS_NTF
C ble_sec_evt_t | BLE Security event structure
C ble_sec_nc_t | SEC number comparison value
C ble_sec_oob_t | SEC OOB value
C ble_sec_param_t | SEC Parameter
C ble_sec_tk_t | TK value
C ble_slp_config_t | BLE Sleep configure defination
C ble_uuid_t | GATT UUID structure
C bms_init_t | BMS Service init stucture. This contains all option and data needed for initialization of the service
C bod_env_t | BOD device structure definition
C boot_timing_params_t | Warm boot timing parameters(unit: us)
C bps_ieee_float16_t | SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit value with 12-bit mantissa and 4-bit exponent
C bps_init_t | Blood Pressure Service init stucture. This contains all option and data needed for initialization of the service
C bps_meas_t | Blood Pressure measurement structure
C cgms_cp_cmd_req_t |
C cgms_cp_cmd_rsp_t |
C cgms_get_info_req_t |
C cgms_init_t | CGM Service init stucture. This contains all option and data needed for initialization of the service
C cgms_meas_rec_t | Glucose Measurement structure. This contains glucose measurement value
C cgms_racp_req_t | Continuous Glucose Monitoring Recoerd Access Control Point request value
C cgms_racp_rsp_t | Continuous Glucose Monitoring Recoerd Access Control Point response value
C chip_ble_config_t | Chip configure defination
C comp_env_t | COMP device structure definition
C cscs_evt_t | Cycling Speed and Cadence Service event
C cscs_init_t | Cycling Speed and Cadence Service init stucture. This contains all option and data needed for initialization of the service
C cscs_meas_val_t | Cycling Speed and Cadence Measurement Character value structure
C cts_adj_info_t | CTS Adjust information
C cts_c_cur_time_t | Current Time value
C cts_c_evt_t | Current Time Service Client event
C cts_c_exact_time_256_t | Exact Time 256
C cts_c_handles_t | Handles on the connected peer device needed to interact with it
C cts_c_loc_time_info_t | Local Time Information
C cts_c_ref_time_info_t | Reference Time Information
C cts_cur_time_t | CTS Current Time value
C cts_evt_t | Current Time Service event
C cts_exact_time_256_t | CTS Exact Time 256
C cts_init_t | Current Time Service init structure. This contains all option and data needed for initialization of the service
C cts_loc_time_info_t | CTS Local Time Information
C cts_ref_time_info_t | CTS Reference Time Information
C cts_updata_ref_time_info_t | CTS Reference Time Updata Information
C dbg_ble_llcp_info_entry_s |
C dfu_boot_info_t | Boot information definition
C dfu_buf_table_t | DFU used buffers definition
C dfu_func_t | DFU used functions config definition
C dfu_image_info_t | Image information definition
C dfu_pro_callback_t | DFU program state callback definition
C dfu_receive_frame_t | DFU frame information definition
C dfu_spi_flash_func_t | SPI used functions config definition
C dis_c_evt_t | Device Information Service Client event
C dis_c_handles_t | Handles on the connected peer device needed to interact with it
C dis_c_pnp_id_t | Response data for PnP ID parameters
C dis_c_reg_cert_data_list_t | Response data for IEEE 11073-20601 Regulatory Certification Data List Structure
C dis_c_string_t | Response data for string-based DIS characteristics
C dis_c_sys_id_t | Response data for System ID parameters
C dis_init_t | Device Information Service init structure. This contains all options and data needed for initialization of the service
C dis_pnp_id_t | PnP ID parameters
C dis_reg_cert_data_list_t | IEEE 11073-20601 Regulatory Certification Data List Structure
C dis_string_t | UTF-8 string data type
C dis_sys_id_t | System ID parameters. The first field is the LSOs and the second field contains the MSOs
C dma_env_t | DMA device structure definition
C dss_evt_t | Device Synchronize Service Synchronize event
C dual_tim_env_t | DUAL_TIM device structure definition
C esls_ap_sync_param_t | Electronic Shelf Label Service sync parameter format
C esls_c_evt_t | Electronic Shelf Label Client event
C esls_c_handles_t | Handles on the connected peer device needed to interact with it
C esls_c_led_infor_t | Electronic Shelf Label LED infor type
C esls_char_infor_t | Electronic Shelf Label Service characteristic information
C esls_display_arr_t | Electronic Shelf Label Service display information data
C esls_evt_t | Electronic Shelf Label Service event
C esls_init_t | Electronic Shelf Label Service Init variable
C esls_led_arr_t | Electronic Shelf Label Service led information data
C esls_nvds_cb_t | Electronic Shelf Label Service NVDS callback func
C esls_sensor_arr_t | Electronic Shelf Label Service sensor information data
C exflash_func_t | EXFLASH function Structure definition
C gap_conn_cmp_t | Connection complete info
C gap_connless_cte_trans_param_t | Set connectionless CTE transmit parameters
C gap_slv_pref_t | Slave preferred connection parameters
C gapc_set_dev_info_ind_t | GAP Device inforamtion write indication
C gatts_prep_write_req_cb_t | GATT prepare write request struct
C gatts_read_req_cb_t | GATT read request struct
C gatts_write_req_cb_t | GATT write request struct
C gdx_lcp_config_t | LCP Parameter
C gls_evt_t | Glucose Service event
C gls_ieee_float16_t | SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit value with 12-bit mantissa and 4-bit exponent)
C gls_init_t | Glucose Service init stucture. This contains all option and data needed for initialization of the service
C gls_meas_ctx_t | Glucose measurement context structure
C gls_meas_val_t | Glucose Measurement structure. This contains glucose measurement value
C gls_racp_filter_t | Glucose Recoerd Access Control Point filter value
C gls_racp_req_t | Glucose Recoerd Access Control Point request value
C gls_racp_rsp_t | Glucose Recoerd Access Control Point response value
C gls_rec_t | Glucose measurement record
C gpio_init_t | GPIO init structure definition
C gus_c_evt_t | Goodix UART Service Client event
C gus_c_handles_t | Handles on the connected peer device needed to interact with it
C gus_evt_t | Goodix UART Service event
C gus_init_t | Goodix UART Service init stucture. This contains all option and data needed for initialization of the service
C hal_gpio_callback_t | HAL_GPIO Callback function definition
C hids_evt_t | HID Service event
C hids_hid_info_t | HID Information characteristic value
C hids_init_t | HID Service initialization variable
C hids_report_int_t | HID Service Report characteristic define
C hids_report_map_t | HID Service Report Map characteristic value
C hids_report_ref_t | Value of a Report Reference descriptor
C hrrcps_evt_t | HRS RSCS Relay Control Point Service event
C hrrcps_rsp_val_t | HRS RSCS Relay Control Point Response value
C hrs_c_evt_t | Heart Rate Service Client event
C hrs_c_handles_t | Handles on the connected peer device needed to interact with it
C hrs_c_hr_meas_t | Heart Rate Measurement characteristic value structure
C hrs_evt_t | Heart Rate Service event
C hrs_init_t | Heart Rate Service Init variable
C hts_evt_t | Health Thermometer Service event
C hts_init_t | Health Thermometer Service init stucture. This contains all option and data needed for initialization of the service
C hts_meas_val_t | Health Theromometer Measurement Character value structure
C i2c_env_t | I2C device structure definition
C ias_c_evt_t | Immediate Alert Service Client event
C ias_c_handles_t | Handles on the connected peer device needed to interact with it
C ias_evt_t | Immediate Alert Service event
C ias_init_t | Immediate Alert Service init stucture. This contains all option and data needed for initialization of the service
C ieee_float32_t | SFLOAT format (IEEE-11073 32-bit FLOAT, defined as a 32-bit vlue with 24-bit mantissa and 8-bit exponent
C lecb_add_credits_ind_t | LE credit based connection addition indication
C lecb_conn_ind_t | LE credit based connection created indication
C lecb_conn_req_ind_t | Receive LE credit based connection request packet indication
C lecb_disconn_ind_t | LE credit based disconnect indication
C lecb_sdu_send_evt_t | LE credit based SDU sending complete event
C link_node | ADC sample-node definition
C ll_dual_timer_init_t | LL DUAL TIMER init Structure definition
C ll_msio_init_t | LL MSIO init Structure definition
C ll_rng_init_t | LL RNG Init Structure definition
C lls_c_evt_t | Link Loss Service Client event
C lls_c_handles_t | Handles on the connected peer device needed to interact with it
C lls_evt_t | Link Loss Service event
C lls_init_t | Link Loss Service init stucture. This contains all option and data needed for initialization of the service
C lms_evt_t | LMS Service event
C lms_init_t | LMS Service initialization variable
C lns_evt_t | Log Notification Service event
C lns_log_data_t | Log Information data
C mlmr_c_evt_t | Multi Link Multi Role Service Client event
C mlmr_c_handles_t | Handles on the connected peer device needed to interact with it
C mlmr_evt_t | Multi Link Multi Role Service event
C mlmr_init_t | Multi Link Multi Role Service init stucture. This contains all option and data needed for initialization of the service
C ndcs_time_dst_t | Time with DST
C ntf_source_pdu_t | IOS notification structure
C otas_c_evt_t | OTA Service Client event
C otas_c_handles_t | Handles on the connected peer device needed to interact with it
C otas_evt_t | OTA Service event
C otas_init_t | OTA Service initialization variable
C pass_c_evt_t | Phone Alert Status Client Service event
C pass_c_handles_t | Handles on the connected peer device needed to interact with it
C pass_evt_t | Phone Alert Status Service event
C pass_init_t | Phone Alert Status Service init stucture. This contains all option and data needed for initialization of the service
C pcs_evt_t | PCS Service event
C pcs_init_t | PCS Service init stucture. This contains all option and data needed for initialization of the service
C pkc_init_t | PKC Init Structure definition
C pmu_trim_info_t | PMU trim parameter information definition
C prf_att_info_t | Attribute information
C prf_char_pres_fmt_t | Characteristic Presentation Format Descriptor structure. The packed size is PRF_CHAR_PRES_FMT_SIZE
C prf_date_time_t | The date and time structure. The packed size is 7 bytes
C prf_server_info_t | Profile server register information structure
C pwm_coding_channel_init_t | PWM Coding Channel init Structure definition
C pwm_coding_init_t | PWM Coding Init Structure definition
C pwm_comp_config_t | PWM COMP value init Structure definition
C pwm_env_t | PWM device structure definition
C pwm_handle_t | PWM handle Structure definition
C pwm_init_t | PWM Init Structure definition
C pwm_none_coding_channel_init_t | PWM None Coding Channel init Structure definition
C pwm_none_coding_init_t | PWM None Coding Init Structure definition
C pwr_mgmt_var_box_t | Power manager setting parameter. Use pwr_mgmt_var_set to transfer the parameters in the structure to PMU, and then the pwr_mgmt_mode_set function will use the new parameters for power management. Note that this is an advanced API, the wrong setting of parameters may lead to abnormal power management, so please use it carefully
C pwr_table_t | Parameter configuration table
C ras_ad_evt_t | Raning Service Adaptor event
C ras_ad_send_nti_ind_cmp_info_t | Event parameter for RAS_AD_EVT_SEND_NTI_IND_CMP
C ras_ad_set_cccd_info_t | Event parameter for set cccd
C ras_c_ad_discover_rsp_t |
C ras_c_ad_evt_t |
C ras_c_ad_read_ntf_ind_data_t |
C ras_c_ad_write_req_t |
C ras_c_ad_write_rsp_t |
C ras_c_discover_rsp_t |
C ras_c_evt_t |
C ras_c_read_rsp_t |
C ras_c_subevt_report_t |
C ras_c_write_req_t |
C ras_c_write_rsp_t |
C ras_cmp_data_rsp_operand_t |
C ras_ctr_data_operand_t |
C ras_ctr_lost_data_seg_operand_t |
C ras_ctr_pt_operation_t |
C ras_ctr_pt_rsp_t |
C ras_filter_data_operand_t |
C rf_trim_info_t | RF trim parameter information definition
C ringo_trim_info_t | Ringo trim information definition
C rng_env_t | RNG device structure definition
C rscs_c_evt_t | Running Speed and Cadence Service Client event
C rscs_c_handles_t | Handles on the connected peer device needed to interact with it
C rscs_c_meas_val_t | Running Speed and Cadence Measurement Character value structure
C rscs_evt_t | Running Speed and Cadence Service event
C rscs_init_t | Running Speed and Cadence Service init stucture. This contains all option and data needed for initialization of the service
C rscs_meas_val_t | Running Speed and Cadence Measurement Character value structure
C rtc_init_t | Rtc init params
C rtus_evt_t | RTUS Event data
C rtus_init_t | Reference Time Update Service init structure. This contains all option and data needed for initialization of the service
C rtus_update_state_t | RTUS Time Update State
C samples_evt_t | Sample Service event
C samples_init_t | Sample Service init stucture. This contains all option and data needed for initialization of the service
C sdk_version_t | SDK version definition
C spi_env_t | SPI device structure definition
C stack_heaps_table_t | The table contains the pointers to four arrays which are used as heap memory by BLE stack in ROM. The size of four arrays depends on the number of connections and the number of attributes of profiles
C sys_assert_cb_t | Assert callbacks
C ths_c_evt_t | Throughput Service Client event
C ths_c_handles_t | Handles on the connected peer device needed to interact with it
C ths_evt_t | Throughput Service event
C ths_init_t | Throughput Service init stucture. This contains all option and data needed for initialization of the service
C thscps_adv_param_t | THS Control Point Advertising Parameters
C thscps_evt_t | THS Control Point Service event
C thscps_rsp_val_t | THS Control Point Response value
C thscps_setting_t | THS Setting Information value
C thscps_test_conn_info_t | THS connect Information value
C thscps_test_info_t | THS Test Information value
C tick_handle_t | Tick handle params
C tim_env_t | TIM device structure definition
C tps_c_evt_t | Tx Power Service Client event
C tps_c_handles_t | Handles on the connected peer device needed to interact with it
C tps_init_t | Tx Power Servic init stucture. This contains all option and data needed for initialization of the service
C uart_env_t | UART device structure definition
C uds_chars_flag_t | UDS Characteristics Flags structure
C uds_chars_val_t | UDS Characteristics value structure
C uds_evt_t | User Data Service event
C uds_init_t | User Data Service init structure. This contains all option and data needed for initialization of the service
C uds_regi_user_data_flag_t | Registered User Data Flags structure
C uds_regi_user_data_stream_t | UDS Registered User Data stream
C wechat_data_t | WeChat service data
C wechat_evt_t | WeChat Service event
C wechat_init_t | WeChat Service Init variable
C wechat_pedo_meas_t | WeChat current pedometer measurement variable
C wechat_pedo_target_t | WeChat pedometer target variable
C wss_evt_t | Weight Scale Service event
C wss_init_t | Weight Scale Service Init variable
C wss_meas_val_t | Weight Scale Measurement data