Macros
Clock Phase
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_SPI_SCPHA_1EDGE 0x00000000UL
#define | LL_SPI_SCPHA_2EDGE (1UL << SPI_CTRL0_SERIAL_CLK_PHASE_POS)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SPI_SCPHA_1EDGE

#define LL_SPI_SCPHA_1EDGE 0x00000000UL

First clock transition is the first data capture edge

Definition at line 270 of file ll_spi.h.

## ◆ LL_SPI_SCPHA_2EDGE

#define LL_SPI_SCPHA_2EDGE (1UL << SPI_CTRL0_SERIAL_CLK_PHASE_POS)

Second clock transition is the first data capture edge

Definition at line 271 of file ll_spi.h.