Macros
InitStruct default configuartion
Peripheral Driver » LL Driver » ADC » Defines » ADC Private Macros

## Macros
#define | LL_ADC_DEFAULT_CONFIG
| LL ADC InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_ADC_DEFAULT_CONFIG

#define LL_ADC_DEFAULT_CONFIG

Value:
{ \
.channel_p = LL_ADC_INPUT_SRC_IO0, \
.channel_n = LL_ADC_INPUT_SRC_IO1, \
.input_mode = LL_ADC_INPUT_DIFFERENTIAL, \
.ref_source = LL_ADC_REF_SRC_BUF_INT, \
.ref_value = LL_ADC_REF_VALUE_1P2, \
.clock = LL_ADC_CLK_16M \
}

LL ADC InitStrcut default configuartion.

Definition at line 230 of file ll_adc.h.

LL_ADC_INPUT_SRC_IO0
#define LL_ADC_INPUT_SRC_IO0
Definition: ll_adc.h:157
LL_ADC_REF_VALUE_1P2
#define LL_ADC_REF_VALUE_1P2
Definition: ll_adc.h:142
LL_ADC_INPUT_SRC_IO1
#define LL_ADC_INPUT_SRC_IO1
Definition: ll_adc.h:158
LL_ADC_REF_SRC_BUF_INT
#define LL_ADC_REF_SRC_BUF_INT
Definition: ll_adc.h:174
LL_ADC_INPUT_DIFFERENTIAL
#define LL_ADC_INPUT_DIFFERENTIAL
Definition: ll_adc.h:151
LL_ADC_CLK_16M
#define LL_ADC_CLK_16M
Definition: ll_adc.h:127