Macros
UART Interrupt_definition
Peripheral Driver » HAL Driver » UART » Defines » UART Exported Constants

## Macros
#define | UART_IT_MS LL_UART_IER_MS
#define | UART_IT_RLS LL_UART_IER_RLS
#define | UART_IT_THRE LL_UART_IER_THRE
#define | UART_IT_RDA LL_UART_IER_RDA

## Detailed Description

## Macro Definition Documentation

## ◆ UART_IT_MS

#define UART_IT_MS LL_UART_IER_MS

Enable Modem Status Interrupt

Definition at line 297 of file hal_uart.h.

## ◆ UART_IT_RDA

#define UART_IT_RDA LL_UART_IER_RDA

Enable Received Data Available Interrupt and Character Timeout Interrupt

Definition at line 300 of file hal_uart.h.

## ◆ UART_IT_RLS

#define UART_IT_RLS LL_UART_IER_RLS

Enable Receiver Line Status Interrupt

Definition at line 298 of file hal_uart.h.

## ◆ UART_IT_THRE

#define UART_IT_THRE LL_UART_IER_THRE

Enable Transmit Holding Register Empty Interrupt

Definition at line 299 of file hal_uart.h.