Public Attributes | List of all members
_ll_pwm_none_coding_mode_init_t Struct Reference
Peripheral Driver » LL Driver » PWM » Structures » PWM Exported init structures

LL PWM none coding mode Structure definition. More...

`#include <ll_pwm.h>`

## Public Attributes
uint32_t | align
uint32_t | prescaler
uint32_t | bprescaler
uint32_t | hprescaler
uint32_t | breathstop_lvl
ll_pwm_none_coding_channel_init_t | channel_a
ll_pwm_none_coding_channel_init_t | channel_b
ll_pwm_none_coding_channel_init_t | channel_c

## Detailed Description

LL PWM none coding mode Structure definition.

Definition at line 132 of file ll_pwm.h.

## Member Data Documentation

## ◆ align

uint32_t _ll_pwm_none_coding_mode_init_t::align

Specifies the PWM alignment pulses. This parameter can be a value of PWM alignment pulses.

Definition at line 134 of file ll_pwm.h.

## ◆ bprescaler

uint32_t _ll_pwm_none_coding_mode_init_t::bprescaler

Specifies the required prescaler that the duty changes from 0% to 100% in breath mode. This parameter must be a number ranges between Min_Data=0 and Max_Data=0xFFFFFFFF. This parameter is recommended to be larger than 128*prescaler to guarantee an ideal breath effect.

This feature can be modified afterwards using unitary function ll_pwm_set_breath_prescaler().

Definition at line 143 of file ll_pwm.h.

## ◆ breathstop_lvl

uint32_t _ll_pwm_none_coding_mode_init_t::breathstop_lvl

Specifies the IO level when breath stop. This parameter can be a value of PWM stop io level.

Definition at line 154 of file ll_pwm.h.

## ◆ channel_a

ll_pwm_none_coding_channel_init_t _ll_pwm_none_coding_mode_init_t::channel_a

Specifies the configuration of channelA. This parameter can be a value of ll_pwm_none_coding_channel_init_t.

Definition at line 157 of file ll_pwm.h.

## ◆ channel_b

ll_pwm_none_coding_channel_init_t _ll_pwm_none_coding_mode_init_t::channel_b

Specifies the configuration of channelB. This parameter can be a value of ll_pwm_none_coding_channel_init_t.

Definition at line 160 of file ll_pwm.h.

## ◆ channel_c

ll_pwm_none_coding_channel_init_t _ll_pwm_none_coding_mode_init_t::channel_c

Specifies the configuration of channelC. This parameter can be a value of ll_pwm_none_coding_channel_init_t.

Definition at line 163 of file ll_pwm.h.

## ◆ hprescaler

uint32_t _ll_pwm_none_coding_mode_init_t::hprescaler

Specifies the required prescaler in breath hold state. This parameter must be a number ranges between Min_Data=0 and Max_Data=0xFFFFFF.

This feature can be modified afterwards using unitary function ll_pwm_set_hold_prescaler().

Definition at line 149 of file ll_pwm.h.

## ◆ prescaler

uint32_t _ll_pwm_none_coding_mode_init_t::prescaler

Specifies the prescaler value which will be used configure PWM output frequency. This parameter must be a number ranges between Min_Data = 0 and Max_Data = 0xFFFFFFFF. This parameter should be larger than 128.

This feature can be modified afterwards using unitary function ll_pwm_set_prescaler().

Definition at line 137 of file ll_pwm.h.

The documentation for this struct was generated from the following file:

- ll_pwm.h