Here is a list of all file members with links to the files they belong to:

### - c -

- CALENDAR_ALARM_DISABLE_ALL : hal_calendar.h
- CALENDAR_ALARM_DISABLE_DATE : hal_calendar.h
- CALENDAR_ALARM_DISABLE_TICK : hal_calendar.h
- CALENDAR_ALARM_SEL_DATE : hal_calendar.h
- CALENDAR_ALARM_SEL_WEEKDAY : hal_calendar.h
- calendar_alarm_t : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_FRI : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_MON : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_SAT : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_SUN : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_THU : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_TUE : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_WED : hal_calendar.h
- CALENDAR_FLAG_ALARM : hal_calendar.h
- CALENDAR_FLAG_TICK : hal_calendar.h
- CALENDAR_FLAG_WRAP : hal_calendar.h
- calendar_handle_t : hal_calendar.h
- CALENDAR_IT_ALARM : hal_calendar.h
- CALENDAR_IT_TICK : hal_calendar.h
- CALENDAR_IT_WRAP : hal_calendar.h
- CALENDAR_TICK_AUTO : hal_calendar.h
- CALENDAR_TICK_SINGLE : hal_calendar.h
- calendar_time_t : hal_calendar.h
- callback_t : gr5405_sys_sdk.h
- CFG_ANCS_ATTRIBUTE_MAXLEN : ancs_protocol.h
- CGC_CLK_OFF : hal_cgc.h
- CGC_CLK_ON : hal_cgc.h
- cgc_clk_state_t : hal_cgc.h
- CGC_CLOCK_DISABLE : ll_cgc.h
- CGC_CLOCK_ENABLE : ll_cgc.h
- CGC_DEFAULT_CONFIG : hal_cgc.h
- CGC_FRC_ALL_CLK : hal_cgc.h
- CGC_FRC_AON_MCUSUB_HCLK : hal_cgc.h
- CGC_FRC_APB_SUB_HCLK : hal_cgc.h
- CGC_FRC_BLE_BRG_HCLK : hal_cgc.h
- CGC_FRC_DMA_HCLK : hal_cgc.h
- CGC_FRC_GPIO_HCLK : hal_cgc.h
- CGC_FRC_HTB_HCLK : hal_cgc.h
- CGC_FRC_I2C0_HCLK : hal_cgc.h
- CGC_FRC_I2C1_HCLK : hal_cgc.h
- CGC_FRC_I2S_HCLK : hal_cgc.h
- CGC_FRC_I2S_S_HCLK : hal_cgc.h
- CGC_FRC_PWM_HCLK : hal_cgc.h
- CGC_FRC_QSPI0_HCLK : hal_cgc.h
- CGC_FRC_QSPI1_HCLK : hal_cgc.h
- CGC_FRC_ROM_HCLK : hal_cgc.h
- CGC_FRC_SECU_DIV4_PCLK : hal_cgc.h
- CGC_FRC_SECU_HCLK : hal_cgc.h
- CGC_FRC_SERIAL_HCLK : hal_cgc.h
- CGC_FRC_SIM_HCLK : hal_cgc.h
- CGC_FRC_SNSADC_HCLK : hal_cgc.h
- CGC_FRC_SPIM_HCLK : hal_cgc.h
- CGC_FRC_SPIS_HCLK : hal_cgc.h
- CGC_FRC_SRAM_HCLK : hal_cgc.h
- CGC_FRC_UART0_HCLK : hal_cgc.h
- CGC_FRC_UART1_HCLK : hal_cgc.h
- CGC_FRC_XF_XQSPI_HCLK : hal_cgc.h
- CGC_FRC_XQSPI_DIV4_PCLK : hal_cgc.h
- cgc_init_t : hal_cgc.h
- CGC_WFI_ALL_CLK : hal_cgc.h
- CGC_WFI_AON_MCUSUB_HCLK : hal_cgc.h
- CGC_WFI_APB_SUB_HCLK : hal_cgc.h
- CGC_WFI_BLE_BRG_HCLK : hal_cgc.h
- CGC_WFI_DMA_HCLK : hal_cgc.h
- CGC_WFI_GPIO_HCLK : hal_cgc.h
- CGC_WFI_HTB_HCLK : hal_cgc.h
- CGC_WFI_I2S_S_HCLK : hal_cgc.h
- CGC_WFI_PWM_HCLK : hal_cgc.h
- CGC_WFI_ROM_HCLK : hal_cgc.h
- CGC_WFI_SECU_DIV4_PCLK : hal_cgc.h
- CGC_WFI_SECU_HCLK : hal_cgc.h
- CGC_WFI_SERIAL_HCLK : hal_cgc.h
- CGC_WFI_SIM_HCLK : hal_cgc.h
- CGC_WFI_SNSADC_HCLK : hal_cgc.h
- CGC_WFI_SRAM_HCLK : hal_cgc.h
- CGC_WFI_XF_XQSPI_HCLK : hal_cgc.h
- CGC_WFI_XQSPI_DIV4_PCLK : hal_cgc.h
- CGMS_ANN_CAL_TEMP_CAL_NOT_ALLOWED : cgms.h
- CGMS_ANN_CAL_TEMP_CAL_PROCESS_PENDING : cgms.h
- CGMS_ANN_CAL_TEMP_CAL_RECOMMENED : cgms.h
- CGMS_ANN_CAL_TEMP_CAL_REQ : cgms.h
- CGMS_ANN_CAL_TEMP_TEMP_TOO_HIGH : cgms.h
- CGMS_ANN_CAL_TEMP_TEMP_TOO_LOW : cgms.h
- CGMS_ANN_CAL_TEMP_TIME_SYNC_REQ : cgms.h
- CGMS_ANN_STATUS_DEV_BATTERY_LOW : cgms.h
- CGMS_ANN_STATUS_DEV_SPEC_ALERT : cgms.h
- CGMS_ANN_STATUS_GEN_DEV_FAULT : cgms.h
- CGMS_ANN_STATUS_SENSOR_MALFUNCTION : cgms.h
- CGMS_ANN_STATUS_SENSOR_TYPE_INCORRECT : cgms.h
- CGMS_ANN_STATUS_SESSION_STOPPED : cgms.h
- CGMS_ANN_WARN_RATE_OF_DECREASE_EXCEEDED : cgms.h
- CGMS_ANN_WARN_RATE_OF_INCREASE_EXCEEDED : cgms.h
- CGMS_ANN_WARN_RESULT_HIGHER_THAN_DEV_CAN_PROCESS : cgms.h
- CGMS_ANN_WARN_RESULT_HIGHER_THAN_HYPER_LVL : cgms.h
- CGMS_ANN_WARN_RESULT_HIGHER_THAN_PATIENT_HIGH_LVL : cgms.h
- CGMS_ANN_WARN_RESULT_LOWER_THAN_DEV_CAN_PROCESS : cgms.h
- CGMS_ANN_WARN_RESULT_LOWER_THAN_HYPO_LVL : cgms.h
- CGMS_ANN_WARN_RESULT_LOWER_THAN_PATIENT_LOW_LVL : cgms.h
- CGMS_CAL_STATUS_OUT_OF_RANGE : cgms.h
- CGMS_CAL_STATUS_PROCESS_PENGDING : cgms.h
- CGMS_CAL_STATUS_REJECT : cgms.h
- cgms_cal_status_t : cgms.h
- cgms_cccd_change_handler_t : cgms.h
- CGMS_CCCD_STATUS_FEAT_DISABLED : cgms.h
- CGMS_CCCD_STATUS_FEAT_ENABLED : cgms.h
- CGMS_CCCD_STATUS_MEAS_DISABLED : cgms.h
- CGMS_CCCD_STATUS_MEAS_ENABLED : cgms.h
- CGMS_CCCD_STATUS_RACP_DISABLED : cgms.h
- CGMS_CCCD_STATUS_RACP_ENABLED : cgms.h
- CGMS_CCCD_STATUS_SPCP_DISABLED : cgms.h
- CGMS_CCCD_STATUS_SPCP_ENABLED : cgms.h
- cgms_cccd_status_t : cgms.h
- CGMS_CMD_RET_CODE_INVALID_OPERAND : cgms.h
- CGMS_CMD_RET_CODE_NOT_SUPPORT : cgms.h
- CGMS_CMD_RET_CODE_PARAM_OUT_OF_RANGE : cgms.h
- CGMS_CMD_RET_CODE_PROCEDURE_NOT_COMPLETED : cgms.h
- CGMS_CMD_RET_CODE_RESERVED : cgms.h
- CGMS_CMD_RET_CODE_SUCESS : cgms.h
- CGMS_CONNECTION_MAX : cgms.h
- cgms_cp_cmd_code_t : cgms.h
- cgms_cp_cmd_req_handler_t : cgms.h
- cgms_cp_cmd_ret_t : cgms.h
- cgms_cp_cmd_rsp_send() : cgms.h
- CGMS_CP_CODE_GET_CAL_VALUE : cgms.h
- CGMS_CP_CODE_GET_COM_INTERVAL : cgms.h
- CGMS_CP_CODE_GET_HYPER_LVL : cgms.h
- CGMS_CP_CODE_GET_HYPO_LVL : cgms.h
- CGMS_CP_CODE_GET_PATIENT_HIGHT_LVL : cgms.h
- CGMS_CP_CODE_GET_PATIENT_LOW_LVL : cgms.h
- CGMS_CP_CODE_GET_RATE_OF_DEC_LVL : cgms.h
- CGMS_CP_CODE_GET_RATE_OF_INC_LVL : cgms.h
- CGMS_CP_CODE_NONE : cgms.h
- CGMS_CP_CODE_RESET_DEV_SPEC_ALERT : cgms.h
- CGMS_CP_CODE_SET_CAL_VALUE : cgms.h
- CGMS_CP_CODE_SET_COM_INTERVAL : cgms.h
- CGMS_CP_CODE_SET_HYPER_LVL : cgms.h
- CGMS_CP_CODE_SET_HYPO_LVL : cgms.h
- CGMS_CP_CODE_SET_PATIENT_HIGHT_LVL : cgms.h
- CGMS_CP_CODE_SET_PATIENT_LOW_LVL : cgms.h
- CGMS_CP_CODE_SET_RATE_OF_DEC_LVL : cgms.h
- CGMS_CP_CODE_SET_RATE_OF_INC_LVL : cgms.h
- CGMS_CP_CODE_SET_SES_START_TIME : cgms.h
- CGMS_CP_CODE_START_THE_SESSION : cgms.h
- CGMS_CP_CODE_STOP_THE_SESSION : cgms.h
- cgms_db_rec_delete_func_t : cgms.h
- cgms_db_rec_get_func_t : cgms.h
- CGMS_ERROR_CCCD_NOT_CFG : cgms.h
- CGMS_ERROR_INVALID_CRC : cgms.h
- CGMS_ERROR_MISSING_CRC : cgms.h
- CGMS_ERROR_PRO_IN_PROCESS : cgms.h
- CGMS_FEAT_CALIBRATION : cgms.h
- CGMS_FEAT_DEV_SPEC_ALERT : cgms.h
- CGMS_FEAT_E2E_CRC : cgms.h
- CGMS_FEAT_FULL : cgms.h
- CGMS_FEAT_GENERAL_DEV_FAULT_DET : cgms.h
- CGMS_FEAT_HYPER_ALERT : cgms.h
- CGMS_FEAT_HYPO_ALERT : cgms.h
- CGMS_FEAT_LOW_BATTERY_DET : cgms.h
- CGMS_FEAT_MULTIPLE_BOND : cgms.h
- CGMS_FEAT_MULTIPLE_SESSION : cgms.h
- CGMS_FEAT_PATIENT_HIGH_LOW_ALERT : cgms.h
- CGMS_FEAT_QUALITY : cgms.h
- CGMS_FEAT_RATE_INC_DEC_ALERT : cgms.h
- CGMS_FEAT_RESULT_HIGH_LOW_DET : cgms.h
- CGMS_FEAT_SENSOR_MAL_DET : cgms.h
- CGMS_FEAT_SENSOR_TYPE_ERR_DET : cgms.h
- CGMS_FEAT_TEMP_HIGH_LOW_DET : cgms.h
- CGMS_FEAT_TREND_INFORMATION : cgms.h
- cgms_feature_update() : cgms.h
- CGMS_FEATURE_VAL_LEN_MAX : cgms.h
- CGMS_GET_INFO_ANN_STATUS : cgms.h
- cgms_get_info_code_t : cgms.h
- CGMS_GET_INFO_NONE : cgms.h
- cgms_get_info_req_handler_t : cgms.h
- CGMS_GET_INFO_SES_RUN_TIME : cgms.h
- CGMS_GET_INFO_SES_START_TIME : cgms.h
- CGMS_MEAS_FLAG_CAL_TEMP_PRESENT : cgms.h
- CGMS_MEAS_FLAG_FULL : cgms.h
- CGMS_MEAS_FLAG_QUALITY_PRESENT : cgms.h
- CGMS_MEAS_FLAG_STATUS_PRESENT : cgms.h
- CGMS_MEAS_FLAG_TREND_INFO_PRESENT : cgms.h
- CGMS_MEAS_FLAG_WARING_PRESENT : cgms.h
- CGMS_MEAS_LOC_AST : cgms.h
- CGMS_MEAS_LOC_CONTROL : cgms.h
- CGMS_MEAS_LOC_EAR : cgms.h
- CGMS_MEAS_LOC_FINGER : cgms.h
- CGMS_MEAS_LOC_SUB_TISSUE : cgms.h
- cgms_meas_loc_t : cgms.h
- CGMS_MEAS_TYPE_ART_BLOOD : cgms.h
- CGMS_MEAS_TYPE_ART_PLASMA : cgms.h
- CGMS_MEAS_TYPE_CAP_BLOOD : cgms.h
- CGMS_MEAS_TYPE_CAP_PLASMA : cgms.h
- CGMS_MEAS_TYPE_CONTROL : cgms.h
- CGMS_MEAS_TYPE_FLUID : cgms.h
- cgms_meas_type_t : cgms.h
- CGMS_MEAS_TYPE_UNDET_BLOOD : cgms.h
- CGMS_MEAS_TYPE_UNDET_PLASMA : cgms.h
- CGMS_MEAS_TYPE_VEN_BLOOD : cgms.h
- CGMS_MEAS_TYPE_VEN_PLASMA : cgms.h
- cgms_meas_val_send() : cgms.h
- CGMS_MEASUREMENT_VAL_LEN_MAX : cgms.h
- CGMS_RACP_FILTER_RESERVED : cgms_racp.h
- CGMS_RACP_FILTER_TIME_OFFSET : cgms_racp.h
- CGMS_RACP_FILTER_TIME_OFFSET_LEN : cgms_racp.h
- cgms_racp_filter_type_t : cgms_racp.h
- CGMS_RACP_OP_ABORT_OP : cgms_racp.h
- cgms_racp_op_code_t : cgms_racp.h
- CGMS_RACP_OP_DEL_STRD_RECS : cgms_racp.h
- CGMS_RACP_OP_NB_OF_STRD_RECS_RSP : cgms_racp.h
- CGMS_RACP_OP_REP_NB_OF_STRD_RECS : cgms_racp.h
- CGMS_RACP_OP_REP_STRD_RECS : cgms_racp.h
- CGMS_RACP_OP_RESERVED : cgms_racp.h
- CGMS_RACP_OP_RSP_CODE : cgms_racp.h
- cgms_racp_operand_t : cgms_racp.h
- CGMS_RACP_OPERATOR_ALL_RECS : cgms_racp.h
- CGMS_RACP_OPERATOR_FIRST_REC : cgms_racp.h
- CGMS_RACP_OPERATOR_GT_OR_EQ : cgms_racp.h
- CGMS_RACP_OPERATOR_LAST_REC : cgms_racp.h
- CGMS_RACP_OPERATOR_LE_OR_EQ : cgms_racp.h
- CGMS_RACP_OPERATOR_NULL : cgms_racp.h
- cgms_racp_operator_t : cgms_racp.h
- CGMS_RACP_OPERATOR_WITHIN_RANGE_OF : cgms_racp.h
- cgms_racp_req_decode() : cgms_racp.h
- cgms_racp_req_handler_t : cgms.h
- CGMS_RACP_RSP_ABORT_UNSUCCESSFUL : cgms_racp.h
- cgms_racp_rsp_encode() : cgms_racp.h
- CGMS_RACP_RSP_INVALID_OPERAND : cgms_racp.h
- CGMS_RACP_RSP_INVALID_OPERATOR : cgms_racp.h
- CGMS_RACP_RSP_NO_RECS_FOUND : cgms_racp.h
- CGMS_RACP_RSP_OP_CODE_NOT_SUP : cgms_racp.h
- CGMS_RACP_RSP_OPERAND_NOT_SUP : cgms_racp.h
- CGMS_RACP_RSP_OPERATOR_NOT_SUP : cgms_racp.h
- CGMS_RACP_RSP_PROCEDURE_NOT_COMPLETED : cgms_racp.h
- CGMS_RACP_RSP_RESERVED : cgms_racp.h
- CGMS_RACP_RSP_SUCCESS : cgms_racp.h
- CGMS_RACP_RSP_VALID_DECODE : cgms_racp.h
- CGMS_RACP_VAL_LEN_MAX : cgms.h
- CGMS_RACP_VAL_LEN_MIN : cgms.h
- cgms_rec_num_get_func_t : cgms.h
- CGMS_RUN_TIME_VAL_LEN_MAX : cgms.h
- cgms_service_init() : cgms.h
- CGMS_START_TIME_VAL_LEN_MAX : cgms.h
- CGMS_STATUS_VAL_LEN_MAX : cgms.h
- CHECK_IS_ON_FPGA : gr5405_sys_sdk.h
- CHIP_TRIM_PATTERN : gr5405_chip_trim.h
- CLDR_REG_READ : ll_calendar.h
- clock_calib_notify_cb_t : platform_sdk.h
- clock_calib_notify_register() : platform_sdk.h
- clock_calib_notify_unregister() : platform_sdk.h
- clock_calibration_irq_handler() : platform_sdk.h
- clock_calibration_is_done() : platform_sdk.h
- CLOSED : hal_rtc.h
- CO_BIT : ble_gapm.h
- COLD_BOOT : gr5405_pwr.h
- COMP_DEFAULT_CONFIG : hal_comp.h
- comp_handle_t : hal_comp.h
- COMP_HYST_NEGATIVE : hal_comp.h
- COMP_HYST_POSITIVE : hal_comp.h
- comp_init_t : hal_comp.h
- COMP_INPUT_SRC_IO0 : hal_comp.h
- COMP_INPUT_SRC_IO1 : hal_comp.h
- COMP_INPUT_SRC_IO2 : hal_comp.h
- COMP_INPUT_SRC_IO3 : hal_comp.h
- COMP_INPUT_SRC_IO4 : hal_comp.h
- COMP_INPUT_SRC_IO5 : hal_comp.h
- COMP_INPUT_SRC_IO6 : hal_comp.h
- COMP_INPUT_SRC_IO7 : hal_comp.h
- COMP_INPUT_SRC_VBAT : hal_comp.h
- COMP_INPUT_SRC_VREF : hal_comp.h
- COMP_PWR_ID : app_pwr_mgmt.h
- COMP_REF_SRC_IO0 : hal_comp.h
- COMP_REF_SRC_IO1 : hal_comp.h
- COMP_REF_SRC_IO2 : hal_comp.h
- COMP_REF_SRC_IO3 : hal_comp.h
- COMP_REF_SRC_IO4 : hal_comp.h
- COMP_REF_SRC_IO5 : hal_comp.h
- COMP_REF_SRC_IO6 : hal_comp.h
- COMP_REF_SRC_IO7 : hal_comp.h
- COMP_REF_SRC_VBAT : hal_comp.h
- COMP_REF_SRC_VREF : hal_comp.h
- COMP_RES_DEGENERATION_NEGATIVE : hal_comp.h
- COMP_RES_DEGENERATION_POSITIVE : hal_comp.h
- COMP_WAKEUP_EDGE_BOTH : hal_comp.h
- COMP_WAKEUP_EDGE_FALLING : hal_comp.h
- COMP_WAKEUP_EDGE_RISING : hal_comp.h
- CONFIGURING_STATE : esls.h
- CS_END_STATE_ABORT_CPLT : hal_spi.h
- CS_END_STATE_POLL_EEPREAD : hal_spi.h
- CS_END_STATE_POLL_RX : hal_spi.h
- CS_END_STATE_POLL_TX : hal_spi.h
- CS_END_STATE_POLL_TX_RX : hal_spi.h
- CS_END_STATE_RX_ABORT_CPLT : hal_spi.h
- CS_END_STATE_RX_CPLT : hal_spi.h
- CS_END_STATE_TX_ABORT_CPLT : hal_spi.h
- CS_END_STATE_TX_CPLT : hal_spi.h
- CS_END_STATE_TX_RX_CPLT : hal_spi.h
- CS_END_STATE_XFER_ERR : hal_spi.h
- CS_STA_STATE_DMA_EEPREAD : hal_spi.h
- CS_STA_STATE_DMA_LLP_TX : hal_spi.h
- CS_STA_STATE_DMA_RX : hal_spi.h
- CS_STA_STATE_DMA_SCATTER_RX : hal_spi.h
- CS_STA_STATE_DMA_TX : hal_spi.h
- CS_STA_STATE_DMA_TX_RX : hal_spi.h
- CS_STA_STATE_IT_EEPREAD : hal_spi.h
- CS_STA_STATE_IT_RX : hal_spi.h
- CS_STA_STATE_IT_TX : hal_spi.h
- CS_STA_STATE_IT_TX_RX : hal_spi.h
- CS_STA_STATE_POLL_EEPREAD : hal_spi.h
- CS_STA_STATE_POLL_RX : hal_spi.h
- CS_STA_STATE_POLL_TX : hal_spi.h
- CS_STA_STATE_POLL_TX_RX : hal_spi.h
- CSCS_CHAR_FULL : cscs.h
- CSCS_CHAR_MANDATORY : cscs.h
- CSCS_CHAR_SC_CTRL_POINT : cscs.h
- CSCS_CHAR_SENSOR_LOC_SUP : cscs.h
- CSCS_CONNECTION_MAX : cscs.h
- cscs_ctrl_pt_op_code_t : cscs.h
- CSCS_CTRL_PT_OP_REQ_SUP_LOC : cscs.h
- CSCS_CTRL_PT_OP_RESERVED : cscs.h
- CSCS_CTRL_PT_OP_RSP_CODE : cscs.h
- CSCS_CTRL_PT_OP_SET_CUMUL_VAL : cscs.h
- CSCS_CTRL_PT_OP_START_CALIB : cscs.h
- CSCS_CTRL_PT_OP_UPD_LOC : cscs.h
- CSCS_CTRL_PT_RSP_FAILED : cscs.h
- CSCS_CTRL_PT_RSP_INVALID_PARAM : cscs.h
- CSCS_CTRL_PT_RSP_LEN_MIN : cscs.h
- CSCS_CTRL_PT_RSP_NOT_SUP : cscs.h
- CSCS_CTRL_PT_RSP_RESERVED : cscs.h
- cscs_ctrl_pt_rsp_send() : cscs.h
- CSCS_CTRL_PT_RSP_SUCCESS : cscs.h
- cscs_ctrl_pt_rsp_t : cscs.h
- CSCS_CTRL_PT_VAL_LEN_MAX : cscs.h
- CSCS_ERROR_CCCD_INVALID : cscs.h
- CSCS_ERROR_PROC_IN_PROGRESS : cscs.h
- CSCS_EVT_CSC_MEAS_NOTIFICATION_DISABLE : cscs.h
- CSCS_EVT_CSC_MEAS_NOTIFICATION_ENABLE : cscs.h
- CSCS_EVT_CSC_MEAS_SEND_CPLT : cscs.h
- CSCS_EVT_CTRL_POINT_INDICATION_DISABLE : cscs.h
- CSCS_EVT_CTRL_POINT_INDICATION_ENABLE : cscs.h
- CSCS_EVT_CTRL_POINT_RSP_CPLT : cscs.h
- CSCS_EVT_CUMUL_VAL_SET : cscs.h
- cscs_evt_handler_t : cscs.h
- CSCS_EVT_INVALID : cscs.h
- CSCS_EVT_SEBSOR_CALIBRATION : cscs.h
- CSCS_EVT_SEBSOR_LOC_UPD : cscs.h
- CSCS_EVT_SUP_SEBSOR_LOC_REQ : cscs.h
- cscs_evt_type_t : cscs.h
- CSCS_FEAR_FULL_BIT : cscs.h
- CSCS_FEAT_CRANK_REVOLUTION_SUP_BIT : cscs.h
- CSCS_FEAT_MULTIPLE_SENSORS_BIT : cscs.h
- CSCS_FEAT_VAL_LEN_MAX : cscs.h
- CSCS_FEAT_WHEEL_REVOLUTION_SUP_BIT : cscs.h
- CSCS_MEAS_FLAG_CRANK_REVOLUTION_BIT : cscs.h
- CSCS_MEAS_FLAG_WHEEL_REVOLUTION_BIT : cscs.h
- CSCS_MEAS_VAL_LEN_MAX : cscs.h
- cscs_measurement_send() : cscs.h
- CSCS_SENSOR_LOC_FRONT_HUB : cscs.h
- CSCS_SENSOR_LOC_FRONT_WHEEL : cscs.h
- CSCS_SENSOR_LOC_HIP : cscs.h
- CSCS_SENSOR_LOC_LEFT_PEDAL : cscs.h
- CSCS_SENSOR_LOC_OTHER : cscs.h
- CSCS_SENSOR_LOC_RIGHT_PEDAL : cscs.h
- CSCS_SENSOR_LOC_SHOE_IN : cscs.h
- CSCS_SENSOR_LOC_SHOE_TOP : cscs.h
- CSCS_SENSOR_LOC_SUP_NB : cscs.h
- cscs_sensor_loc_t : cscs.h
- cscs_sensor_loc_update() : cscs.h
- CSCS_SENSOR_LOC_VAL_LEN_MAX : cscs.h
- cscs_service_init() : cscs.h
- CTRL_POINT_GET_APP_ATTRIBUTE : ancs_protocol.h
- CTRL_POINT_GET_NTF_ATTRIBUTE : ancs_protocol.h
- CTRL_POINT_PERFORM_NTF_ACTION : ancs_protocol.h
- CTS_AR_DST_CHANGE : cts.h
- CTS_AR_EXT_REF_TIME_UPDATE : cts.h
- CTS_AR_MAUAL_TIME_UPDATE : cts.h
- CTS_AR_NO_CHANGE : cts.h
- CTS_AR_TIME_ZONE_CHANGE : cts.h
- CTS_C_AR_DST_CHANGE : cts_c.h
- CTS_C_AR_EXT_REF_TIME_UPDATE : cts_c.h
- CTS_C_AR_MAUAL_TIME_UPDATE : cts_c.h
- CTS_C_AR_NO_CHANGE : cts_c.h
- CTS_C_AR_TIME_ZONE_CHANGE : cts_c.h
- CTS_C_CONNECTION_MAX : cts_c.h
- cts_c_cur_time_notify_set() : cts_c.h
- cts_c_cur_time_read() : cts_c.h
- cts_c_cur_time_set() : cts_c.h
- CTS_C_CUR_TIME_VAL_LEN : cts_c.h
- cts_c_data_parse() : cts.h , cts_c.h
- cts_c_disc_srvc_start() : cts_c.h
- CTS_C_DST_OFFSET_DAYLIGHT_TIME : cts_c.h
- CTS_C_DST_OFFSET_DOUB_DAYLIGHT_TIME : cts_c.h
- CTS_C_DST_OFFSET_HALF_HOUR : cts_c.h
- CTS_C_DST_OFFSET_STANDAR_TIME : cts_c.h
- cts_c_dst_offset_t : cts_c.h
- CTS_C_ERROR_FIELDS_IGNORED : cts_c.h
- CTS_C_EVT_CUR_TIME_NTF_SET_SUCCESS : cts_c.h
- CTS_C_EVT_CUR_TIME_SET_SUCCESS : cts_c.h
- CTS_C_EVT_DISCOVERY_COMPLETE : cts_c.h
- CTS_C_EVT_DISCOVERY_FAIL : cts_c.h
- cts_c_evt_handler_t : cts_c.h
- CTS_C_EVT_INVALID : cts_c.h
- CTS_C_EVT_INVALID_CUR_TIME_REC : cts_c.h
- CTS_C_EVT_INVALID_LOC_TIME_INFO_REC : cts_c.h
- CTS_C_EVT_INVALID_REF_TIME_INFO_REC : cts_c.h
- CTS_C_EVT_LOC_TIME_INFO_SET_SUCCESS : cts_c.h
- cts_c_evt_type_t : cts_c.h
- CTS_C_EVT_VALID_CUR_TIME_REC : cts_c.h
- CTS_C_EVT_VALID_LOC_TIME_INFO_REC : cts_c.h
- CTS_C_EVT_VALID_REF_TIME_INFO_REC : cts_c.h
- CTS_C_EVT_WRITE_OP_ERR : cts_c.h
- cts_c_loc_time_info_read() : cts_c.h
- cts_c_loc_time_info_set() : cts_c.h
- CTS_C_LOC_TIME_INFO_VAL_LEN : cts_c.h
- cts_c_ref_time_info_read() : cts_c.h
- cts_c_ref_time_source_t : cts_c.h
- CTS_C_REF_TIME_SRC_ATOMIC_CLOCK : cts_c.h
- CTS_C_REF_TIME_SRC_CELLUAR_NET : cts_c.h
- CTS_C_REF_TIME_SRC_GPS : cts_c.h
- CTS_C_REF_TIME_SRC_MANUAL : cts_c.h
- CTS_C_REF_TIME_SRC_NET_TIME_PROTOCOL : cts_c.h
- CTS_C_REF_TIME_SRC_RADIO_TIME_SIGNAL : cts_c.h
- CTS_C_REF_TIME_SRC_UNKNOWN : cts_c.h
- CTS_C_TIME_ACCURACT_UNKNOWN : cts_c.h
- CTS_C_TIME_ACCURACY_OUT_RANGE : cts_c.h
- CTS_C_TIME_Y_M_D_UNKNOWN : cts_c.h
- CTS_C_TIME_YEAR_VALID_VAL_MAX : cts_c.h
- CTS_C_TIME_YEAR_VALID_VAL_MIN : cts_c.h
- CTS_C_TIME_ZONE_OFFSET_MAX : cts_c.h
- CTS_C_TIME_ZONE_OFFSET_MIN : cts_c.h
- cts_c_week_day_t : cts_c.h
- CTS_C_WEEK_FRIDAY : cts_c.h
- CTS_C_WEEK_MONDAY : cts_c.h
- CTS_C_WEEK_SATURDAY : cts_c.h
- CTS_C_WEEK_SUNDAY : cts_c.h
- CTS_C_WEEK_THURSDAT : cts_c.h
- CTS_C_WEEK_TUSEDAY : cts_c.h
- CTS_C_WEEK_UNKNOWN_DAY : cts_c.h
- CTS_C_WEEK_WEDNESDAY : cts_c.h
- CTS_CHAR_FULL : cts.h
- CTS_CHAR_LOC_TIME_INFO_SUP : cts.h
- CTS_CHAR_MANDATORY : cts.h
- CTS_CHAR_REF_TIME_INFO_SUP : cts.h
- cts_client_init() : cts_c.h
- CTS_CONNECTION_MAX : cts.h
- cts_cur_time_adjust() : cts.h
- cts_cur_time_send() : cts.h
- CTS_CUR_TIME_VAL_LEN : cts.h
- CTS_DST_OFFSET_DAYLIGHT_TIME : cts.h
- CTS_DST_OFFSET_DOUB_DAYLIGHT_TIME : cts.h
- CTS_DST_OFFSET_DOUB_UNKNOWED_TIME : cts.h
- CTS_DST_OFFSET_HALF_HOUR : cts.h
- CTS_DST_OFFSET_STANDAR_TIME : cts.h
- cts_dst_offset_t : cts.h
- CTS_ERROR_FIELDS_IGNORED : cts.h
- CTS_EVT_CUR_TIME_NOTIFICATION_DISABLED : cts.h
- CTS_EVT_CUR_TIME_NOTIFICATION_ENABLED : cts.h
- CTS_EVT_CUR_TIME_SET_BY_PEER : cts.h
- cts_evt_handler_t : cts.h
- CTS_EVT_INVALID : cts.h
- CTS_EVT_LOC_TIME_INFO_SET_BY_PEER : cts.h
- cts_evt_type_t : cts.h
- cts_exact_time_get() : cts.h
- cts_exact_time_update() : cts.h
- CTS_LOC_TIME_INFO_VAL_LEN : cts.h
- CTS_REF_TIME_INFO_VAL_LEN : cts.h
- cts_ref_time_source_t : cts.h
- CTS_REF_TIME_SRC_ATOMIC_CLOCK : cts.h
- CTS_REF_TIME_SRC_CELLUAR_NET : cts.h
- CTS_REF_TIME_SRC_GPS : cts.h
- CTS_REF_TIME_SRC_MANUAL : cts.h
- CTS_REF_TIME_SRC_NET_TIME_PROTOCOL : cts.h
- CTS_REF_TIME_SRC_RADIO_TIME_SIGNAL : cts.h
- CTS_REF_TIME_SRC_UNKNOWN : cts.h
- cts_service_init() : cts.h
- CTS_TIME_ACCURACT_UNKNOWN : cts.h
- CTS_TIME_ACCURACY_OUT_RANGE : cts.h
- CTS_TIME_YEAR_VALID_VAL_MAX : cts.h
- CTS_TIME_YEAR_VALID_VAL_MIN : cts.h
- CTS_TIME_ZONE_OFFSET_MAX : cts.h
- CTS_TIME_ZONE_OFFSET_MIN : cts.h
- cts_week_day_t : cts.h
- CTS_WEEK_FRIDAY : cts.h
- CTS_WEEK_MONDAY : cts.h
- CTS_WEEK_SATURDAY : cts.h
- CTS_WEEK_SUNDAY : cts.h
- CTS_WEEK_THURSDAT : cts.h
- CTS_WEEK_TUSEDAY : cts.h
- CTS_WEEK_UNKNOWN_DAY : cts.h
- CTS_WEEK_WEDNESDAY : cts.h
- current_time_encode() : cts.h
- current_time_universal_decode() : cts.h