Classes
Structures
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control

## Classes
struct | ble_gap_addr_t
| The struct of address. More...
struct | ble_gap_bdaddr_t
| The struct of broadcast address with broadcast type. More...
struct | ble_gap_sync_established_ind_t
| Sync established indication. More...
struct | ble_gap_ext_adv_report_ind_t
| APP receives the extended advertising report indication info struct. More...
struct | ble_gap_conn_update_cmp_t
| Connection parameter used to update connection parameters. More...
struct | ble_gap_conn_param_t
| The parameter of connection. More...
struct | ble_gap_conn_update_param_t
| The parameter of update connection. More...
struct | gap_conn_cmp_t
| Connection complete info. More...
struct | ble_gap_chnl_map_t
| Channel map structure. More...
struct | ble_gap_le_phy_ind_t
| PHY info. More...
union | ble_gap_conn_info_t
| Connection info. More...
struct | ble_gap_conn_info_param_t
| The info of connecting operation. More...
struct | ble_gap_peer_version_ind_t
| Peer version info. More...
struct | ble_gap_peer_features_ind_t
| LE features info. More...
union | ble_gap_peer_info_t
| LE peer info. More...
struct | ble_gap_peer_info_param_t
| Get peer info operation struct. More...
struct | ble_gap_le_pkt_size_ind_t
| Supported data length size Indication. More...
struct | ble_gap_con_plan_tag_t
| The Structure for BLE Connection Arrangement. More...
struct | ble_gap_set_pref_slave_evt_dur_param_t
| Set preference slave event duration. More...
struct | ble_gap_dev_name_ind_t
| GAP Device name struct. More...
union | ble_gapc_set_dev_info_t
| Device information data struct. More...
struct | gapc_set_dev_info_ind_t
| GAP Device inforamtion write indication. More...
struct | ble_gap_per_sync_trans_param_t
| Default periodic advertising synchronization transfer parameters. More...
struct | ble_gap_connless_iq_report_t
| Connectionless IQ Report info. More...
struct | ble_gap_set_conn_cte_trans_param_t
| Set connection CTE transmit parameters info. More...
struct | ble_gap_set_conn_cte_rcv_param_t
| Set connection CTE receive parameters info. More...
struct | ble_gap_set_conn_cte_req_enable_t
| Set connection CTE Request enable info. More...
struct | ble_gap_conn_iq_report_t
| Connection IQ Report info. More...
struct | ble_gap_set_path_loss_report_param_t
| Set path loss reporting parameter info. More...
struct | ble_gap_evt_phy_update_t
| PHY update event for BLE_GAPC_EVT_PHY_UPDATED. More...
struct | ble_gap_evt_connected_t
| Connection complete event for BLE_GAPC_EVT_CONNECTED. More...
struct | ble_gap_evt_disconnected_t
| Disconnection event for BLE_GAPC_EVT_DISCONNECTED. More...
struct | ble_gap_evt_peer_name_get_t
| Name of peer device indication event for BLE_GAPC_EVT_PEER_NAME_GOT. More...
struct | ble_gap_evt_peer_info_t
| Get peer info event for BLE_GAPC_EVT_PEER_INFO_GOT. More...
struct | ble_gap_evt_conn_param_updated_t
| Connection parameter updated event for BLE_GAPC_EVT_CONN_PARAM_UPDATED. More...
struct | ble_gap_evt_conn_param_update_req_t
| Connection parameter update request event for BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ. More...
struct | ble_gap_evt_conn_info_t
| Get Connection info event for BLE_GAPC_EVT_CONN_INFO_GOT. More...
struct | ble_gap_evt_data_length_t
| Data Length Updated event for BLE_GAPC_EVT_DATA_LENGTH_UPDATED. More...
struct | ble_gap_evt_dev_info_set_t
| Device Information set event for BLE_GAPC_EVT_DEV_INFO_SET. More...
struct | ble_gap_evt_conn_iq_report_t
| Connection IQ Report info event for BLE_GAPC_EVT_CONNECT_IQ_REPORT. More...
struct | ble_gap_evt_connless_iq_report_t
| Connectionless IQ Report info event for BLE_GAPC_EVT_CONNECTLESS_IQ_REPORT. More...
struct | ble_gap_evt_le_event_noti_report_t
| Le event notification reporting info event for BLE_GAPC_EVT_LE_EVT_NOTI_REPORT. More...
struct | ble_gapc_evt_t
| BLE GAPC event structure. More...

## Detailed Description