Macros
Condition
Peripheral Driver » LL Driver » PWR » Defines » PWR Exported Constants

## Macros
#define | LL_PWR_AON_IRQ_EVT_BLE_PWR_ON AON_CTL_AON_IRQ_BLE_PWR
#define | LL_PWR_AON_IRQ_EVT_BLE_PWR_DN AON_CTL_AON_IRQ_BLE_PWR_DN
#define | LL_PWR_AON_IRQ_EVT_BOD_RISE AON_CTL_AON_IRQ_PMU_BOD_RISE
#define | LL_PWR_AON_IRQ_EVT_CPLL_DN AON_CTL_AON_IRQ_AONPLL_CHG
#define | LL_PWR_AON_IRQ_EVT_BOD_FALL AON_CTL_AON_IRQ_PMU_BOD_FALL
#define | LL_PWR_AON_IRQ_EVT_BLE_MAC AON_CTL_AON_IRQ_BLE_MAC_IRQ
#define | LL_PWR_AON_IRQ_EVT_SLP_FAIL AON_CTL_AON_IRQ_SLP_FAIL_IRQ
#define | LL_PWR_AON_IRQ_EVT_ALL AON_CTL_AON_IRQ_BLE_ALL

## Detailed Description

## Macro Definition Documentation

## ◆ LL_PWR_AON_IRQ_EVT_ALL

#define LL_PWR_AON_IRQ_EVT_ALL AON_CTL_AON_IRQ_BLE_ALL

All IRQ event mask

Definition at line 110 of file ll_pwr.h.

## ◆ LL_PWR_AON_IRQ_EVT_BLE_MAC

#define LL_PWR_AON_IRQ_EVT_BLE_MAC AON_CTL_AON_IRQ_BLE_MAC_IRQ

BLE MAC IRQ event

Definition at line 108 of file ll_pwr.h.

## ◆ LL_PWR_AON_IRQ_EVT_BLE_PWR_DN

#define LL_PWR_AON_IRQ_EVT_BLE_PWR_DN AON_CTL_AON_IRQ_BLE_PWR_DN

BLE power down done IRQ event

Definition at line 104 of file ll_pwr.h.

## ◆ LL_PWR_AON_IRQ_EVT_BLE_PWR_ON

#define LL_PWR_AON_IRQ_EVT_BLE_PWR_ON AON_CTL_AON_IRQ_BLE_PWR

BLE power up done IRQ event

Definition at line 103 of file ll_pwr.h.

## ◆ LL_PWR_AON_IRQ_EVT_BOD_FALL

#define LL_PWR_AON_IRQ_EVT_BOD_FALL AON_CTL_AON_IRQ_PMU_BOD_FALL

PMU BOD fall edge IRQ event

Definition at line 107 of file ll_pwr.h.

## ◆ LL_PWR_AON_IRQ_EVT_BOD_RISE

#define LL_PWR_AON_IRQ_EVT_BOD_RISE AON_CTL_AON_IRQ_PMU_BOD_RISE

BOD rise edge IRQ event

Definition at line 105 of file ll_pwr.h.

## ◆ LL_PWR_AON_IRQ_EVT_CPLL_DN

#define LL_PWR_AON_IRQ_EVT_CPLL_DN AON_CTL_AON_IRQ_AONPLL_CHG

PLL power on done IRQ event

Definition at line 106 of file ll_pwr.h.

## ◆ LL_PWR_AON_IRQ_EVT_SLP_FAIL

#define LL_PWR_AON_IRQ_EVT_SLP_FAIL AON_CTL_AON_IRQ_SLP_FAIL_IRQ

Sleep fail IRQ event

Definition at line 109 of file ll_pwr.h.