### - i -

- I2C_ADDRESSINGMODE_10BIT : hal_i2c.h
- I2C_ADDRESSINGMODE_7BIT : hal_i2c.h
- I2C_DEFAULT_CONFIG : hal_i2c.h
- I2C_FIRST_AND_LAST_FRAME : hal_i2c.h
- I2C_FIRST_AND_NEXT_FRAME : hal_i2c.h
- I2C_FIRST_FRAME : hal_i2c.h
- I2C_GENERALCALL_DISABLE : hal_i2c.h
- I2C_GENERALCALL_ENABLE : hal_i2c.h
- I2C_LAST_FRAME : hal_i2c.h
- I2C_MEM_ADD_LSB : hal_i2c.h
- I2C_MEM_ADD_MSB : hal_i2c.h
- I2C_MEMADD_SIZE_16BIT : hal_i2c.h
- I2C_MEMADD_SIZE_8BIT : hal_i2c.h
- I2C_NEXT_FRAME : hal_i2c.h
- I2C_SPEED_1000K : hal_i2c.h
- I2C_SPEED_100K : hal_i2c.h
- I2C_SPEED_400K : hal_i2c.h
- IAS_C_CONNECTION_MAX : ias_c.h
- INDI_PAYLOAD_HEADER_LEN : bcs.h
- IO_MUX_GPIO : hal_gpio.h
- IS_ADC_CLOCK : hal_adc.h
- IS_ADC_INPUT : hal_adc.h
- IS_ADC_INPUT_MODE : hal_adc.h
- IS_ADC_REF : hal_adc.h
- IS_ADC_REF_VALUE : hal_adc.h
- IS_AON_GPIO_MODE : hal_aon_gpio.h
- IS_AON_GPIO_PIN : hal_aon_gpio.h
- IS_AON_GPIO_PIN_ACTION : hal_aon_gpio.h
- IS_AON_GPIO_PULL : hal_aon_gpio.h
- IS_CALENDAR_ALARM_TYPE : hal_calendar.h
- IS_CALENDAR_DATE : hal_calendar.h
- IS_CALENDAR_LEAP_YEAR : hal_calendar.h
- IS_CALENDAR_WEEKDAY : hal_calendar.h
- IS_COMP_HYST_NEG : hal_comp.h
- IS_COMP_HYST_POS : hal_comp.h
- IS_COMP_INPUT : hal_comp.h
- IS_COMP_REF : hal_comp.h
- IS_COMP_RES_DEGENERATION_NEG : hal_comp.h
- IS_COMP_RES_DEGENERATION_POS : hal_comp.h
- IS_DMA_ALL_INSTANCE : hal_dma.h
- IS_DMA_ALL_P_INSTANCE : hal_dma.h
- IS_DMA_ALL_REQUEST : hal_dma.h
- IS_DMA_BUFFER_SIZE : hal_dma.h
- IS_DMA_DESTINATION_DATA_SIZE : hal_dma.h
- IS_DMA_DESTINATION_INC_STATE : hal_dma.h
- IS_DMA_DIRECTION : hal_dma.h
- IS_DMA_PRIORITY : hal_dma.h
- IS_DMA_SOURCE_DATA_SIZE : hal_dma.h
- IS_DMA_SOURCE_INC_STATE : hal_dma.h
- IS_DUAL_TIMER_COUNTERMODE : hal_dual_tim.h
- IS_DUAL_TIMER_IO_ACT_MODE : hal_dual_tim.h
- IS_DUAL_TIMER_IO_INIT_STATE : hal_dual_tim.h
- IS_DUAL_TIMER_PRESCALER : hal_dual_tim.h
- IS_GPIO_MODE : hal_gpio.h
- IS_GPIO_PIN : hal_gpio.h
- IS_GPIO_PIN_ACTION : hal_gpio.h
- IS_GPIO_PULL : hal_gpio.h
- IS_I2C_ADDRESSING_MODE : hal_i2c.h
- IS_I2C_GENERAL_CALL : hal_i2c.h
- IS_I2C_MEMADD_SIZE : hal_i2c.h
- IS_I2C_OWN_ADDRESS : hal_i2c.h
- IS_I2C_SLV_ADDRESS : hal_i2c.h
- IS_I2C_SPEED : hal_i2c.h
- IS_I2C_TRANSFER_OPTIONS_REQUEST : hal_i2c.h
- IS_MSIO_DIRECTION : hal_msio.h
- IS_MSIO_MODE : hal_msio.h
- IS_MSIO_PIN : hal_msio.h
- IS_MSIO_PIN_ACTION : hal_msio.h
- IS_MSIO_PULL : hal_msio.h
- IS_PKC_BIGMULTI_BITS_LENGTH : hal_pkc.h
- IS_PKC_BITS_LENGTH : hal_pkc.h
- IS_PKC_SECURE_MODE : hal_pkc.h
- IS_PWM_ALIGNMENT_MODE : hal_pwm.h
- IS_PWM_DRIVEPOLARITY : hal_pwm.h
- IS_PWM_MODE : hal_pwm.h
- IS_PWM_STOP_LVL : hal_pwm.h
- IS_PWM_WAITING_TIME_LVL : hal_pwm.h
- IS_PWR_MEM_BLOCK : hal_pwr.h
- IS_PWR_MEM_POWER_STAT : hal_pwr.h
- IS_PWR_PWR_TIMER_TYPE : hal_pwr.h
- IS_PWR_WAKEUP_CONDITION : hal_pwr.h
- IS_SPI_BAUDRATE_PRESCALER : hal_spi.h
- IS_SPI_CPHA : hal_spi.h
- IS_SPI_CPOL : hal_spi.h
- IS_SPI_DATASIZE : hal_spi.h
- IS_SPI_DIRECTION : hal_spi.h
- IS_SPI_FIFO_THRESHOLD : hal_spi.h
- IS_SPI_RX_SAMPLE_DLY : hal_spi.h
- IS_SPI_SLAVE : hal_spi.h
- IS_SPI_TIMODE : hal_spi.h
- IS_TRANSFER_REQUEST : hal_i2c.h
- IS_UART_BAUDRATE : hal_uart.h
- IS_UART_DATABITS : hal_uart.h
- IS_UART_HARDWARE_FLOW_CONTROL : hal_uart.h
- IS_UART_PARITY : hal_uart.h
- IS_UART_STOPBITS : hal_uart.h
- IS_XQSPI_ADDRESS_SIZE : hal_xqspi.h
- IS_XQSPI_BAUD_RATE : hal_xqspi.h
- IS_XQSPI_CACHE_FLUSH : hal_xqspi.h
- IS_XQSPI_CACHE_MAPPING : hal_xqspi.h
- IS_XQSPI_CACHE_MODE : hal_xqspi.h
- IS_XQSPI_CLOCK_MODE : hal_xqspi.h
- IS_XQSPI_DATA_MODE : hal_xqspi.h
- IS_XQSPI_FIFO_THRESHOLD : hal_xqspi.h
- IS_XQSPI_INSTADDR_MODE : hal_xqspi.h
- IS_XQSPI_INSTRUCTION_SIZE : hal_xqspi.h
- IS_XQSPI_READ_CMD : hal_xqspi.h
- IS_XQSPI_WORK_MODE : hal_xqspi.h