Enumerations
Enumerations
Peripheral Driver » HAL Driver » EXFLASH

## Enumerations
enum | { BLE_GATT_COMMON_EVT_MTU_EXCHANGE = BLE_GATT_COMMON_EVT_BASE, BLE_GATT_COMMON_EVT_PRF_REGISTER, BLE_GATT_COMMON_EVT_MAX, AMS_PLAYER_ATTR_ID_NAME, AMS_PLAYER_ATTR_ID_PLAYBACK_INFO, AMS_PLAYER_ATTR_ID_VOLUME, IAS_ALERT_NONE, IAS_ALERT_MILD, IAS_ALERT_HIGH, EXFLASH_CONFIG_CACHE_MODE = 0x00, EXFLASH_CONFIG_READ_CMD = 0x01, EXFLASH_CONFIG_BAUD_RATE = 0x02, EXFLASH_CONFIG_CLOCK_MODE = 0x03, EXFLASH_CONFIG_CACHE_FLUSH = 0x04, EXFLASH_CONFIG_PAGE_TYPE = 0x05, LL_PWM_FLICKER_MODE = 0x00, LL_PWM_BREATH_MODE, LL_PWM_CODING_MODE, DFU_CACHE_TYPE_CALL_STACK = 0x00, DFU_CACHE_TYPE_REG, TRC_PWR_WFE_MODE = 0, TRC_PWR_DSLEEP_MODE, TRC_PWR_ACTIVE_MODE, TRC_PWR_BLE_RET_DSLEEP, TRC_PWR_APP_TIMER_REFUSE, TRC_PWR_APP_TIMER_PASS, TRC_PWR_BLE_TIMER_REFUSE, TRC_PWR_BLE_TIMER_PASS, TRC_PWR_RTC_TIMER_REFUSE, TRC_PWR_RTC_TIMER_PASS, TRC_PWR_RTC1_TIMER_REFUSE, TRC_PWR_RTC1_TIMER_PASS, TRC_PWR_WDT_TIMER_REFUSE, TRC_PWR_WDT_TIMER_PASS }

## Detailed Description

## Enumeration Type Documentation

## ◆ anonymous enum

anonymous enum

Enumerator
BLE_GATT_COMMON_EVT_MTU_EXCHANGE | MTU Exchange event.
BLE_GATT_COMMON_EVT_PRF_REGISTER | Service Register event.
BLE_GATT_COMMON_EVT_MAX |
AMS_PLAYER_ATTR_ID_NAME | Player attribute index of name.
AMS_PLAYER_ATTR_ID_PLAYBACK_INFO | Player attribute index of playback information.
AMS_PLAYER_ATTR_ID_VOLUME | Player attribute index of volume.
IAS_ALERT_NONE | No alert.
IAS_ALERT_MILD | Mild alert.
IAS_ALERT_HIGH | High alert.
EXFLASH_CONFIG_CACHE_MODE |
EXFLASH_CONFIG_READ_CMD |
EXFLASH_CONFIG_BAUD_RATE |
EXFLASH_CONFIG_CLOCK_MODE |
EXFLASH_CONFIG_CACHE_FLUSH |
EXFLASH_CONFIG_PAGE_TYPE |
LL_PWM_FLICKER_MODE | Choose PWM Flicker Mode
LL_PWM_BREATH_MODE | Choose PWM Breath Mode
LL_PWM_CODING_MODE | Choose PWM Coding Mode
DFU_CACHE_TYPE_CALL_STACK | call stack buffer.
DFU_CACHE_TYPE_REG | register buffer.
TRC_PWR_WFE_MODE | WFE mode.
TRC_PWR_DSLEEP_MODE | Deep sleep mode.
TRC_PWR_ACTIVE_MODE | Active mode.
TRC_PWR_BLE_RET_DSLEEP | BLE return deep sleep.
TRC_PWR_APP_TIMER_REFUSE | App timer refuse.
TRC_PWR_APP_TIMER_PASS | App timer pass.
TRC_PWR_BLE_TIMER_REFUSE | BLE timer refuse.
TRC_PWR_BLE_TIMER_PASS | BLE timer pass.
TRC_PWR_RTC_TIMER_REFUSE | RTC timer refuse.
TRC_PWR_RTC_TIMER_PASS | RTC timer pass.
TRC_PWR_RTC1_TIMER_REFUSE | RTC timer refuse.
TRC_PWR_RTC1_TIMER_PASS | RTC timer pass.
TRC_PWR_WDT_TIMER_REFUSE | AON WDT timer refuse.
TRC_PWR_WDT_TIMER_PASS | AON WDT timer pass.

Definition at line 193 of file hal_exflash.h.