### - c -

- CALENDAR_ALARM_DISABLE_ALL : hal_calendar.h
- CALENDAR_ALARM_DISABLE_DATE : hal_calendar.h
- CALENDAR_ALARM_DISABLE_TICK : hal_calendar.h
- CALENDAR_ALARM_SEL_DATE : hal_calendar.h
- CALENDAR_ALARM_SEL_WEEKDAY : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_FRI : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_MON : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_SAT : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_SUN : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_THU : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_TUE : hal_calendar.h
- CALENDAR_ALARM_WEEKDAY_WED : hal_calendar.h
- CALENDAR_FLAG_ALARM : hal_calendar.h
- CALENDAR_FLAG_TICK : hal_calendar.h
- CALENDAR_FLAG_WRAP : hal_calendar.h
- CALENDAR_IT_ALARM : hal_calendar.h
- CALENDAR_IT_TICK : hal_calendar.h
- CALENDAR_IT_WRAP : hal_calendar.h
- CALENDAR_TICK_AUTO : hal_calendar.h
- CALENDAR_TICK_SINGLE : hal_calendar.h
- CFG_ANCS_ATTRIBUTE_MAXLEN : ancs_protocol.h
- CGC_CLOCK_DISABLE : ll_cgc.h
- CGC_CLOCK_ENABLE : ll_cgc.h
- CGC_DEFAULT_CONFIG : hal_cgc.h
- CGC_FRC_ALL_CLK : hal_cgc.h
- CGC_FRC_AON_MCUSUB_HCLK : hal_cgc.h
- CGC_FRC_APB_SUB_HCLK : hal_cgc.h
- CGC_FRC_BLE_BRG_HCLK : hal_cgc.h
- CGC_FRC_DMA_HCLK : hal_cgc.h
- CGC_FRC_GPIO_HCLK : hal_cgc.h
- CGC_FRC_HTB_HCLK : hal_cgc.h
- CGC_FRC_I2C0_HCLK : hal_cgc.h
- CGC_FRC_I2C1_HCLK : hal_cgc.h
- CGC_FRC_I2S_HCLK : hal_cgc.h
- CGC_FRC_I2S_S_HCLK : hal_cgc.h
- CGC_FRC_PWM_HCLK : hal_cgc.h
- CGC_FRC_QSPI0_HCLK : hal_cgc.h
- CGC_FRC_QSPI1_HCLK : hal_cgc.h
- CGC_FRC_ROM_HCLK : hal_cgc.h
- CGC_FRC_SECU_DIV4_PCLK : hal_cgc.h
- CGC_FRC_SECU_HCLK : hal_cgc.h
- CGC_FRC_SERIAL_HCLK : hal_cgc.h
- CGC_FRC_SIM_HCLK : hal_cgc.h
- CGC_FRC_SNSADC_HCLK : hal_cgc.h
- CGC_FRC_SPIM_HCLK : hal_cgc.h
- CGC_FRC_SPIS_HCLK : hal_cgc.h
- CGC_FRC_SRAM_HCLK : hal_cgc.h
- CGC_FRC_UART0_HCLK : hal_cgc.h
- CGC_FRC_UART1_HCLK : hal_cgc.h
- CGC_FRC_XF_XQSPI_HCLK : hal_cgc.h
- CGC_FRC_XQSPI_DIV4_PCLK : hal_cgc.h
- CGC_WFI_ALL_CLK : hal_cgc.h
- CGC_WFI_AON_MCUSUB_HCLK : hal_cgc.h
- CGC_WFI_APB_SUB_HCLK : hal_cgc.h
- CGC_WFI_BLE_BRG_HCLK : hal_cgc.h
- CGC_WFI_DMA_HCLK : hal_cgc.h
- CGC_WFI_GPIO_HCLK : hal_cgc.h
- CGC_WFI_HTB_HCLK : hal_cgc.h
- CGC_WFI_I2S_S_HCLK : hal_cgc.h
- CGC_WFI_PWM_HCLK : hal_cgc.h
- CGC_WFI_ROM_HCLK : hal_cgc.h
- CGC_WFI_SECU_DIV4_PCLK : hal_cgc.h
- CGC_WFI_SECU_HCLK : hal_cgc.h
- CGC_WFI_SERIAL_HCLK : hal_cgc.h
- CGC_WFI_SIM_HCLK : hal_cgc.h
- CGC_WFI_SNSADC_HCLK : hal_cgc.h
- CGC_WFI_SRAM_HCLK : hal_cgc.h
- CGC_WFI_XF_XQSPI_HCLK : hal_cgc.h
- CGC_WFI_XQSPI_DIV4_PCLK : hal_cgc.h
- CGMS_ANN_CAL_TEMP_CAL_NOT_ALLOWED : cgms.h
- CGMS_ANN_CAL_TEMP_CAL_PROCESS_PENDING : cgms.h
- CGMS_ANN_CAL_TEMP_CAL_RECOMMENED : cgms.h
- CGMS_ANN_CAL_TEMP_CAL_REQ : cgms.h
- CGMS_ANN_CAL_TEMP_TEMP_TOO_HIGH : cgms.h
- CGMS_ANN_CAL_TEMP_TEMP_TOO_LOW : cgms.h
- CGMS_ANN_CAL_TEMP_TIME_SYNC_REQ : cgms.h
- CGMS_ANN_STATUS_DEV_BATTERY_LOW : cgms.h
- CGMS_ANN_STATUS_DEV_SPEC_ALERT : cgms.h
- CGMS_ANN_STATUS_GEN_DEV_FAULT : cgms.h
- CGMS_ANN_STATUS_SENSOR_MALFUNCTION : cgms.h
- CGMS_ANN_STATUS_SENSOR_TYPE_INCORRECT : cgms.h
- CGMS_ANN_STATUS_SESSION_STOPPED : cgms.h
- CGMS_ANN_WARN_RATE_OF_DECREASE_EXCEEDED : cgms.h
- CGMS_ANN_WARN_RATE_OF_INCREASE_EXCEEDED : cgms.h
- CGMS_ANN_WARN_RESULT_HIGHER_THAN_DEV_CAN_PROCESS : cgms.h
- CGMS_ANN_WARN_RESULT_HIGHER_THAN_HYPER_LVL : cgms.h
- CGMS_ANN_WARN_RESULT_HIGHER_THAN_PATIENT_HIGH_LVL : cgms.h
- CGMS_ANN_WARN_RESULT_LOWER_THAN_DEV_CAN_PROCESS : cgms.h
- CGMS_ANN_WARN_RESULT_LOWER_THAN_HYPO_LVL : cgms.h
- CGMS_ANN_WARN_RESULT_LOWER_THAN_PATIENT_LOW_LVL : cgms.h
- CGMS_CONNECTION_MAX : cgms.h
- CGMS_ERROR_CCCD_NOT_CFG : cgms.h
- CGMS_ERROR_INVALID_CRC : cgms.h
- CGMS_ERROR_MISSING_CRC : cgms.h
- CGMS_ERROR_PRO_IN_PROCESS : cgms.h
- CGMS_FEAT_CALIBRATION : cgms.h
- CGMS_FEAT_DEV_SPEC_ALERT : cgms.h
- CGMS_FEAT_E2E_CRC : cgms.h
- CGMS_FEAT_FULL : cgms.h
- CGMS_FEAT_GENERAL_DEV_FAULT_DET : cgms.h
- CGMS_FEAT_HYPER_ALERT : cgms.h
- CGMS_FEAT_HYPO_ALERT : cgms.h
- CGMS_FEAT_LOW_BATTERY_DET : cgms.h
- CGMS_FEAT_MULTIPLE_BOND : cgms.h
- CGMS_FEAT_MULTIPLE_SESSION : cgms.h
- CGMS_FEAT_PATIENT_HIGH_LOW_ALERT : cgms.h
- CGMS_FEAT_QUALITY : cgms.h
- CGMS_FEAT_RATE_INC_DEC_ALERT : cgms.h
- CGMS_FEAT_RESULT_HIGH_LOW_DET : cgms.h
- CGMS_FEAT_SENSOR_MAL_DET : cgms.h
- CGMS_FEAT_SENSOR_TYPE_ERR_DET : cgms.h
- CGMS_FEAT_TEMP_HIGH_LOW_DET : cgms.h
- CGMS_FEAT_TREND_INFORMATION : cgms.h
- CGMS_FEATURE_VAL_LEN_MAX : cgms.h
- CGMS_MEAS_FLAG_CAL_TEMP_PRESENT : cgms.h
- CGMS_MEAS_FLAG_FULL : cgms.h
- CGMS_MEAS_FLAG_QUALITY_PRESENT : cgms.h
- CGMS_MEAS_FLAG_STATUS_PRESENT : cgms.h
- CGMS_MEAS_FLAG_TREND_INFO_PRESENT : cgms.h
- CGMS_MEAS_FLAG_WARING_PRESENT : cgms.h
- CGMS_MEASUREMENT_VAL_LEN_MAX : cgms.h
- CGMS_RACP_FILTER_TIME_OFFSET_LEN : cgms_racp.h
- CGMS_RACP_VAL_LEN_MAX : cgms.h
- CGMS_RACP_VAL_LEN_MIN : cgms.h
- CGMS_RUN_TIME_VAL_LEN_MAX : cgms.h
- CGMS_START_TIME_VAL_LEN_MAX : cgms.h
- CGMS_STATUS_VAL_LEN_MAX : cgms.h
- CHECK_IS_ON_FPGA : gr5405_sys_sdk.h
- CHIP_TRIM_PATTERN : gr5405_chip_trim.h
- CLDR_REG_READ : ll_calendar.h
- CO_BIT : ble_gapm.h
- COMP_DEFAULT_CONFIG : hal_comp.h
- COMP_HYST_NEGATIVE : hal_comp.h
- COMP_HYST_POSITIVE : hal_comp.h
- COMP_INPUT_SRC_IO0 : hal_comp.h
- COMP_INPUT_SRC_IO1 : hal_comp.h
- COMP_INPUT_SRC_IO2 : hal_comp.h
- COMP_INPUT_SRC_IO3 : hal_comp.h
- COMP_INPUT_SRC_IO4 : hal_comp.h
- COMP_INPUT_SRC_IO5 : hal_comp.h
- COMP_INPUT_SRC_IO6 : hal_comp.h
- COMP_INPUT_SRC_IO7 : hal_comp.h
- COMP_INPUT_SRC_VBAT : hal_comp.h
- COMP_INPUT_SRC_VREF : hal_comp.h
- COMP_REF_SRC_IO0 : hal_comp.h
- COMP_REF_SRC_IO1 : hal_comp.h
- COMP_REF_SRC_IO2 : hal_comp.h
- COMP_REF_SRC_IO3 : hal_comp.h
- COMP_REF_SRC_IO4 : hal_comp.h
- COMP_REF_SRC_IO5 : hal_comp.h
- COMP_REF_SRC_IO6 : hal_comp.h
- COMP_REF_SRC_IO7 : hal_comp.h
- COMP_REF_SRC_VBAT : hal_comp.h
- COMP_REF_SRC_VREF : hal_comp.h
- COMP_RES_DEGENERATION_NEGATIVE : hal_comp.h
- COMP_RES_DEGENERATION_POSITIVE : hal_comp.h
- COMP_WAKEUP_EDGE_BOTH : hal_comp.h
- COMP_WAKEUP_EDGE_FALLING : hal_comp.h
- COMP_WAKEUP_EDGE_RISING : hal_comp.h
- CS_END_STATE_ABORT_CPLT : hal_spi.h
- CS_END_STATE_POLL_EEPREAD : hal_spi.h
- CS_END_STATE_POLL_RX : hal_spi.h
- CS_END_STATE_POLL_TX : hal_spi.h
- CS_END_STATE_POLL_TX_RX : hal_spi.h
- CS_END_STATE_RX_ABORT_CPLT : hal_spi.h
- CS_END_STATE_RX_CPLT : hal_spi.h
- CS_END_STATE_TX_ABORT_CPLT : hal_spi.h
- CS_END_STATE_TX_CPLT : hal_spi.h
- CS_END_STATE_TX_RX_CPLT : hal_spi.h
- CS_END_STATE_XFER_ERR : hal_spi.h
- CS_STA_STATE_DMA_EEPREAD : hal_spi.h
- CS_STA_STATE_DMA_LLP_TX : hal_spi.h
- CS_STA_STATE_DMA_RX : hal_spi.h
- CS_STA_STATE_DMA_SCATTER_RX : hal_spi.h
- CS_STA_STATE_DMA_TX : hal_spi.h
- CS_STA_STATE_DMA_TX_RX : hal_spi.h
- CS_STA_STATE_IT_EEPREAD : hal_spi.h
- CS_STA_STATE_IT_RX : hal_spi.h
- CS_STA_STATE_IT_TX : hal_spi.h
- CS_STA_STATE_IT_TX_RX : hal_spi.h
- CS_STA_STATE_POLL_EEPREAD : hal_spi.h
- CS_STA_STATE_POLL_RX : hal_spi.h
- CS_STA_STATE_POLL_TX : hal_spi.h
- CS_STA_STATE_POLL_TX_RX : hal_spi.h
- CSCS_CHAR_FULL : cscs.h
- CSCS_CHAR_MANDATORY : cscs.h
- CSCS_CHAR_SC_CTRL_POINT : cscs.h
- CSCS_CHAR_SENSOR_LOC_SUP : cscs.h
- CSCS_CONNECTION_MAX : cscs.h
- CSCS_CTRL_PT_RSP_LEN_MIN : cscs.h
- CSCS_CTRL_PT_VAL_LEN_MAX : cscs.h
- CSCS_ERROR_CCCD_INVALID : cscs.h
- CSCS_ERROR_PROC_IN_PROGRESS : cscs.h
- CSCS_FEAR_FULL_BIT : cscs.h
- CSCS_FEAT_CRANK_REVOLUTION_SUP_BIT : cscs.h
- CSCS_FEAT_MULTIPLE_SENSORS_BIT : cscs.h
- CSCS_FEAT_VAL_LEN_MAX : cscs.h
- CSCS_FEAT_WHEEL_REVOLUTION_SUP_BIT : cscs.h
- CSCS_MEAS_FLAG_CRANK_REVOLUTION_BIT : cscs.h
- CSCS_MEAS_FLAG_WHEEL_REVOLUTION_BIT : cscs.h
- CSCS_MEAS_VAL_LEN_MAX : cscs.h
- CSCS_SENSOR_LOC_VAL_LEN_MAX : cscs.h
- CTS_AR_DST_CHANGE : cts.h
- CTS_AR_EXT_REF_TIME_UPDATE : cts.h
- CTS_AR_MAUAL_TIME_UPDATE : cts.h
- CTS_AR_NO_CHANGE : cts.h
- CTS_AR_TIME_ZONE_CHANGE : cts.h
- CTS_C_AR_DST_CHANGE : cts_c.h
- CTS_C_AR_EXT_REF_TIME_UPDATE : cts_c.h
- CTS_C_AR_MAUAL_TIME_UPDATE : cts_c.h
- CTS_C_AR_NO_CHANGE : cts_c.h
- CTS_C_AR_TIME_ZONE_CHANGE : cts_c.h
- CTS_C_CONNECTION_MAX : cts_c.h
- CTS_C_CUR_TIME_VAL_LEN : cts_c.h
- CTS_C_ERROR_FIELDS_IGNORED : cts_c.h
- CTS_C_LOC_TIME_INFO_VAL_LEN : cts_c.h
- CTS_C_TIME_ACCURACT_UNKNOWN : cts_c.h
- CTS_C_TIME_ACCURACY_OUT_RANGE : cts_c.h
- CTS_C_TIME_Y_M_D_UNKNOWN : cts_c.h
- CTS_C_TIME_YEAR_VALID_VAL_MAX : cts_c.h
- CTS_C_TIME_YEAR_VALID_VAL_MIN : cts_c.h
- CTS_C_TIME_ZONE_OFFSET_MAX : cts_c.h
- CTS_C_TIME_ZONE_OFFSET_MIN : cts_c.h
- CTS_CHAR_FULL : cts.h
- CTS_CHAR_LOC_TIME_INFO_SUP : cts.h
- CTS_CHAR_MANDATORY : cts.h
- CTS_CHAR_REF_TIME_INFO_SUP : cts.h
- CTS_CONNECTION_MAX : cts.h
- CTS_CUR_TIME_VAL_LEN : cts.h
- CTS_ERROR_FIELDS_IGNORED : cts.h
- CTS_LOC_TIME_INFO_VAL_LEN : cts.h
- CTS_REF_TIME_INFO_VAL_LEN : cts.h
- CTS_TIME_ACCURACT_UNKNOWN : cts.h
- CTS_TIME_ACCURACY_OUT_RANGE : cts.h
- CTS_TIME_YEAR_VALID_VAL_MAX : cts.h
- CTS_TIME_YEAR_VALID_VAL_MIN : cts.h
- CTS_TIME_ZONE_OFFSET_MAX : cts.h
- CTS_TIME_ZONE_OFFSET_MIN : cts.h