Macros
Mode
Peripheral Driver » LL Driver » AON_GPIO » Defines » AON_GPIO Exported Constants

## Macros
#define | LL_AON_GPIO_MODE_NONE ((uint32_t)0x0U)
#define | LL_AON_GPIO_MODE_INPUT ((uint32_t)0x1U)
#define | LL_AON_GPIO_MODE_OUTPUT ((uint32_t)0x2U)
#define | LL_AON_GPIO_MODE_INOUT ((uint32_t)0x3U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_AON_GPIO_MODE_INOUT

#define LL_AON_GPIO_MODE_INOUT ((uint32_t)0x3U)

Select input and output mode

Definition at line 160 of file ll_aon_gpio.h.

## ◆ LL_AON_GPIO_MODE_INPUT

#define LL_AON_GPIO_MODE_INPUT ((uint32_t)0x1U)

Select input mode

Definition at line 158 of file ll_aon_gpio.h.

## ◆ LL_AON_GPIO_MODE_NONE

#define LL_AON_GPIO_MODE_NONE ((uint32_t)0x0U)

No input or output

Definition at line 157 of file ll_aon_gpio.h.

## ◆ LL_AON_GPIO_MODE_OUTPUT

#define LL_AON_GPIO_MODE_OUTPUT ((uint32_t)0x2U)

Select output mode

Definition at line 159 of file ll_aon_gpio.h.