### - b -

- B : _ll_ecc_curve_init
- b_country_code : hids_hid_info_t
- b_disable_rx_oneshot_mode : gdx_lcp_config_t
- bas_bat_level_cccd_handle : bas_c_handles_t
- bas_bat_level_handle : bas_c_handles_t
- bas_bat_level_pres_handle : bas_c_handles_t
- bas_srvc_end_handle : bas_c_handles_t
- bas_srvc_start_handle : bas_c_handles_t
- basal_metabolism : bcs_meas_val_t
- basal_metabolism_present : bcs_meas_flag_t
- base_time : gls_meas_val_t
- bat_level : bas_c_evt_t
- batt_lvl : bas_init_t
- baud_rate : _ll_spim_init_t , _ll_uart_init_t , _ll_xqspi_init_t , _uart_init , _xqspi_init_t
- baudrate_prescaler : _spi_init
- bcd_hid : hids_hid_info_t
- bcs_height_res : bcs_init_t
- bcs_mass_res : bcs_init_t
- bcs_meas_flags : bcs_init_t
- bcs_unit : bcs_init_t
- bd_addr : ble_gap_evt_sync_established_t , ble_gap_period_adv_addr_cfg_t , ble_gap_ral_dev_info_t , ble_gap_sync_established_ind_t
- before_updata_sec : cts_updata_ref_time_info_t
- bin_size : dfu_boot_info_t
- birth_date_present : uds_chars_flag_t
- bit_mask : ras_filter_data_operand_t
- bl_unit_in_kpa : bps_meas_t
- ble_sch_cfg : chip_ble_config_t
- ble_slp_cfg : chip_ble_config_t
- block_size : _aes_handle , _hmac_handle , _ll_dma_init
- blue : esls_c_led_infor_t
- bm_buf : stack_heaps_table_t
- bm_size : stack_heaps_table_t
- bmi : wss_meas_val_t
- bmi_present : wss_init_t
- bod2_auto_power_bypass_en : _ll_bod_init
- bod2_en : _ll_bod_init
- bod2_lvl : _ll_bod_init
- bod_en : _ll_bod_init
- bod_env : app_bod_params_t
- bod_fedge_callback : _hal_bod_callback
- bod_msp_deinit : _hal_bod_callback
- bod_msp_init : _hal_bod_callback
- bod_redge_callback : _hal_bod_callback
- bod_state : bod_env_t
- bod_static_en : _ll_bod_init
- bod_trim : __attribute__
- body_fat_percentage : bcs_meas_val_t
- body_water_mass : bcs_meas_val_t
- body_water_mass_present : bcs_meas_flag_t
- boot_delay : dfu_boot_info_t
- boot_info : dfu_image_info_t
- bp_feature : bps_init_t
- bperiod : pwm_none_coding_init_t
- bprescaler : _ll_pwm_none_coding_mode_init_t
- breathstop_lvl : _ll_pwm_none_coding_mode_init_t
- broadcaster_addr : ble_gap_evt_adv_report_t , ble_gap_ext_adv_report_ind_t
- bstoplvl : pwm_none_coding_init_t
- bt_addr : __attribute__
- buf_size : stack_heaps_table_t
- buff_count : _adc_handle
- buff_pixel_depth : app_spi_screen_config_t
- buff_pixel_height : app_spi_screen_config_t
- buff_pixel_stride : app_spi_screen_config_t
- buff_pixel_width : app_spi_screen_config_t
- buff_size : _adc_handle
- build : sdk_version_t
- bus_lock_en : _dma_lock_config
- bus_lock_level : _dma_lock_config