Macros
IO strength
Peripheral Driver » LL Driver » AON_GPIO » Defines » AON_GPIO Exported Constants

## Macros
#define | LL_AON_GPIO_STRENGTH_LOW ((uint32_t)0x00U)
#define | LL_AON_GPIO_STRENGTH_MEDIUM ((uint32_t)0x01U)
#define | LL_AON_GPIO_STRENGTH_HIGH ((uint32_t)0x10U)
#define | LL_AON_GPIO_STRENGTH_ULTRA ((uint32_t)0x11U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_AON_GPIO_STRENGTH_HIGH

#define LL_AON_GPIO_STRENGTH_HIGH ((uint32_t)0x10U)

Select high output driver strength

Definition at line 185 of file ll_aon_gpio.h.

## ◆ LL_AON_GPIO_STRENGTH_LOW

#define LL_AON_GPIO_STRENGTH_LOW ((uint32_t)0x00U)

Select low output driver strength

Definition at line 183 of file ll_aon_gpio.h.

## ◆ LL_AON_GPIO_STRENGTH_MEDIUM

#define LL_AON_GPIO_STRENGTH_MEDIUM ((uint32_t)0x01U)

Select medium output driver strength

Definition at line 184 of file ll_aon_gpio.h.

## ◆ LL_AON_GPIO_STRENGTH_ULTRA

#define LL_AON_GPIO_STRENGTH_ULTRA ((uint32_t)0x11U)

Select high output driver strength

Definition at line 186 of file ll_aon_gpio.h.