Here is a list of all file members with links to the files they belong to:

### - m -

- MAX_XO_REQUEST_DEVICE_NUM : hal_clock.h
- MEAS_PACKET_FIRST : bcs.h
- MEAS_PACKET_SUB : bcs.h
- mem_check_proc_t : gr5405_pwr.h
- MEM_POWER_AUTO_MODE : platform_sdk.h
- MEM_POWER_FULL_MODE : platform_sdk.h
- mem_power_t : platform_sdk.h
- mem_pwr_mgmt_mode_set() : platform_sdk.h
- mem_pwr_mgmt_mode_set_from() : platform_sdk.h
- MIRROR_16M : platform_sdk.h
- MIRROR_24M : platform_sdk.h
- MIRROR_32M : platform_sdk.h
- MIRROR_48M : platform_sdk.h
- MIRROR_64M : platform_sdk.h
- MIRROR_XO16M : platform_sdk.h
- MLMR_C_CONNECTION_MAX : mlmr_c.h
- mlmr_c_disc_srvc_start() : mlmr_c.h
- MLMR_C_EVT_DISCOVERY_COMPLETE : mlmr_c.h
- MLMR_C_EVT_DISCOVERY_FAIL : mlmr_c.h
- MLMR_C_EVT_FLOW_CTRL_NTF_SET_SUCCESS : mlmr_c.h
- mlmr_c_evt_handler_t : mlmr_c.h
- MLMR_C_EVT_INVALID : mlmr_c.h
- MLMR_C_EVT_PEER_DATA_RECEIVE : mlmr_c.h
- MLMR_C_EVT_RX_FLOW_UPDATE_CPLT : mlmr_c.h
- MLMR_C_EVT_TX_CPLT : mlmr_c.h
- MLMR_C_EVT_TX_FLOW_OFF : mlmr_c.h
- MLMR_C_EVT_TX_FLOW_ON : mlmr_c.h
- MLMR_C_EVT_TX_NTF_SET_SUCCESS : mlmr_c.h
- mlmr_c_evt_type_t : mlmr_c.h
- MLMR_C_EVT_WRITE_OP_ERR : mlmr_c.h
- mlmr_c_flow_ctrl_notify_set() : mlmr_c.h
- mlmr_c_flow_ctrl_state : mlmr_c.h
- MLMR_C_FLOW_CTRL_STATE_OFF : mlmr_c.h
- MLMR_C_FLOW_CTRL_STATE_ON : mlmr_c.h
- mlmr_c_flow_ctrl_state_t : mlmr_c.h
- MLMR_C_FLOW_CTRL_UUID : mlmr_c.h
- MLMR_C_RX_CHAR_UUID : mlmr_c.h
- mlmr_c_rx_flow_ctrl_set() : mlmr_c.h
- MLMR_C_SVC_UUID : mlmr_c.h
- MLMR_C_TX_CHAR_UUID : mlmr_c.h
- mlmr_c_tx_data_send() : mlmr_c.h
- mlmr_c_tx_notify_set() : mlmr_c.h
- mlmr_client_init() : mlmr_c.h
- MLMR_CONNECTION_MAX : mlmr.h
- MLMR_EVT_FLOW_CTRL_DISABLE : mlmr.h
- MLMR_EVT_FLOW_CTRL_ENABLE : mlmr.h
- mlmr_evt_handler_t : mlmr.h
- MLMR_EVT_INVALID : mlmr.h
- MLMR_EVT_RX_DATA_RECEIVED : mlmr.h
- MLMR_EVT_TX_DATA_SENT : mlmr.h
- MLMR_EVT_TX_FLOW_OFF : mlmr.h
- MLMR_EVT_TX_FLOW_ON : mlmr.h
- MLMR_EVT_TX_PORT_CLOSED : mlmr.h
- MLMR_EVT_TX_PORT_OPENED : mlmr.h
- mlmr_evt_type_t : mlmr.h
- MLMR_FLOW_CTRL_LEN : mlmr.h
- mlmr_flow_ctrl_state : mlmr.h
- MLMR_FLOW_CTRL_STATE_OFF : mlmr.h
- MLMR_FLOW_CTRL_STATE_ON : mlmr.h
- mlmr_flow_ctrl_state_t : mlmr.h
- MLMR_MAX_DATA_LEN : mlmr.h
- mlmr_rx_flow_ctrl_set() : mlmr.h
- mlmr_service_init() : mlmr.h
- MLMR_SERVICE_UUID : mlmr.h
- mlmr_tx_data_send() : mlmr.h
- MODE0_MEA_FREQ_OFFSET : ras_common.h
- MODE0_PACKET_ANT : ras_common.h
- MODE0_PACKET_QUALITY : ras_common.h
- MODE0_PACKET_RSSI : ras_common.h
- MODE1_PACKET_ANT : ras_common.h
- MODE1_PACKET_NADM : ras_common.h
- MODE1_PACKET_PCT1 : ras_common.h
- MODE1_PACKET_PCT2 : ras_common.h
- MODE1_PACKET_QUALITY : ras_common.h
- MODE1_PACKET_RSSI : ras_common.h
- MODE1_TOD_TOA : ras_common.h
- MODE2_ANT_PATH_1 : ras_common.h
- MODE2_ANT_PATH_2 : ras_common.h
- MODE2_ANT_PATH_3 : ras_common.h
- MODE2_ANT_PATH_4 : ras_common.h
- MODE2_ANT_PERM_IDX : ras_common.h
- MODE2_TON_PCT : ras_common.h
- MODE2_TON_QUALITY_IND : ras_common.h
- MODE3_ANT_PATH_1 : ras_common.h
- MODE3_ANT_PATH_2 : ras_common.h
- MODE3_ANT_PATH_3 : ras_common.h
- MODE3_ANT_PATH_4 : ras_common.h
- MODE3_ANT_PERM_IDX : ras_common.h
- MODE3_PACKET_ANT : ras_common.h
- MODE3_PACKET_NADM : ras_common.h
- MODE3_PACKET_PCT1 : ras_common.h
- MODE3_PACKET_PCT2 : ras_common.h
- MODE3_PACKET_QUALITY : ras_common.h
- MODE3_PACKET_RSSI : ras_common.h
- MODE3_TOD_TOA : ras_common.h
- MODE3_TON_QUALITY_IND : ras_common.h
- MODE3_TONE_PCT : ras_common.h
- MPU_PWR_ID : app_pwr_mgmt.h
- MSG_ID : ble_id.h
- MSIO_DEFAULT_CONFIG : hal_msio.h
- MSIO_DIRECTION_INOUT : hal_msio.h
- MSIO_DIRECTION_INPUT : hal_msio.h
- MSIO_DIRECTION_NONE : hal_msio.h
- MSIO_DIRECTION_OUTPUT : hal_msio.h
- msio_init_t : hal_msio.h
- MSIO_INPUT_TYPE_CMOS : hal_msio.h
- MSIO_INPUT_TYPE_SCHMITT : hal_msio.h
- MSIO_MODE_ANALOG : hal_msio.h
- MSIO_MODE_DIGITAL : hal_msio.h
- MSIO_NOPULL : hal_msio.h
- msio_pad_t : ll_msio.h
- MSIO_PIN_0 : hal_msio.h
- MSIO_PIN_1 : hal_msio.h
- MSIO_PIN_2 : hal_msio.h
- MSIO_PIN_3 : hal_msio.h
- MSIO_PIN_4 : hal_msio.h
- MSIO_PIN_5 : hal_msio.h
- MSIO_PIN_6 : hal_msio.h
- MSIO_PIN_7 : hal_msio.h
- MSIO_PIN_8 : hal_msio.h
- MSIO_PIN_9 : hal_msio.h
- MSIO_PIN_ALL : hal_msio.h
- MSIO_PIN_MASK : hal_msio.h
- MSIO_PIN_RESET : hal_msio.h
- MSIO_PIN_SET : hal_msio.h
- msio_pin_state_t : hal_msio.h
- MSIO_PULLDOWN : hal_msio.h
- MSIO_PULLUP : hal_msio.h
- MSIO_SPEED_HIGH : hal_msio.h
- MSIO_SPEED_MEDIUM : hal_msio.h
- MSIO_STRENGTH_HIGH : hal_msio.h
- MSIO_STRENGTH_LOW : hal_msio.h
- MSIO_STRENGTH_MEDIUM : hal_msio.h
- MSIO_STRENGTH_ULTRA : hal_msio.h
- MSIOA : ll_msio.h