Public Attributes | List of all members
_ll_pwm_coding_channel_init_t Struct Reference
Peripheral Driver » LL Driver » PWM » Structures » PWM Exported init structures

LL PWM Output Channel init Structure definition. More...

`#include <ll_pwm.h>`

## Public Attributes
uint32_t | ll_comp0
uint32_t | ll_comp1
uint8_t | ll_drive_polarity
uint8_t | ll_waiting_time_lvl

## Detailed Description

LL PWM Output Channel init Structure definition.

Definition at line 111 of file ll_pwm.h.

## Member Data Documentation

## ◆ ll_comp0

uint32_t _ll_pwm_coding_channel_init_t::ll_comp0

Specifies current channel first compare value This parameter must be a number ranges between Min_Data=0 and Max_Data=period.

Definition at line 113 of file ll_pwm.h.

## ◆ ll_comp1

uint32_t _ll_pwm_coding_channel_init_t::ll_comp1

Specifies current channel second compare value This parameter must be a number ranges between Min_Data=0 and Max_Data=period.

Definition at line 116 of file ll_pwm.h.

## ◆ ll_drive_polarity

uint8_t _ll_pwm_coding_channel_init_t::ll_drive_polarity

Specifies the drive polarity in PWM output mode. This parameter can be a value of PWM drive polarity. This feature can be modified afterwards using unitary function ll_pwm_enable_positive_drive_channel_x() and ll_pwm_disable_positive_drive_channel_x() where X can be (A, B, C).

Definition at line 119 of file ll_pwm.h.

## ◆ ll_waiting_time_lvl

uint8_t _ll_pwm_coding_channel_init_t::ll_waiting_time_lvl

Specifies the waiting time level in coding mode. This parameter can be a value of PWM waiting time io level.

Definition at line 124 of file ll_pwm.h.

The documentation for this struct was generated from the following file:

- ll_pwm.h