Macros
Clock Selection defines
Peripheral Driver » LL Driver » LL Clock Calibration » Defines

## Macros
#define | LL_DDVS_CLK_SEL_XO_32M (0U)
#define | LL_DDVS_CLK_SEL_XO_16M (1U)
#define | LL_DDVS_CLK_SEL_SYS_32M (2U)
#define | LL_DDVS_CLK_SEL_SYS_16M (3U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_DDVS_CLK_SEL_SYS_16M

#define LL_DDVS_CLK_SEL_SYS_16M (3U)

DDVS Clock Select SYS_16M

Definition at line 105 of file ll_ddvs.h.

## ◆ LL_DDVS_CLK_SEL_SYS_32M

#define LL_DDVS_CLK_SEL_SYS_32M (2U)

DDVS Clock Select SYS_32M

Definition at line 104 of file ll_ddvs.h.

## ◆ LL_DDVS_CLK_SEL_XO_16M

#define LL_DDVS_CLK_SEL_XO_16M (1U)

DDVS Clock Select XO_16M

Definition at line 103 of file ll_ddvs.h.

## ◆ LL_DDVS_CLK_SEL_XO_32M

#define LL_DDVS_CLK_SEL_XO_32M (0U)

DDVS Clock Select XO_32M

Definition at line 102 of file ll_ddvs.h.