Macros
QSPI interrupt Defines
Peripheral Driver » LL Driver » Defines » XQSPI Exported Constants

Interrupt defines which can be used with LL_XQSPI_ReadReg and LL_XQSPI_WriteReg functions. More...

## Macros
#define | LL_XQSPI_QSPI_IM_DONE XQSPI_QSPI_XFER_DPULSE_Msk
#define | LL_XQSPI_QSPI_IM_RFF XQSPI_QSPI_RX_FPULSE_Msk
#define | LL_XQSPI_QSPI_IM_RFTF XQSPI_QSPI_RX_WPULSE_Msk
#define | LL_XQSPI_QSPI_IM_TFTF XQSPI_QSPI_TX_WPULSE_Msk
#define | LL_XQSPI_QSPI_IM_TFE XQSPI_QSPI_TX_EPULSE_Msk
#define | LL_XQSPI_QSPI_IS_DONE XQSPI_QSPI_XFER_DPULSE_Msk
#define | LL_XQSPI_QSPI_IS_RFF XQSPI_QSPI_RX_FPULSE_Msk
#define | LL_XQSPI_QSPI_IS_RFTF XQSPI_QSPI_RX_WPULSE_Msk
#define | LL_XQSPI_QSPI_IS_TFTF XQSPI_QSPI_TX_WPULSE_Msk
#define | LL_XQSPI_QSPI_IS_TFE XQSPI_QSPI_TX_EPULSE_Msk

## Detailed Description

Interrupt defines which can be used with LL_XQSPI_ReadReg and LL_XQSPI_WriteReg functions.

## Macro Definition Documentation

## ◆ LL_XQSPI_QSPI_IM_DONE

#define LL_XQSPI_QSPI_IM_DONE XQSPI_QSPI_XFER_DPULSE_Msk

Transmite Done Interrupt enable

Definition at line 242 of file ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IM_RFF

#define LL_XQSPI_QSPI_IM_RFF XQSPI_QSPI_RX_FPULSE_Msk

Receive FIFO Full Interrupt enable

Definition at line 243 of file ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IM_RFTF

#define LL_XQSPI_QSPI_IM_RFTF XQSPI_QSPI_RX_WPULSE_Msk

Receive FIFO Watermark Interrupt enable

Definition at line 244 of file ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IM_TFE

#define LL_XQSPI_QSPI_IM_TFE XQSPI_QSPI_TX_EPULSE_Msk

Transmit FIFO Empty Interrupt enable

Definition at line 246 of file ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IM_TFTF

#define LL_XQSPI_QSPI_IM_TFTF XQSPI_QSPI_TX_WPULSE_Msk

Transmit FIFO Watermark Interrupt enable

Definition at line 245 of file ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IS_DONE

#define LL_XQSPI_QSPI_IS_DONE XQSPI_QSPI_XFER_DPULSE_Msk

Transmite Done Interrupt flag

Definition at line 248 of file ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IS_RFF

#define LL_XQSPI_QSPI_IS_RFF XQSPI_QSPI_RX_FPULSE_Msk

Receive FIFO Full Interrupt flag

Definition at line 249 of file ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IS_RFTF

#define LL_XQSPI_QSPI_IS_RFTF XQSPI_QSPI_RX_WPULSE_Msk

Receive FIFO Watermark Interrupt flag

Definition at line 250 of file ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IS_TFE

#define LL_XQSPI_QSPI_IS_TFE XQSPI_QSPI_TX_EPULSE_Msk

Transmit FIFO Empty Interrupt flag

Definition at line 252 of file ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IS_TFTF

#define LL_XQSPI_QSPI_IS_TFTF XQSPI_QSPI_TX_WPULSE_Msk

Transmit FIFO Watermark Interrupt flag

Definition at line 251 of file ll_xqspi.h.