### - h -

- HAL_ADC_ERROR_DMA : hal_adc.h
- HAL_ADC_ERROR_INVALID_PARAM : hal_adc.h
- HAL_ADC_ERROR_NONE : hal_adc.h
- HAL_ADC_ERROR_TIMEOUT : hal_adc.h
- HAL_ADC_MODULE_ENABLED : gr5405_feat.h
- HAL_AES_ERROR_BUSY : hal_aes.h
- HAL_AES_ERROR_INVALID_PARAM : hal_aes.h
- HAL_AES_ERROR_NONE : hal_aes.h
- HAL_AES_ERROR_TIMEOUT : hal_aes.h
- HAL_AES_ERROR_TRANSFER : hal_aes.h
- HAL_AON_GPIO_MODULE_ENABLED : gr5405_feat.h
- HAL_AON_WDT_MODULE : gr5405_feat.h
- HAL_AON_WDT_MODULE_ENABLED : gr5405_feat.h
- HAL_BOD2_AUTO_POWER_BYPASS_DISABLE : hal_bod.h
- HAL_BOD2_AUTO_POWER_BYPASS_ENABLE : hal_bod.h
- HAL_BOD2_DISABLE : hal_bod.h
- HAL_BOD2_ENABLE : hal_bod.h
- HAL_BOD2_LEVEL_0 : hal_bod.h
- HAL_BOD2_LEVEL_1 : hal_bod.h
- HAL_BOD2_LEVEL_2 : hal_bod.h
- HAL_BOD2_LEVEL_3 : hal_bod.h
- HAL_BOD2_LEVEL_4 : hal_bod.h
- HAL_BOD2_LEVEL_5 : hal_bod.h
- HAL_BOD2_LEVEL_6 : hal_bod.h
- HAL_BOD2_LEVEL_7 : hal_bod.h
- HAL_BOD_DISABLE : hal_bod.h
- HAL_BOD_ENABLE : hal_bod.h
- HAL_BOD_MODULE_ENABLED : gr5405_feat.h
- HAL_BOD_STATIC_DISABLE : hal_bod.h
- HAL_BOD_STATIC_ENABLE : hal_bod.h
- HAL_CALENDAR_MODULE_ENABLED : gr5405_feat.h
- HAL_CLOCK_MODULE : gr5405_feat.h
- HAL_CLOCK_MODULE_ENABLED : gr5405_feat.h
- HAL_CLOCK_SETTING_IN_DRV : gr5405_feat.h
- HAL_COMP_ERROR_INVALID_PARAM : hal_comp.h
- HAL_COMP_ERROR_NONE : hal_comp.h
- HAL_COMP_ERROR_TIMEOUT : hal_comp.h
- HAL_COMP_MODULE_ENABLED : gr5405_feat.h
- HAL_DELAY_LEGACY : gr5405_feat.h
- HAL_DEV_PWR_MGMT : gr5405_feat.h
- HAL_DMA_ERROR_INVALID_PARAM : hal_dma.h
- HAL_DMA_ERROR_NO_XFER : hal_dma.h
- HAL_DMA_ERROR_NONE : hal_dma.h
- HAL_DMA_ERROR_TE : hal_dma.h
- HAL_DMA_ERROR_TIMEOUT : hal_dma.h
- HAL_DMA_MAX_CHANNEL : gr5405_feat.h
- HAL_DMA_MODULE_ENABLED : gr5405_feat.h
- HAL_DUAL_TIMER_MODULE_ENABLED : gr5405_feat.h
- HAL_EFUSE_ERROR_INVALID_PARAM : hal_efuse.h
- HAL_EFUSE_ERROR_NONE : hal_efuse.h
- HAL_EFUSE_ERROR_TIMEOUT : hal_efuse.h
- HAL_EFUSE_MODULE_ENABLED : gr5405_feat.h
- HAL_ERR_CODE_CHECK : app_drv_error.h
- HAL_EXFLASH_MODULE_ENABLED : gr5405_feat.h
- HAL_EXFLASH_RETRY_DEFAULT_VALUE : hal_exflash.h
- HAL_GPIO_MODULE_ENABLED : gr5405_feat.h
- HAL_GPIO_MUX_0 : hal_gpio.h
- HAL_GPIO_MUX_1 : hal_gpio.h
- HAL_GPIO_MUX_2 : hal_gpio.h
- HAL_GPIO_MUX_3 : hal_gpio.h
- HAL_GPIO_MUX_4 : hal_gpio.h
- HAL_GPIO_MUX_5 : hal_gpio.h
- HAL_GPIO_MUX_6 : hal_gpio.h
- HAL_HMAC_DPA_MODE_DISABLE : hal_hmac.h
- HAL_HMAC_DPA_MODE_ENABLE : hal_hmac.h
- HAL_HMAC_ERROR_BUSY : hal_hmac.h
- HAL_HMAC_ERROR_INVALID_PARAM : hal_hmac.h
- HAL_HMAC_ERROR_NONE : hal_hmac.h
- HAL_HMAC_ERROR_TIMEOUT : hal_hmac.h
- HAL_HMAC_ERROR_TRANSFER : hal_hmac.h
- HAL_HMAC_KEYTYPE_AHB : hal_hmac.h
- HAL_HMAC_KEYTYPE_KRAM : hal_hmac.h
- HAL_HMAC_KEYTYPE_MCU : hal_hmac.h
- HAL_HMAC_TIMEOUT_DEFAULT_VALUE : hal_hmac.h
- HAL_I2C_ERROR_ARB_LOST : hal_i2c.h
- HAL_I2C_ERROR_DMA : hal_i2c.h
- HAL_I2C_ERROR_INVALID_PARAM : hal_i2c.h
- HAL_I2C_ERROR_NOACK : hal_i2c.h
- HAL_I2C_ERROR_NONE : hal_i2c.h
- HAL_I2C_ERROR_NOTE : hal_i2c.h
- HAL_I2C_ERROR_OVER : hal_i2c.h
- HAL_I2C_ERROR_SCL_STUCK_AT_LOW : hal_i2c.h
- HAL_I2C_ERROR_SDA_STUCK_AT_LOW : hal_i2c.h
- HAL_I2C_ERROR_TIMEOUT : hal_i2c.h
- HAL_I2C_MODULE_ENABLED : gr5405_feat.h
- HAL_I2C_VERSION_OLD : gr5405_feat.h
- HAL_IS_BIT_CLR : hal_def.h
- HAL_IS_BIT_SET : hal_def.h
- HAL_MAX_DELAY : hal_def.h
- HAL_MPU_V7 : gr5405_feat.h
- HAL_MSIO_MODULE_ENABLED : gr5405_feat.h
- HAL_NEVER_TIMEOUT : hal_def.h
- HAL_PKC_ERROR_INVALID_PARAM : hal_pkc.h
- HAL_PKC_ERROR_INVERSE_K : hal_pkc.h
- HAL_PKC_ERROR_IRREVERSIBLE : hal_pkc.h
- HAL_PKC_ERROR_NONE : hal_pkc.h
- HAL_PKC_ERROR_OVERFLOW : hal_pkc.h
- HAL_PKC_ERROR_TIMEOUT : hal_pkc.h
- HAL_PKC_ERROR_TRANSFER : hal_pkc.h
- HAL_PKC_TIMEOUT_DEFAULT_VALUE : hal_pkc.h
- HAL_PM_ASSERT : hal_pwr_mgmt.h
- HAL_PM_ASSERT_ENABLE : hal_pwr_mgmt.h
- HAL_PM_ENABLE : gr5405_feat.h
- HAL_PM_SUSPEND : hal_pwr_mgmt.h
- HAL_PMU_MODULE_ENABLED : gr5405_feat.h
- HAL_PWM_CHANNEL_A_ERROR : hal_pwm.h
- HAL_PWM_CHANNEL_B_ERROR : hal_pwm.h
- HAL_PWM_CHANNEL_C_ERROR : hal_pwm.h
- HAL_PWM_ERROR_NONE : hal_pwm.h
- HAL_PWM_FEATURE_LEGACY : gr5405_feat.h
- HAL_PWM_MODULE_ENABLED : gr5405_feat.h
- HAL_PWMG_STATE_CHECK : gr5405_feat.h
- HAL_PWR_MGMT_ENABLED : gr5405_feat.h
- HAL_PWR_MGMT_REGISTER_ENABLED : gr5405_feat.h
- HAL_PWR_TIMEOUT_DEFAULT_VALUE : hal_pwr.h , hal_sleep_timer.h
- HAL_RNG_MODULE_ENABLED : gr5405_feat.h
- HAL_RTC_ERROR_INVALID_PARAM : hal_rtc.h
- HAL_RTC_ERROR_NONE : hal_rtc.h
- HAL_RTC_ERROR_TIMEOUT : hal_rtc.h
- HAL_RTC_MODULE_ENABLED : gr5405_feat.h
- HAL_SLEEP_TIMER_MODULE_ENABLED : gr5405_feat.h
- HAL_SLP_TIMER_OVERFLOW_VALUE : hal_sleep_timer.h
- HAL_SPI_ERROR_DMA : hal_spi.h
- HAL_SPI_ERROR_INVALID_PARAM : hal_spi.h
- HAL_SPI_ERROR_NONE : hal_spi.h
- HAL_SPI_ERROR_TIMEOUT : hal_spi.h
- HAL_SPI_ERROR_TRANSFER : hal_spi.h
- HAL_SPI_MODULE_ENABLED : gr5405_feat.h
- HAL_SPI_TIMEOUT_DEFAULT_VALUE : hal_spi.h
- HAL_STATUS_CHECK : gr5405_feat.h
- HAL_TIMEOUT_GET_TICK : hal_def.h
- HAL_TIMER_MODULE_ENABLED : gr5405_feat.h
- HAL_UART_ERROR_BI : hal_uart.h
- HAL_UART_ERROR_BUSY : hal_uart.h
- HAL_UART_ERROR_DMA : hal_uart.h
- HAL_UART_ERROR_FE : hal_uart.h
- HAL_UART_ERROR_INVALID_PARAM : hal_uart.h
- HAL_UART_ERROR_NONE : hal_uart.h
- HAL_UART_ERROR_OE : hal_uart.h
- HAL_UART_ERROR_PE : hal_uart.h
- HAL_UART_MODULE_ENABLED : gr5405_feat.h
- HAL_UART_TIMEOUT_DEFAULT_VALUE : hal_uart.h
- HAL_VERSION_MODULE : gr5405_feat.h
- HAL_XQSPI_ERROR_INVALID_PARAM : hal_xqspi.h
- HAL_XQSPI_ERROR_NONE : hal_xqspi.h
- HAL_XQSPI_ERROR_TIMEOUT : hal_xqspi.h
- HAL_XQSPI_ERROR_TRANSFER : hal_xqspi.h
- HAL_XQSPI_MODULE_ENABLED : gr5405_feat.h
- HAL_XQSPI_RETRY_DEFAULT_VALUE : hal_xqspi.h
- HID_INFO_FLAG_NORMALLY_CONNECTABLE_MSK : hids.h
- HID_INFO_FLAG_REMOTE_WAKE_MSK : hids.h
- HIDS_CONNECTION_MAX : hids.h
- HIDS_REP_TYPE_FEATURE : hids.h
- HIDS_REP_TYPE_INPUT : hids.h
- HIDS_REP_TYPE_OUTPUT : hids.h
- HIDS_REPORT_MAP_MAX_SIZE : hids.h
- HIDS_REPORT_MAX_SIZE : hids.h
- HMAC_BLOCKSIZE_BITS : hal_hmac.h
- HMAC_BLOCKSIZE_BYTES : hal_hmac.h
- HMAC_BLOCKSIZE_WORDS : hal_hmac.h
- HMAC_DIGESTSIZE_BITS : hal_hmac.h
- HMAC_DIGESTSIZE_BYTES : hal_hmac.h
- HMAC_DIGESTSIZE_WORDS : hal_hmac.h
- HMAC_DMA_BLOCK_MAX : hal_hmac.h
- HMAC_FLAG_DATAREADY_HMAC : hal_hmac.h
- HMAC_FLAG_DATAREADY_SHA : hal_hmac.h
- HMAC_FLAG_DMA_DONE : hal_hmac.h
- HMAC_FLAG_DMA_ERR : hal_hmac.h
- HMAC_FLAG_DMA_MESSAGEDONE : hal_hmac.h
- HMAC_FLAG_KEY_VALID : hal_hmac.h
- HMAC_IT_DONE : hal_hmac.h
- HMAC_MODE_HMAC : hal_hmac.h
- HMAC_MODE_SHA : hal_hmac.h
- HRRCPS_CONNECTION_MAX : hrrcps.h
- HRRCPS_CTRL_PT_RSP_VAL_LEN : hrrcps.h
- HRRCPS_CTRL_PT_VAL_LEN : hrrcps.h
- HRRCPS_SERVICE_UUID : hrrcps.h
- HRS_C_CONNECTION_MAX : hrs_c.h
- HRS_C_CTRL_POINT_ENERGY_EXP : hrs_c.h
- HRS_C_RR_INTERVALS_NUM_MAX : hrs_c.h
- HRS_CHAR_BODY_SENSOR_LOC_SUP : hrs.h
- HRS_CHAR_ENGY_EXP_SUP : hrs.h
- HRS_CHAR_MANDATORY : hrs.h
- HRS_CONNECTION_MAX : hrs.h
- HRS_MAX_BUFFERED_RR_INTERVALS : hrs.h
- HRS_MEAS_MAX_LEN : hrs.h
- HTS_CHAR_FULL : hts.h
- HTS_CHAR_INTM_TEM_SUP : hts.h
- HTS_CHAR_MANDATORY : hts.h
- HTS_CHAR_MEAS_INTERVAL_SUP : hts.h
- HTS_CHAR_TEM_TYPE_SUP : hts.h
- HTS_CONNECTION_MAX : hts.h
- HTS_INTM_TEM_MAX_LEN : hts.h
- HTS_MEAS_INTERVAL_MAX_LEN : hts.h
- HTS_MEAS_INTV_DFLT_MAX : hts.h
- HTS_MEAS_INTV_DFLT_MIN : hts.h
- HTS_TEM_MEAS_MAX_LEN : hts.h
- HTS_TEM_TYPE_MAX_LEN : hts.h